nb7MIB DEFINITIONS ::= BEGIN

--
-- Top-level infrastructure of the Net-SNMP project enterprise MIB tree
--

IMPORTS
    MODULE-IDENTITY, enterprises          	FROM SNMPv2-SMI
    MODULE-IDENTITY, OBJECT-TYPE, Integer32,
    NOTIFICATION-TYPE                       FROM SNMPv2-SMI
    SnmpAdminString                         FROM SNMP-FRAMEWORK-MIB
    netSnmp                                 FROM NET-SNMP-MIB
    RowStatus, StorageType, DisplayString   FROM SNMPv2-TC
    InetAddressType, InetAddress            FROM INET-ADDRESS-MIB
    nlcMIB			    	    FROM lspnlcMIB
    nbMIB			    	    FROM nbMIB;
;

nb7MIB MODULE-IDENTITY
    LAST-UPDATED "202103011010Z"
    ORGANIZATION "LifeSafety Power, Inc. "
    CONTACT-INFO    
     "http://www.lifesafetypower.com/
	 
	  EMail: gliu@lifesafetypower.com
	 "
    DESCRIPTION
    "This is the MIB Module for NLC objects for managing NLC device."

	REVISION	"202103011010Z"
	DESCRIPTION
	"Updated to support Net-SNMP compile."
    ::= { nbMIB 7}

nb7-mcu          	OBJECT IDENTIFIER ::= { nb7MIB 1}

nb7-fp1 OBJECT IDENTIFIER ::= {nb7MIB 34}
nb7-fp2 OBJECT IDENTIFIER ::= {nb7MIB 35}
nb7-fp3 OBJECT IDENTIFIER ::= {nb7MIB 36}
nb7-fp4 OBJECT IDENTIFIER ::= {nb7MIB 37}
nb7-fp5 OBJECT IDENTIFIER ::= {nb7MIB 38}
nb7-fp6 OBJECT IDENTIFIER ::= {nb7MIB 39}
nb7-fp7 OBJECT IDENTIFIER ::= {nb7MIB 40}
nb7-fp8 OBJECT IDENTIFIER ::= {nb7MIB 41}

nb7-m8-1          	OBJECT IDENTIFIER ::= { nb7MIB 67}
nb7-m8-1-1  		OBJECT IDENTIFIER ::= { nb7-m8-1  1}
nb7-m8-1-2  		OBJECT IDENTIFIER ::= { nb7-m8-1  2}
nb7-m8-1-3  		OBJECT IDENTIFIER ::= { nb7-m8-1  3}
nb7-m8-1-4  		OBJECT IDENTIFIER ::= { nb7-m8-1  4}
nb7-m8-1-5  		OBJECT IDENTIFIER ::= { nb7-m8-1  5}
nb7-m8-1-6  		OBJECT IDENTIFIER ::= { nb7-m8-1  6}
nb7-m8-1-7  		OBJECT IDENTIFIER ::= { nb7-m8-1  7}
nb7-m8-1-8  		OBJECT IDENTIFIER ::= { nb7-m8-1  8}


nb7-m8-2          	OBJECT IDENTIFIER ::= { nb7MIB 68}
nb7-m8-2-1  		OBJECT IDENTIFIER ::= { nb7-m8-2  1}
nb7-m8-2-2  		OBJECT IDENTIFIER ::= { nb7-m8-2  2}
nb7-m8-2-3  		OBJECT IDENTIFIER ::= { nb7-m8-2  3}
nb7-m8-2-4  		OBJECT IDENTIFIER ::= { nb7-m8-2  4}
nb7-m8-2-5  		OBJECT IDENTIFIER ::= { nb7-m8-2  5}
nb7-m8-2-6  		OBJECT IDENTIFIER ::= { nb7-m8-2  6}
nb7-m8-2-7  		OBJECT IDENTIFIER ::= { nb7-m8-2  7}
nb7-m8-2-8  		OBJECT IDENTIFIER ::= { nb7-m8-2  8}

nb7-m8-3          	OBJECT IDENTIFIER ::= { nb7MIB 69}
nb7-m8-3-1  		OBJECT IDENTIFIER ::= { nb7-m8-3  1}
nb7-m8-3-2  		OBJECT IDENTIFIER ::= { nb7-m8-3  2}
nb7-m8-3-3  		OBJECT IDENTIFIER ::= { nb7-m8-3  3}
nb7-m8-3-4  		OBJECT IDENTIFIER ::= { nb7-m8-3  4}
nb7-m8-3-5  		OBJECT IDENTIFIER ::= { nb7-m8-3  5}
nb7-m8-3-6  		OBJECT IDENTIFIER ::= { nb7-m8-3  6}
nb7-m8-3-7  		OBJECT IDENTIFIER ::= { nb7-m8-3  7}
nb7-m8-3-8  		OBJECT IDENTIFIER ::= { nb7-m8-3  8}

nb7-m8-4          	OBJECT IDENTIFIER ::= { nb7MIB 70}
nb7-m8-4-1  		OBJECT IDENTIFIER ::= { nb7-m8-4  1}
nb7-m8-4-2  		OBJECT IDENTIFIER ::= { nb7-m8-4  2}
nb7-m8-4-3  		OBJECT IDENTIFIER ::= { nb7-m8-4  3}
nb7-m8-4-4  		OBJECT IDENTIFIER ::= { nb7-m8-4  4}
nb7-m8-4-5  		OBJECT IDENTIFIER ::= { nb7-m8-4  5}
nb7-m8-4-6  		OBJECT IDENTIFIER ::= { nb7-m8-4  6}
nb7-m8-4-7  		OBJECT IDENTIFIER ::= { nb7-m8-4  7}
nb7-m8-4-8  		OBJECT IDENTIFIER ::= { nb7-m8-4  8}

nb7-m8-5          	OBJECT IDENTIFIER ::= { nb7MIB 71}
nb7-m8-5-1  		OBJECT IDENTIFIER ::= { nb7-m8-5  1}
nb7-m8-5-2  		OBJECT IDENTIFIER ::= { nb7-m8-5  2}
nb7-m8-5-3  		OBJECT IDENTIFIER ::= { nb7-m8-5  3}
nb7-m8-5-4  		OBJECT IDENTIFIER ::= { nb7-m8-5  4}
nb7-m8-5-5  		OBJECT IDENTIFIER ::= { nb7-m8-5  5}
nb7-m8-5-6  		OBJECT IDENTIFIER ::= { nb7-m8-5  6}
nb7-m8-5-7  		OBJECT IDENTIFIER ::= { nb7-m8-5  7}
nb7-m8-5-8  		OBJECT IDENTIFIER ::= { nb7-m8-5  8}

nb7-m8-6          	OBJECT IDENTIFIER ::= { nb7MIB 72}
nb7-m8-6-1  		OBJECT IDENTIFIER ::= { nb7-m8-6  1}
nb7-m8-6-2  		OBJECT IDENTIFIER ::= { nb7-m8-6  2}
nb7-m8-6-3  		OBJECT IDENTIFIER ::= { nb7-m8-6  3}
nb7-m8-6-4  		OBJECT IDENTIFIER ::= { nb7-m8-6  4}
nb7-m8-6-5  		OBJECT IDENTIFIER ::= { nb7-m8-6  5}
nb7-m8-6-6  		OBJECT IDENTIFIER ::= { nb7-m8-6  6}
nb7-m8-6-7  		OBJECT IDENTIFIER ::= { nb7-m8-6  7}
nb7-m8-6-8  		OBJECT IDENTIFIER ::= { nb7-m8-6  8}

nb7-m8-7          	OBJECT IDENTIFIER ::= { nb7MIB 73}
nb7-m8-7-1  		OBJECT IDENTIFIER ::= { nb7-m8-7  1}
nb7-m8-7-2  		OBJECT IDENTIFIER ::= { nb7-m8-7  2}
nb7-m8-7-3  		OBJECT IDENTIFIER ::= { nb7-m8-7  3}
nb7-m8-7-4  		OBJECT IDENTIFIER ::= { nb7-m8-7  4}
nb7-m8-7-5  		OBJECT IDENTIFIER ::= { nb7-m8-7  5}
nb7-m8-7-6  		OBJECT IDENTIFIER ::= { nb7-m8-7  6}
nb7-m8-7-7  		OBJECT IDENTIFIER ::= { nb7-m8-7  7}
nb7-m8-7-8  		OBJECT IDENTIFIER ::= { nb7-m8-7  8}

nb7-m8-8          	OBJECT IDENTIFIER ::= { nb7MIB 74}
nb7-m8-8-1  		OBJECT IDENTIFIER ::= { nb7-m8-8  1}
nb7-m8-8-2  		OBJECT IDENTIFIER ::= { nb7-m8-8  2}
nb7-m8-8-3  		OBJECT IDENTIFIER ::= { nb7-m8-8  3}
nb7-m8-8-4  		OBJECT IDENTIFIER ::= { nb7-m8-8  4}
nb7-m8-8-5  		OBJECT IDENTIFIER ::= { nb7-m8-8  5}
nb7-m8-8-6  		OBJECT IDENTIFIER ::= { nb7-m8-8  6}
nb7-m8-8-7  		OBJECT IDENTIFIER ::= { nb7-m8-8  7}
nb7-m8-8-8  		OBJECT IDENTIFIER ::= { nb7-m8-8  8}



nb7-sd16-1          OBJECT IDENTIFIER ::= { nb7MIB 100}
nb7-sd16-1-1  		OBJECT IDENTIFIER ::= { nb7-sd16-1  1}
nb7-sd16-1-2  		OBJECT IDENTIFIER ::= { nb7-sd16-1  2}
nb7-sd16-1-3  		OBJECT IDENTIFIER ::= { nb7-sd16-1  3}
nb7-sd16-1-4  		OBJECT IDENTIFIER ::= { nb7-sd16-1  4}
nb7-sd16-1-5  		OBJECT IDENTIFIER ::= { nb7-sd16-1  5}
nb7-sd16-1-6  		OBJECT IDENTIFIER ::= { nb7-sd16-1  6}
nb7-sd16-1-7  		OBJECT IDENTIFIER ::= { nb7-sd16-1  7}
nb7-sd16-1-8  		OBJECT IDENTIFIER ::= { nb7-sd16-1  8}
nb7-sd16-1-9  		OBJECT IDENTIFIER ::= { nb7-sd16-1  9}
nb7-sd16-1-10  		OBJECT IDENTIFIER ::= { nb7-sd16-1  10}
nb7-sd16-1-11  		OBJECT IDENTIFIER ::= { nb7-sd16-1  11}
nb7-sd16-1-12  		OBJECT IDENTIFIER ::= { nb7-sd16-1  12}
nb7-sd16-1-13  		OBJECT IDENTIFIER ::= { nb7-sd16-1  13}
nb7-sd16-1-14  		OBJECT IDENTIFIER ::= { nb7-sd16-1  14}
nb7-sd16-1-15  		OBJECT IDENTIFIER ::= { nb7-sd16-1  15}
nb7-sd16-1-16  		OBJECT IDENTIFIER ::= { nb7-sd16-1  16}

nb7-sd16-2          OBJECT IDENTIFIER ::= { nb7MIB 101}
nb7-sd16-2-1  		OBJECT IDENTIFIER ::= { nb7-sd16-2  1}
nb7-sd16-2-2  		OBJECT IDENTIFIER ::= { nb7-sd16-2  2}
nb7-sd16-2-3  		OBJECT IDENTIFIER ::= { nb7-sd16-2  3}
nb7-sd16-2-4  		OBJECT IDENTIFIER ::= { nb7-sd16-2  4}
nb7-sd16-2-5  		OBJECT IDENTIFIER ::= { nb7-sd16-2  5}
nb7-sd16-2-6  		OBJECT IDENTIFIER ::= { nb7-sd16-2  6}
nb7-sd16-2-7  		OBJECT IDENTIFIER ::= { nb7-sd16-2  7}
nb7-sd16-2-8  		OBJECT IDENTIFIER ::= { nb7-sd16-2  8}
nb7-sd16-2-9  		OBJECT IDENTIFIER ::= { nb7-sd16-2  9}
nb7-sd16-2-10  		OBJECT IDENTIFIER ::= { nb7-sd16-2  10}
nb7-sd16-2-11  		OBJECT IDENTIFIER ::= { nb7-sd16-2  11}
nb7-sd16-2-12  		OBJECT IDENTIFIER ::= { nb7-sd16-2  12}
nb7-sd16-2-13  		OBJECT IDENTIFIER ::= { nb7-sd16-2  13}
nb7-sd16-2-14  		OBJECT IDENTIFIER ::= { nb7-sd16-2  14}
nb7-sd16-2-15  		OBJECT IDENTIFIER ::= { nb7-sd16-2  15}
nb7-sd16-2-16  		OBJECT IDENTIFIER ::= { nb7-sd16-2  16}

nb7-sd16-3          OBJECT IDENTIFIER ::= { nb7MIB 102}
nb7-sd16-3-1  		OBJECT IDENTIFIER ::= { nb7-sd16-3  1}
nb7-sd16-3-2  		OBJECT IDENTIFIER ::= { nb7-sd16-3  2}
nb7-sd16-3-3  		OBJECT IDENTIFIER ::= { nb7-sd16-3  3}
nb7-sd16-3-4  		OBJECT IDENTIFIER ::= { nb7-sd16-3  4}
nb7-sd16-3-5  		OBJECT IDENTIFIER ::= { nb7-sd16-3  5}
nb7-sd16-3-6  		OBJECT IDENTIFIER ::= { nb7-sd16-3  6}
nb7-sd16-3-7  		OBJECT IDENTIFIER ::= { nb7-sd16-3  7}
nb7-sd16-3-8  		OBJECT IDENTIFIER ::= { nb7-sd16-3  8}
nb7-sd16-3-9  		OBJECT IDENTIFIER ::= { nb7-sd16-3  9}
nb7-sd16-3-10  		OBJECT IDENTIFIER ::= { nb7-sd16-3  10}
nb7-sd16-3-11  		OBJECT IDENTIFIER ::= { nb7-sd16-3  11}
nb7-sd16-3-12  		OBJECT IDENTIFIER ::= { nb7-sd16-3  12}
nb7-sd16-3-13  		OBJECT IDENTIFIER ::= { nb7-sd16-3  13}
nb7-sd16-3-14  		OBJECT IDENTIFIER ::= { nb7-sd16-3  14}
nb7-sd16-3-15  		OBJECT IDENTIFIER ::= { nb7-sd16-3  15}
nb7-sd16-3-16  		OBJECT IDENTIFIER ::= { nb7-sd16-3  16}

nb7-sd16-4          OBJECT IDENTIFIER ::= { nb7MIB 103}
nb7-sd16-4-1  		OBJECT IDENTIFIER ::= { nb7-sd16-4  1}
nb7-sd16-4-2  		OBJECT IDENTIFIER ::= { nb7-sd16-4  2}
nb7-sd16-4-3  		OBJECT IDENTIFIER ::= { nb7-sd16-4  3}
nb7-sd16-4-4  		OBJECT IDENTIFIER ::= { nb7-sd16-4  4}
nb7-sd16-4-5  		OBJECT IDENTIFIER ::= { nb7-sd16-4  5}
nb7-sd16-4-6  		OBJECT IDENTIFIER ::= { nb7-sd16-4  6}
nb7-sd16-4-7  		OBJECT IDENTIFIER ::= { nb7-sd16-4  7}
nb7-sd16-4-8  		OBJECT IDENTIFIER ::= { nb7-sd16-4  8}
nb7-sd16-4-9  		OBJECT IDENTIFIER ::= { nb7-sd16-4  9}
nb7-sd16-4-10  		OBJECT IDENTIFIER ::= { nb7-sd16-4  10}
nb7-sd16-4-11  		OBJECT IDENTIFIER ::= { nb7-sd16-4  11}
nb7-sd16-4-12  		OBJECT IDENTIFIER ::= { nb7-sd16-4  12}
nb7-sd16-4-13  		OBJECT IDENTIFIER ::= { nb7-sd16-4  13}
nb7-sd16-4-14  		OBJECT IDENTIFIER ::= { nb7-sd16-4  14}
nb7-sd16-4-15  		OBJECT IDENTIFIER ::= { nb7-sd16-4  15}
nb7-sd16-4-16  		OBJECT IDENTIFIER ::= { nb7-sd16-4  16}

nb7-sd16-5          OBJECT IDENTIFIER ::= { nb7MIB 104}
nb7-sd16-5-1  		OBJECT IDENTIFIER ::= { nb7-sd16-5  1}
nb7-sd16-5-2  		OBJECT IDENTIFIER ::= { nb7-sd16-5  2}
nb7-sd16-5-3  		OBJECT IDENTIFIER ::= { nb7-sd16-5  3}
nb7-sd16-5-4  		OBJECT IDENTIFIER ::= { nb7-sd16-5  4}
nb7-sd16-5-5  		OBJECT IDENTIFIER ::= { nb7-sd16-5  5}
nb7-sd16-5-6  		OBJECT IDENTIFIER ::= { nb7-sd16-5  6}
nb7-sd16-5-7  		OBJECT IDENTIFIER ::= { nb7-sd16-5  7}
nb7-sd16-5-8  		OBJECT IDENTIFIER ::= { nb7-sd16-5  8}
nb7-sd16-5-9  		OBJECT IDENTIFIER ::= { nb7-sd16-5  9}
nb7-sd16-5-10  		OBJECT IDENTIFIER ::= { nb7-sd16-5  10}
nb7-sd16-5-11  		OBJECT IDENTIFIER ::= { nb7-sd16-5  11}
nb7-sd16-5-12  		OBJECT IDENTIFIER ::= { nb7-sd16-5  12}
nb7-sd16-5-13  		OBJECT IDENTIFIER ::= { nb7-sd16-5  13}
nb7-sd16-5-14  		OBJECT IDENTIFIER ::= { nb7-sd16-5  14}
nb7-sd16-5-15  		OBJECT IDENTIFIER ::= { nb7-sd16-5  15}
nb7-sd16-5-16  		OBJECT IDENTIFIER ::= { nb7-sd16-5  16}

nb7-sd16-6          OBJECT IDENTIFIER ::= { nb7MIB 105}
nb7-sd16-6-1  		OBJECT IDENTIFIER ::= { nb7-sd16-6  1}
nb7-sd16-6-2  		OBJECT IDENTIFIER ::= { nb7-sd16-6  2}
nb7-sd16-6-3  		OBJECT IDENTIFIER ::= { nb7-sd16-6  3}
nb7-sd16-6-4  		OBJECT IDENTIFIER ::= { nb7-sd16-6  4}
nb7-sd16-6-5  		OBJECT IDENTIFIER ::= { nb7-sd16-6  5}
nb7-sd16-6-6  		OBJECT IDENTIFIER ::= { nb7-sd16-6  6}
nb7-sd16-6-7  		OBJECT IDENTIFIER ::= { nb7-sd16-6  7}
nb7-sd16-6-8  		OBJECT IDENTIFIER ::= { nb7-sd16-6  8}
nb7-sd16-6-9  		OBJECT IDENTIFIER ::= { nb7-sd16-6  9}
nb7-sd16-6-10  		OBJECT IDENTIFIER ::= { nb7-sd16-6  10}
nb7-sd16-6-11  		OBJECT IDENTIFIER ::= { nb7-sd16-6  11}
nb7-sd16-6-12  		OBJECT IDENTIFIER ::= { nb7-sd16-6  12}
nb7-sd16-6-13  		OBJECT IDENTIFIER ::= { nb7-sd16-6  13}
nb7-sd16-6-14  		OBJECT IDENTIFIER ::= { nb7-sd16-6  14}
nb7-sd16-6-15  		OBJECT IDENTIFIER ::= { nb7-sd16-6  15}
nb7-sd16-6-16  		OBJECT IDENTIFIER ::= { nb7-sd16-6  16}

nb7-sd16-7          OBJECT IDENTIFIER ::= { nb7MIB 106}
nb7-sd16-7-1  		OBJECT IDENTIFIER ::= { nb7-sd16-7  1}
nb7-sd16-7-2  		OBJECT IDENTIFIER ::= { nb7-sd16-7  2}
nb7-sd16-7-3  		OBJECT IDENTIFIER ::= { nb7-sd16-7  3}
nb7-sd16-7-4  		OBJECT IDENTIFIER ::= { nb7-sd16-7  4}
nb7-sd16-7-5  		OBJECT IDENTIFIER ::= { nb7-sd16-7  5}
nb7-sd16-7-6  		OBJECT IDENTIFIER ::= { nb7-sd16-7  6}
nb7-sd16-7-7  		OBJECT IDENTIFIER ::= { nb7-sd16-7  7}
nb7-sd16-7-8  		OBJECT IDENTIFIER ::= { nb7-sd16-7  8}
nb7-sd16-7-9  		OBJECT IDENTIFIER ::= { nb7-sd16-7  9}
nb7-sd16-7-10  		OBJECT IDENTIFIER ::= { nb7-sd16-7  10}
nb7-sd16-7-11  		OBJECT IDENTIFIER ::= { nb7-sd16-7  11}
nb7-sd16-7-12  		OBJECT IDENTIFIER ::= { nb7-sd16-7  12}
nb7-sd16-7-13  		OBJECT IDENTIFIER ::= { nb7-sd16-7  13}
nb7-sd16-7-14  		OBJECT IDENTIFIER ::= { nb7-sd16-7  14}
nb7-sd16-7-15  		OBJECT IDENTIFIER ::= { nb7-sd16-7  15}
nb7-sd16-7-16  		OBJECT IDENTIFIER ::= { nb7-sd16-7  16}

nb7-sd16-8          OBJECT IDENTIFIER ::= { nb7MIB 107}
nb7-sd16-8-1  		OBJECT IDENTIFIER ::= { nb7-sd16-8  1}
nb7-sd16-8-2  		OBJECT IDENTIFIER ::= { nb7-sd16-8  2}
nb7-sd16-8-3  		OBJECT IDENTIFIER ::= { nb7-sd16-8  3}
nb7-sd16-8-4  		OBJECT IDENTIFIER ::= { nb7-sd16-8  4}
nb7-sd16-8-5  		OBJECT IDENTIFIER ::= { nb7-sd16-8  5}
nb7-sd16-8-6  		OBJECT IDENTIFIER ::= { nb7-sd16-8  6}
nb7-sd16-8-7  		OBJECT IDENTIFIER ::= { nb7-sd16-8  7}
nb7-sd16-8-8  		OBJECT IDENTIFIER ::= { nb7-sd16-8  8}
nb7-sd16-8-9  		OBJECT IDENTIFIER ::= { nb7-sd16-8  9}
nb7-sd16-8-10  		OBJECT IDENTIFIER ::= { nb7-sd16-8  10}
nb7-sd16-8-11  		OBJECT IDENTIFIER ::= { nb7-sd16-8  11}
nb7-sd16-8-12  		OBJECT IDENTIFIER ::= { nb7-sd16-8  12}
nb7-sd16-8-13  		OBJECT IDENTIFIER ::= { nb7-sd16-8  13}
nb7-sd16-8-14  		OBJECT IDENTIFIER ::= { nb7-sd16-8  14}
nb7-sd16-8-15  		OBJECT IDENTIFIER ::= { nb7-sd16-8  15}
nb7-sd16-8-16  		OBJECT IDENTIFIER ::= { nb7-sd16-8  16}



nb7-sd4-1          	OBJECT IDENTIFIER ::= { nb7MIB 133}
nb7-sd4-1-1  		OBJECT IDENTIFIER ::= { nb7-sd4-1  1}
nb7-sd4-1-2  		OBJECT IDENTIFIER ::= { nb7-sd4-1  2}
nb7-sd4-1-3  		OBJECT IDENTIFIER ::= { nb7-sd4-1  3}
nb7-sd4-1-4  		OBJECT IDENTIFIER ::= { nb7-sd4-1  4}

nb7-sd4-2          	OBJECT IDENTIFIER ::= { nb7MIB 134}
nb7-sd4-2-1  		OBJECT IDENTIFIER ::= { nb7-sd4-2  1}
nb7-sd4-2-2  		OBJECT IDENTIFIER ::= { nb7-sd4-2  2}
nb7-sd4-2-3  		OBJECT IDENTIFIER ::= { nb7-sd4-2  3}
nb7-sd4-2-4  		OBJECT IDENTIFIER ::= { nb7-sd4-2  4}

nb7-sd4-3          	OBJECT IDENTIFIER ::= { nb7MIB 135}
nb7-sd4-3-1  		OBJECT IDENTIFIER ::= { nb7-sd4-3  1}
nb7-sd4-3-2  		OBJECT IDENTIFIER ::= { nb7-sd4-3  2}
nb7-sd4-3-3  		OBJECT IDENTIFIER ::= { nb7-sd4-3  3}
nb7-sd4-3-4  		OBJECT IDENTIFIER ::= { nb7-sd4-3  4}

nb7-sd4-4          	OBJECT IDENTIFIER ::= { nb7MIB 136}
nb7-sd4-4-1  		OBJECT IDENTIFIER ::= { nb7-sd4-4  1}
nb7-sd4-4-2  		OBJECT IDENTIFIER ::= { nb7-sd4-4  2}
nb7-sd4-4-3  		OBJECT IDENTIFIER ::= { nb7-sd4-4  3}
nb7-sd4-4-4  		OBJECT IDENTIFIER ::= { nb7-sd4-4  4}

nb7-sd4-5          	OBJECT IDENTIFIER ::= { nb7MIB 137}
nb7-sd4-5-1  		OBJECT IDENTIFIER ::= { nb7-sd4-5  1}
nb7-sd4-5-2  		OBJECT IDENTIFIER ::= { nb7-sd4-5  2}
nb7-sd4-5-3  		OBJECT IDENTIFIER ::= { nb7-sd4-5  3}
nb7-sd4-5-4  		OBJECT IDENTIFIER ::= { nb7-sd4-5  4}

nb7-sd4-6          	OBJECT IDENTIFIER ::= { nb7MIB 138}
nb7-sd4-6-1  		OBJECT IDENTIFIER ::= { nb7-sd4-6  1}
nb7-sd4-6-2  		OBJECT IDENTIFIER ::= { nb7-sd4-6  2}
nb7-sd4-6-3  		OBJECT IDENTIFIER ::= { nb7-sd4-6  3}
nb7-sd4-6-4  		OBJECT IDENTIFIER ::= { nb7-sd4-6  4}

nb7-sd4-7          	OBJECT IDENTIFIER ::= { nb7MIB 139}
nb7-sd4-7-1  		OBJECT IDENTIFIER ::= { nb7-sd4-7  1}
nb7-sd4-7-2  		OBJECT IDENTIFIER ::= { nb7-sd4-7  2}
nb7-sd4-7-3  		OBJECT IDENTIFIER ::= { nb7-sd4-7  3}
nb7-sd4-7-4  		OBJECT IDENTIFIER ::= { nb7-sd4-7  4}

nb7-sd4-8          	OBJECT IDENTIFIER ::= { nb7MIB 140}
nb7-sd4-8-1  		OBJECT IDENTIFIER ::= { nb7-sd4-8  1}
nb7-sd4-8-2  		OBJECT IDENTIFIER ::= { nb7-sd4-8  2}
nb7-sd4-8-3  		OBJECT IDENTIFIER ::= { nb7-sd4-8  3}
nb7-sd4-8-4  		OBJECT IDENTIFIER ::= { nb7-sd4-8  4}


nb7-b150-1          OBJECT IDENTIFIER ::= { nb7MIB 166}
nb7-b150-2          OBJECT IDENTIFIER ::= { nb7MIB 167}
nb7-b150-3          OBJECT IDENTIFIER ::= { nb7MIB 168}
nb7-b150-4          OBJECT IDENTIFIER ::= { nb7MIB 169}
nb7-b150-5          OBJECT IDENTIFIER ::= { nb7MIB 170}
nb7-b150-6          OBJECT IDENTIFIER ::= { nb7MIB 171}
nb7-b150-7          OBJECT IDENTIFIER ::= { nb7MIB 172}
nb7-b150-8          OBJECT IDENTIFIER ::= { nb7MIB 173}



--
--	nb7-mcu
--    
	
	

Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-mcu 1 }


Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-mcu 2 }

DeviceDetectCNT OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-mcu 3 }
	
ADC1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-mcu 4 }	
	
ADC2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-mcu 5 }		
	
	
ADC3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-mcu 6 }		
	
	
EncloseTemperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-mcu 7 }	

ExternalTemperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-mcu 8 }	

Humidity OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-mcu 9 }		
	
Event OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-mcu 10 }		
	
EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-mcu 11 }	
	
ADC1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-mcu 12 }	
	

ADC1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-mcu 13 }	

	
ADC2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-mcu 14 }	
	

ADC2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-mcu 15 }	

ADC3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-mcu 16 }	
	

ADC3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-mcu 17 }	

EncloseTemperatureLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-mcu 18 }	
	

EncloseTemperatureUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-mcu 19 }	

ExternalTemperatureLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-mcu 20 }	
	

ExternalTemperatureUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-mcu 21 }	

HumidityLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-mcu 22 }	
	

HumidityUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-mcu 23 }	




--
--	FP1
--    
FP1Time OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Time."
    DEFVAL { "" }
    ::= { nb7-fp1  1 }

FP1DeviceID OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "FPO ID."
    DEFVAL { "" }
    ::= { nb7-fp1  2 }

FP1ModNumber OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply Model, Such as FPO75-25, FPO150-100, FPO250-200."
    DEFVAL { "" }
    ::= { nb7-fp1  3 }

FP1SystemFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply system fault status."
    DEFVAL { "" }
    ::= { nb7-fp1  4 }

FP1ACFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply AC lost status, No or Yes."
    DEFVAL { "" }
    ::= { nb7-fp1  5 }

FP1FAIStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI status."
    DEFVAL { "" }
    ::= { nb7-fp1  6 }

FP1OutputLatchingOnFAI OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI latch status."
    DEFVAL { "" }
    ::= { nb7-fp1  7 }
    
FP1ACInputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC input voltage."
    DEFVAL { "" }
    ::= { nb7-fp1  8 }

FP1OutputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output voltage."
    DEFVAL { "" }
    ::= { nb7-fp1  9 }
    
FP1OutputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output Current."
    DEFVAL { "" }
    ::= { nb7-fp1  10 }
    

FP1BatteryVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System battery voltage."
    DEFVAL { "" }
    ::= { nb7-fp1  11 }

FP1BatteryChargeCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery charge current."
    DEFVAL { "" }
    ::= { nb7-fp1  12 }
    
FP1BatteryFaultDetect OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery Fault Detect. For AQL/FPV."
    DEFVAL { "" }
    ::= { nb7-fp1  13 }

FP1TotalPowerupTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power supply total runtime."
    DEFVAL { "" }
    ::= { nb7-fp1  14 }

FP1BatteryInstalledTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery install hours."
    DEFVAL { "" }
    ::= { nb7-fp1  15 }

FP1NumberOfACFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC lost count."
    DEFVAL { "" }
    ::= { nb7-fp1  16 }

FP1NumberOfSystemFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System fault count."
    DEFVAL { "" }
    ::= { nb7-fp1  17 }
	
	
FP1RatedBatteryLife OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "FPO battery lifetime."
    DEFVAL { "" }
    ::= { nb7-fp1  18 }	

	
FP1RatedCapacity  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery capacity."
    DEFVAL { "" }
    ::= { nb7-fp1  19 }	
	
		
FP1BatteryStateOfCharge OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "The FPO battery state of charge."
    DEFVAL { "" }
    ::= { nb7-fp1  20 }	

FP1BatteryStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Enable or Disable calculate battery state of charge."
    DEFVAL { "" }
    ::= { nb7-fp1  21 }		
		
FP1BatteryTestStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery discharge test status, Active or Inactive. Set Value: Testing or Inactive"
    DEFVAL { "" }
    ::= { nb7-fp1  22 }

FP1BatteryLastTestDate OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test date."
    DEFVAL { "" }
    ::= { nb7-fp1  23 }

FP1BatteryLastTestDischargeTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test time."
    DEFVAL { "" }
    ::= { nb7-fp1  24 }
    
FP1RepeatTestInterval OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Repeat Test Interval."
    DEFVAL { "" }
    ::= { nb7-fp1  25 }
    
FP1Version	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "FP1 Ver."
    DEFVAL { "" }
    ::= { nb7-fp1  26 }  
    
FP1SystemFaultDescription	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Fault Description."
    DEFVAL { "" }
    ::= { nb7-fp1  27 }         
    
 FP1BatteryTestsPerformed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Performed."
    DEFVAL { "" }
    ::= { nb7-fp1  28 }   

FP1BatteryTestsFailed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Failed."
    DEFVAL { "" }
    ::= { nb7-fp1  29 }  

   FP1RequiredBatteryRuntime	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS   read-write
    STATUS      current
    DESCRIPTION
    "Required Battery Runtime."
    DEFVAL { "" }
    ::= { nb7-fp1  30 }  

    FP1ActualStandby	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Actual Standby."
    DEFVAL { "" }
    ::= { nb7-fp1  31 }  

    FP1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset output for AQL/FPV-G2/FPG/FPO-G2"
    DEFVAL { "" }
    ::= { nb7-fp1  32 }  

    FP1BatteryScheduleTestDateTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "e.g. Enter '2020-01-01 23:01:59' to configure Battery Schedule Test DateTime"
    DEFVAL { "" }
    ::= { nb7-fp1  33 }  

    FP1OutputResetDelay OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Output Reset Delay Seconds for AQL/FPV-G2/FPG/FPO-G2"
    DEFVAL { "" }
    ::= { nb7-fp1  34 }  
    
--
--	FP2
--    
FP2Time OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Time."
    DEFVAL { "" }
    ::= { nb7-fp2  1 }

FP2DeviceID OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "FPO ID."
    DEFVAL { "" }
    ::= { nb7-fp2  2 }

FP2ModNumber OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply Model, Such as FPO75-25, FPO150-100, FPO250-200."
    DEFVAL { "" }
    ::= { nb7-fp2  3 }

FP2SystemFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply system fault status."
    DEFVAL { "" }
    ::= { nb7-fp2  4 }

FP2ACFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply AC lost status, No or Yes."
    DEFVAL { "" }
    ::= { nb7-fp2  5 }

FP2FAIStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI status."
    DEFVAL { "" }
    ::= { nb7-fp2  6 }

FP2OutputLatchingOnFAI OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI latch status."
    DEFVAL { "" }
    ::= { nb7-fp2  7 }
    
FP2ACInputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC input voltage."
    DEFVAL { "" }
    ::= { nb7-fp2  8 }

FP2OutputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output voltage."
    DEFVAL { "" }
    ::= { nb7-fp2  9 }
    
FP2OutputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output Current."
    DEFVAL { "" }
    ::= { nb7-fp2  10 }
    

FP2BatteryVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System battery voltage."
    DEFVAL { "" }
    ::= { nb7-fp2  11 }

FP2BatteryChargeCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery charge current."
    DEFVAL { "" }
    ::= { nb7-fp2  12 }
    
FP2BatteryFaultDetect OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery Fault Detect. For AQL/FPV."
    DEFVAL { "" }
    ::= { nb7-fp2  13 }

FP2TotalPowerupTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power supply total runtime."
    DEFVAL { "" }
    ::= { nb7-fp2  14 }

FP2BatteryInstalledTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery install hours."
    DEFVAL { "" }
    ::= { nb7-fp2  15 }

FP2NumberOfACFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC lost count."
    DEFVAL { "" }
    ::= { nb7-fp2  16 }

FP2NumberOfSystemFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System fault count."
    DEFVAL { "" }
    ::= { nb7-fp2  17 }
	
	
FP2RatedBatteryLife OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "FPO battery lifetime."
    DEFVAL { "" }
    ::= { nb7-fp2  18 }	

	
FP2RatedCapacity  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery capacity."
    DEFVAL { "" }
    ::= { nb7-fp2  19 }	
	
		
FP2BatteryStateOfCharge OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "The FPO battery state of charge."
    DEFVAL { "" }
    ::= { nb7-fp2  20 }	

FP2BatteryStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Enable or Disable calculate battery state of charge."
    DEFVAL { "" }
    ::= { nb7-fp2  21 }		
		
FP2BatteryTestStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery discharge test status, Active or Inactive. Set Value: Testing or Inactive"
    DEFVAL { "" }
    ::= { nb7-fp2  22 }

FP2BatteryLastTestDate OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test date."
    DEFVAL { "" }
    ::= { nb7-fp2  23 }

FP2BatteryLastTestDischargeTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test time."
    DEFVAL { "" }
    ::= { nb7-fp2  24 }
    
FP2RepeatTestInterval OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Repeat Test Interval."
    DEFVAL { "" }
    ::= { nb7-fp2  25 }
    
FP2Version	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "FP2 Ver."
    DEFVAL { "" }
    ::= { nb7-fp2  26 }  
    
FP2SystemFaultDescription	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Fault Description."
    DEFVAL { "" }
    ::= { nb7-fp2  27 }         
    
 FP2BatteryTestsPerformed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Performed."
    DEFVAL { "" }
    ::= { nb7-fp2  28 }   

FP2BatteryTestsFailed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Failed."
    DEFVAL { "" }
    ::= { nb7-fp2  29 }  

FP2RequiredBatteryRuntime	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS   read-write
    STATUS      current
    DESCRIPTION
    "Required Battery Runtime."
    DEFVAL { "" }
    ::= { nb7-fp2  30 }  

FP2ActualStandby	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Actual Standby."
    DEFVAL { "" }
    ::= { nb7-fp2  31 }  

FP2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset output for AQL/FPV-G2/FPG/FPO-G2"
    DEFVAL { "" }
    ::= { nb7-fp2  32 }  

FP2BatteryScheduleTestDateTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "e.g. Enter '2020-01-01 23:01:59' to configure Battery Schedule Test DateTime"
    DEFVAL { "" }
    ::= { nb7-fp2  33 }  

FP2OutputResetDelay OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Output Reset Delay Seconds for AQL/FPV-G2/FPG/FPO-G2"
    DEFVAL { "" }
    ::= { nb7-fp2  34 }  


--
--	FP3
--    
FP3Time OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Time."
    DEFVAL { "" }
    ::= { nb7-fp3  1 }

FP3DeviceID OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "FPO ID."
    DEFVAL { "" }
    ::= { nb7-fp3  2 }

FP3ModNumber OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply Model, Such as FPO75-25, FPO150-100, FPO250-200."
    DEFVAL { "" }
    ::= { nb7-fp3  3 }

FP3SystemFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply system fault status."
    DEFVAL { "" }
    ::= { nb7-fp3  4 }

FP3ACFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply AC lost status, No or Yes."
    DEFVAL { "" }
    ::= { nb7-fp3  5 }

FP3FAIStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI status."
    DEFVAL { "" }
    ::= { nb7-fp3  6 }

FP3OutputLatchingOnFAI OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI latch status."
    DEFVAL { "" }
    ::= { nb7-fp3  7 }
    
FP3ACInputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC input voltage."
    DEFVAL { "" }
    ::= { nb7-fp3  8 }

FP3OutputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output voltage."
    DEFVAL { "" }
    ::= { nb7-fp3  9 }
    
FP3OutputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output Current."
    DEFVAL { "" }
    ::= { nb7-fp3  10 }
    

FP3BatteryVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System battery voltage."
    DEFVAL { "" }
    ::= { nb7-fp3  11 }

FP3BatteryChargeCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery charge current."
    DEFVAL { "" }
    ::= { nb7-fp3  12 }
    
FP3BatteryFaultDetect OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery Fault Detect. For AQL/FPV."
    DEFVAL { "" }
    ::= { nb7-fp3  13 }

FP3TotalPowerupTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power supply total runtime."
    DEFVAL { "" }
    ::= { nb7-fp3  14 }

FP3BatteryInstalledTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery install hours."
    DEFVAL { "" }
    ::= { nb7-fp3  15 }

FP3NumberOfACFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC lost count."
    DEFVAL { "" }
    ::= { nb7-fp3  16 }

FP3NumberOfSystemFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System fault count."
    DEFVAL { "" }
    ::= { nb7-fp3  17 }
	
	
FP3RatedBatteryLife OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "FPO battery lifetime."
    DEFVAL { "" }
    ::= { nb7-fp3  18 }	

	
FP3RatedCapacity  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery capacity."
    DEFVAL { "" }
    ::= { nb7-fp3  19 }	
	
		
FP3BatteryStateOfCharge OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "The FPO battery state of charge."
    DEFVAL { "" }
    ::= { nb7-fp3  20 }	

FP3BatteryStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Enable or Disable calculate battery state of charge."
    DEFVAL { "" }
    ::= { nb7-fp3  21 }		
		
FP3BatteryTestStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery discharge test status, Active or Inactive. Set Value: Testing or Inactive"
    DEFVAL { "" }
    ::= { nb7-fp3  22 }

FP3BatteryLastTestDate OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test date."
    DEFVAL { "" }
    ::= { nb7-fp3  23 }

FP3BatteryLastTestDischargeTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test time."
    DEFVAL { "" }
    ::= { nb7-fp3  24 }
    
FP3RepeatTestInterval OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Repeat Test Interval."
    DEFVAL { "" }
    ::= { nb7-fp3  25 }
    
FP3Version	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "FP3 Ver."
    DEFVAL { "" }
    ::= { nb7-fp3  26 }  
    
FP3SystemFaultDescription	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Fault Description."
    DEFVAL { "" }
    ::= { nb7-fp3  27 }         
    
 FP3BatteryTestsPerformed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Performed."
    DEFVAL { "" }
    ::= { nb7-fp3  28 }   

FP3BatteryTestsFailed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Failed."
    DEFVAL { "" }
    ::= { nb7-fp3  29 }  

FP3RequiredBatteryRuntime	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS   read-write
    STATUS      current
    DESCRIPTION
    "Required Battery Runtime."
    DEFVAL { "" }
    ::= { nb7-fp3  30 }  

FP3ActualStandby	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Actual Standby."
    DEFVAL { "" }
    ::= { nb7-fp3  31 }  

FP3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset output for AQL/FPV-G2/FPG/FPO-G2"
    DEFVAL { "" }
    ::= { nb7-fp3  32 }  

FP3BatteryScheduleTestDateTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "e.g. Enter '2020-01-01 23:01:59' to configure Battery Schedule Test DateTime"
    DEFVAL { "" }
    ::= { nb7-fp3  33 }  

FP3OutputResetDelay OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Output Reset Delay Seconds for AQL/FPV-G2/FPG/FPO-G2"
    DEFVAL { "" }
    ::= { nb7-fp3  34 }  


--
--	FP4
--    
FP4Time OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Time."
    DEFVAL { "" }
    ::= { nb7-fp4  1 }

FP4DeviceID OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "FPO ID."
    DEFVAL { "" }
    ::= { nb7-fp4  2 }

FP4ModNumber OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply Model, Such as FPO75-25, FPO150-100, FPO250-200."
    DEFVAL { "" }
    ::= { nb7-fp4  3 }

FP4SystemFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply system fault status."
    DEFVAL { "" }
    ::= { nb7-fp4  4 }

FP4ACFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply AC lost status, No or Yes."
    DEFVAL { "" }
    ::= { nb7-fp4  5 }

FP4FAIStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI status."
    DEFVAL { "" }
    ::= { nb7-fp4  6 }

FP4OutputLatchingOnFAI OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI latch status."
    DEFVAL { "" }
    ::= { nb7-fp4  7 }
    
FP4ACInputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC input voltage."
    DEFVAL { "" }
    ::= { nb7-fp4  8 }

FP4OutputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output voltage."
    DEFVAL { "" }
    ::= { nb7-fp4  9 }
    
FP4OutputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output Current."
    DEFVAL { "" }
    ::= { nb7-fp4  10 }
    

FP4BatteryVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System battery voltage."
    DEFVAL { "" }
    ::= { nb7-fp4  11 }

FP4BatteryChargeCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery charge current."
    DEFVAL { "" }
    ::= { nb7-fp4  12 }
    
FP4BatteryFaultDetect OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery Fault Detect. For AQL/FPV."
    DEFVAL { "" }
    ::= { nb7-fp4  13 }

FP4TotalPowerupTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power supply total runtime."
    DEFVAL { "" }
    ::= { nb7-fp4  14 }

FP4BatteryInstalledTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery install hours."
    DEFVAL { "" }
    ::= { nb7-fp4  15 }

FP4NumberOfACFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC lost count."
    DEFVAL { "" }
    ::= { nb7-fp4  16 }

FP4NumberOfSystemFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System fault count."
    DEFVAL { "" }
    ::= { nb7-fp4  17 }
	
	
FP4RatedBatteryLife OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "FPO battery lifetime."
    DEFVAL { "" }
    ::= { nb7-fp4  18 }	

	
FP4RatedCapacity  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery capacity."
    DEFVAL { "" }
    ::= { nb7-fp4  19 }	
	
		
FP4BatteryStateOfCharge OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "The FPO battery state of charge."
    DEFVAL { "" }
    ::= { nb7-fp4  20 }	

FP4BatteryStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Enable or Disable calculate battery state of charge."
    DEFVAL { "" }
    ::= { nb7-fp4  21 }		
		
FP4BatteryTestStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery discharge test status, Active or Inactive. Set Value: Testing or Inactive"
    DEFVAL { "" }
    ::= { nb7-fp4  22 }

FP4BatteryLastTestDate OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test date."
    DEFVAL { "" }
    ::= { nb7-fp4  23 }

FP4BatteryLastTestDischargeTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test time."
    DEFVAL { "" }
    ::= { nb7-fp4  24 }
    
FP4RepeatTestInterval OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Repeat Test Interval."
    DEFVAL { "" }
    ::= { nb7-fp4  25 }
    
FP4Version	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "FP4 Ver."
    DEFVAL { "" }
    ::= { nb7-fp4  26 }  
    
FP4SystemFaultDescription	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Fault Description."
    DEFVAL { "" }
    ::= { nb7-fp4  27 }         
    
 FP4BatteryTestsPerformed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Performed."
    DEFVAL { "" }
    ::= { nb7-fp4  28 }   

FP4BatteryTestsFailed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Failed."
    DEFVAL { "" }
    ::= { nb7-fp4  29 }  

FP4RequiredBatteryRuntime	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS   read-write
    STATUS      current
    DESCRIPTION
    "Required Battery Runtime."
    DEFVAL { "" }
    ::= { nb7-fp4  30 }  

FP4ActualStandby	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Actual Standby."
    DEFVAL { "" }
    ::= { nb7-fp4  31 }  

FP4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset output for AQL/FPV-G2/FPG/FPO-G2"
    DEFVAL { "" }
    ::= { nb7-fp4  32 }  

FP4BatteryScheduleTestDateTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "e.g. Enter '2020-01-01 23:01:59' to configure Battery Schedule Test DateTime"
    DEFVAL { "" }
    ::= { nb7-fp4  33 }  

FP4OutputResetDelay OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Output Reset Delay Seconds for AQL/FPV-G2/FPG/FPO-G2"
    DEFVAL { "" }
    ::= { nb7-fp4  34 }  --
--	FP5
--    
FP5Time OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Time."
    DEFVAL { "" }
    ::= { nb7-fp5  1 }

FP5DeviceID OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "FPO ID."
    DEFVAL { "" }
    ::= { nb7-fp5  2 }

FP5ModNumber OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply Model, Such as FPO75-25, FPO150-100, FPO250-200."
    DEFVAL { "" }
    ::= { nb7-fp5  3 }

FP5SystemFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply system fault status."
    DEFVAL { "" }
    ::= { nb7-fp5  4 }

FP5ACFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply AC lost status, No or Yes."
    DEFVAL { "" }
    ::= { nb7-fp5  5 }

FP5FAIStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI status."
    DEFVAL { "" }
    ::= { nb7-fp5  6 }

FP5OutputLatchingOnFAI OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI latch status."
    DEFVAL { "" }
    ::= { nb7-fp5  7 }
    
FP5ACInputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC input voltage."
    DEFVAL { "" }
    ::= { nb7-fp5  8 }

FP5OutputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output voltage."
    DEFVAL { "" }
    ::= { nb7-fp5  9 }
    
FP5OutputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output Current."
    DEFVAL { "" }
    ::= { nb7-fp5  10 }
    

FP5BatteryVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System battery voltage."
    DEFVAL { "" }
    ::= { nb7-fp5  11 }

FP5BatteryChargeCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery charge current."
    DEFVAL { "" }
    ::= { nb7-fp5  12 }
    
FP5BatteryFaultDetect OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery Fault Detect. For AQL/FPV."
    DEFVAL { "" }
    ::= { nb7-fp5  13 }

FP5TotalPowerupTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power supply total runtime."
    DEFVAL { "" }
    ::= { nb7-fp5  14 }

FP5BatteryInstalledTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery install hours."
    DEFVAL { "" }
    ::= { nb7-fp5  15 }

FP5NumberOfACFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC lost count."
    DEFVAL { "" }
    ::= { nb7-fp5  16 }

FP5NumberOfSystemFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System fault count."
    DEFVAL { "" }
    ::= { nb7-fp5  17 }
	
	
FP5RatedBatteryLife OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "FPO battery lifetime."
    DEFVAL { "" }
    ::= { nb7-fp5  18 }	

	
FP5RatedCapacity  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery capacity."
    DEFVAL { "" }
    ::= { nb7-fp5  19 }	
	
		
FP5BatteryStateOfCharge OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "The FPO battery state of charge."
    DEFVAL { "" }
    ::= { nb7-fp5  20 }	

FP5BatteryStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Enable or Disable calculate battery state of charge."
    DEFVAL { "" }
    ::= { nb7-fp5  21 }		
		
FP5BatteryTestStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery discharge test status, Active or Inactive. Set Value: Testing or Inactive"
    DEFVAL { "" }
    ::= { nb7-fp5  22 }

FP5BatteryLastTestDate OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test date."
    DEFVAL { "" }
    ::= { nb7-fp5  23 }

FP5BatteryLastTestDischargeTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test time."
    DEFVAL { "" }
    ::= { nb7-fp5  24 }
    
FP5RepeatTestInterval OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Repeat Test Interval."
    DEFVAL { "" }
    ::= { nb7-fp5  25 }
    
FP5Version	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "FP5 Ver."
    DEFVAL { "" }
    ::= { nb7-fp5  26 }  
    
FP5SystemFaultDescription	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Fault Description."
    DEFVAL { "" }
    ::= { nb7-fp5  27 }         
    
 FP5BatteryTestsPerformed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Performed."
    DEFVAL { "" }
    ::= { nb7-fp5  28 }   

FP5BatteryTestsFailed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Failed."
    DEFVAL { "" }
    ::= { nb7-fp5  29 }  

FP5RequiredBatteryRuntime	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS   read-write
    STATUS      current
    DESCRIPTION
    "Required Battery Runtime."
    DEFVAL { "" }
    ::= { nb7-fp5  30 }  

FP5ActualStandby	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Actual Standby."
    DEFVAL { "" }
    ::= { nb7-fp5  31 }  

FP5ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset output for AQL/FPV-G2/FPG/FPO-G2"
    DEFVAL { "" }
    ::= { nb7-fp5  32 }  

FP5BatteryScheduleTestDateTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "e.g. Enter '2020-01-01 23:01:59' to configure Battery Schedule Test DateTime"
    DEFVAL { "" }
    ::= { nb7-fp5  33 }  

FP5OutputResetDelay OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Output Reset Delay Seconds for AQL/FPV-G2/FPG/FPO-G2"
    DEFVAL { "" }
    ::= { nb7-fp5  34 }  

--
--	FP6
--    
FP6Time OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Time."
    DEFVAL { "" }
    ::= { nb7-fp6  1 }

FP6DeviceID OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "FPO ID."
    DEFVAL { "" }
    ::= { nb7-fp6  2 }

FP6ModNumber OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply Model, Such as FPO75-25, FPO150-100, FPO250-200."
    DEFVAL { "" }
    ::= { nb7-fp6  3 }

FP6SystemFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply system fault status."
    DEFVAL { "" }
    ::= { nb7-fp6  4 }

FP6ACFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply AC lost status, No or Yes."
    DEFVAL { "" }
    ::= { nb7-fp6  5 }

FP6FAIStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI status."
    DEFVAL { "" }
    ::= { nb7-fp6  6 }

FP6OutputLatchingOnFAI OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI latch status."
    DEFVAL { "" }
    ::= { nb7-fp6  7 }
    
FP6ACInputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC input voltage."
    DEFVAL { "" }
    ::= { nb7-fp6  8 }

FP6OutputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output voltage."
    DEFVAL { "" }
    ::= { nb7-fp6  9 }
    
FP6OutputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output Current."
    DEFVAL { "" }
    ::= { nb7-fp6  10 }
    

FP6BatteryVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System battery voltage."
    DEFVAL { "" }
    ::= { nb7-fp6  11 }

FP6BatteryChargeCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery charge current."
    DEFVAL { "" }
    ::= { nb7-fp6  12 }
    
FP6BatteryFaultDetect OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery Fault Detect. For AQL/FPV."
    DEFVAL { "" }
    ::= { nb7-fp6  13 }

FP6TotalPowerupTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power supply total runtime."
    DEFVAL { "" }
    ::= { nb7-fp6  14 }

FP6BatteryInstalledTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery install hours."
    DEFVAL { "" }
    ::= { nb7-fp6  15 }

FP6NumberOfACFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC lost count."
    DEFVAL { "" }
    ::= { nb7-fp6  16 }

FP6NumberOfSystemFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System fault count."
    DEFVAL { "" }
    ::= { nb7-fp6  17 }
	
	
FP6RatedBatteryLife OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "FPO battery lifetime."
    DEFVAL { "" }
    ::= { nb7-fp6  18 }	

	
FP6RatedCapacity  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery capacity."
    DEFVAL { "" }
    ::= { nb7-fp6  19 }	
	
		
FP6BatteryStateOfCharge OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "The FPO battery state of charge."
    DEFVAL { "" }
    ::= { nb7-fp6  20 }	

FP6BatteryStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Enable or Disable calculate battery state of charge."
    DEFVAL { "" }
    ::= { nb7-fp6  21 }		
		
FP6BatteryTestStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery discharge test status, Active or Inactive. Set Value: Testing or Inactive"
    DEFVAL { "" }
    ::= { nb7-fp6  22 }

FP6BatteryLastTestDate OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test date."
    DEFVAL { "" }
    ::= { nb7-fp6  23 }

FP6BatteryLastTestDischargeTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test time."
    DEFVAL { "" }
    ::= { nb7-fp6  24 }
    
FP6RepeatTestInterval OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Repeat Test Interval."
    DEFVAL { "" }
    ::= { nb7-fp6  25 }
    
FP6Version	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "FP6 Ver."
    DEFVAL { "" }
    ::= { nb7-fp6  26 }  
    
FP6SystemFaultDescription	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Fault Description."
    DEFVAL { "" }
    ::= { nb7-fp6  27 }         
    
 FP6BatteryTestsPerformed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Performed."
    DEFVAL { "" }
    ::= { nb7-fp6  28 }   

FP6BatteryTestsFailed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Failed."
    DEFVAL { "" }
    ::= { nb7-fp6  29 }  

FP6RequiredBatteryRuntime	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS   read-write
    STATUS      current
    DESCRIPTION
    "Required Battery Runtime."
    DEFVAL { "" }
    ::= { nb7-fp6  30 }  

FP6ActualStandby	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Actual Standby."
    DEFVAL { "" }
    ::= { nb7-fp6  31 }  

FP6ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset output for AQL/FPV-G2/FPG/FPO-G2"
    DEFVAL { "" }
    ::= { nb7-fp6  32 }  

FP6BatteryScheduleTestDateTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "e.g. Enter '2020-01-01 23:01:59' to configure Battery Schedule Test DateTime"
    DEFVAL { "" }
    ::= { nb7-fp6  33 }  

FP6OutputResetDelay OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Output Reset Delay Seconds for AQL/FPV-G2/FPG/FPO-G2"
    DEFVAL { "" }
    ::= { nb7-fp6  34 }  



--
--	FP7
--    
FP7Time OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Time."
    DEFVAL { "" }
    ::= { nb7-fp7  1 }

FP7DeviceID OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "FPO ID."
    DEFVAL { "" }
    ::= { nb7-fp7  2 }

FP7ModNumber OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply Model, Such as FPO75-25, FPO150-100, FPO250-200."
    DEFVAL { "" }
    ::= { nb7-fp7  3 }

FP7SystemFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply system fault status."
    DEFVAL { "" }
    ::= { nb7-fp7  4 }

FP7ACFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply AC lost status, No or Yes."
    DEFVAL { "" }
    ::= { nb7-fp7  5 }

FP7FAIStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI status."
    DEFVAL { "" }
    ::= { nb7-fp7  6 }

FP7OutputLatchingOnFAI OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI latch status."
    DEFVAL { "" }
    ::= { nb7-fp7  7 }
    
FP7ACInputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC input voltage."
    DEFVAL { "" }
    ::= { nb7-fp7  8 }

FP7OutputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output voltage."
    DEFVAL { "" }
    ::= { nb7-fp7  9 }
    
FP7OutputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output Current."
    DEFVAL { "" }
    ::= { nb7-fp7  10 }
    

FP7BatteryVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System battery voltage."
    DEFVAL { "" }
    ::= { nb7-fp7  11 }

FP7BatteryChargeCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery charge current."
    DEFVAL { "" }
    ::= { nb7-fp7  12 }
    
FP7BatteryFaultDetect OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery Fault Detect. For AQL/FPV."
    DEFVAL { "" }
    ::= { nb7-fp7  13 }

FP7TotalPowerupTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power supply total runtime."
    DEFVAL { "" }
    ::= { nb7-fp7  14 }

FP7BatteryInstalledTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery install hours."
    DEFVAL { "" }
    ::= { nb7-fp7  15 }

FP7NumberOfACFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC lost count."
    DEFVAL { "" }
    ::= { nb7-fp7  16 }

FP7NumberOfSystemFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System fault count."
    DEFVAL { "" }
    ::= { nb7-fp7  17 }
	
	
FP7RatedBatteryLife OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "FPO battery lifetime."
    DEFVAL { "" }
    ::= { nb7-fp7  18 }	

	
FP7RatedCapacity  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery capacity."
    DEFVAL { "" }
    ::= { nb7-fp7  19 }	
	
		
FP7BatteryStateOfCharge OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "The FPO battery state of charge."
    DEFVAL { "" }
    ::= { nb7-fp7  20 }	

FP7BatteryStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Enable or Disable calculate battery state of charge."
    DEFVAL { "" }
    ::= { nb7-fp7  21 }		
		
FP7BatteryTestStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery discharge test status, Active or Inactive. Set Value: Testing or Inactive"
    DEFVAL { "" }
    ::= { nb7-fp7  22 }

FP7BatteryLastTestDate OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test date."
    DEFVAL { "" }
    ::= { nb7-fp7  23 }

FP7BatteryLastTestDischargeTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test time."
    DEFVAL { "" }
    ::= { nb7-fp7  24 }
    
FP7RepeatTestInterval OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Repeat Test Interval."
    DEFVAL { "" }
    ::= { nb7-fp7  25 }
    
FP7Version	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "FP7 Ver."
    DEFVAL { "" }
    ::= { nb7-fp7  26 }  
    
FP7SystemFaultDescription	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Fault Description."
    DEFVAL { "" }
    ::= { nb7-fp7  27 }         
    
 FP7BatteryTestsPerformed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Performed."
    DEFVAL { "" }
    ::= { nb7-fp7  28 }   

FP7BatteryTestsFailed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Failed."
    DEFVAL { "" }
    ::= { nb7-fp7  29 }  

FP7RequiredBatteryRuntime	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS   read-write
    STATUS      current
    DESCRIPTION
    "Required Battery Runtime."
    DEFVAL { "" }
    ::= { nb7-fp7  30 }  

FP7ActualStandby	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Actual Standby."
    DEFVAL { "" }
    ::= { nb7-fp7  31 }  

FP7ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset output for AQL/FPV-G2/FPG/FPO-G2"
    DEFVAL { "" }
    ::= { nb7-fp7  32 }  

FP7BatteryScheduleTestDateTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "e.g. Enter '2020-01-01 23:01:59' to configure Battery Schedule Test DateTime"
    DEFVAL { "" }
    ::= { nb7-fp7  33 }  

FP7OutputResetDelay OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Output Reset Delay Seconds for AQL/FPV-G2/FPG/FPO-G2"
    DEFVAL { "" }
    ::= { nb7-fp7  34 }  



--
--	FP8
--    
FP8Time OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Time."
    DEFVAL { "" }
    ::= { nb7-fp8  1 }

FP8DeviceID OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "FPO ID."
    DEFVAL { "" }
    ::= { nb7-fp8  2 }

FP8ModNumber OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply Model, Such as FPO75-25, FPO150-100, FPO250-200."
    DEFVAL { "" }
    ::= { nb7-fp8  3 }

FP8SystemFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply system fault status."
    DEFVAL { "" }
    ::= { nb7-fp8  4 }

FP8ACFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply AC lost status, No or Yes."
    DEFVAL { "" }
    ::= { nb7-fp8  5 }

FP8FAIStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI status."
    DEFVAL { "" }
    ::= { nb7-fp8  6 }

FP8OutputLatchingOnFAI OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI latch status."
    DEFVAL { "" }
    ::= { nb7-fp8  7 }
    
FP8ACInputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC input voltage."
    DEFVAL { "" }
    ::= { nb7-fp8  8 }

FP8OutputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output voltage."
    DEFVAL { "" }
    ::= { nb7-fp8  9 }
    
FP8OutputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output Current."
    DEFVAL { "" }
    ::= { nb7-fp8  10 }
    

FP8BatteryVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System battery voltage."
    DEFVAL { "" }
    ::= { nb7-fp8  11 }

FP8BatteryChargeCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery charge current."
    DEFVAL { "" }
    ::= { nb7-fp8  12 }
    
FP8BatteryFaultDetect OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery Fault Detect. For AQL/FPV."
    DEFVAL { "" }
    ::= { nb7-fp8  13 }

FP8TotalPowerupTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power supply total runtime."
    DEFVAL { "" }
    ::= { nb7-fp8  14 }

FP8BatteryInstalledTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery install hours."
    DEFVAL { "" }
    ::= { nb7-fp8  15 }

FP8NumberOfACFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC lost count."
    DEFVAL { "" }
    ::= { nb7-fp8  16 }

FP8NumberOfSystemFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System fault count."
    DEFVAL { "" }
    ::= { nb7-fp8  17 }
	
	
FP8RatedBatteryLife OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "FPO battery lifetime."
    DEFVAL { "" }
    ::= { nb7-fp8  18 }	

	
FP8RatedCapacity  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery capacity."
    DEFVAL { "" }
    ::= { nb7-fp8  19 }	
	
		
FP8BatteryStateOfCharge OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "The FPO battery state of charge."
    DEFVAL { "" }
    ::= { nb7-fp8  20 }	

FP8BatteryStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Enable or Disable calculate battery state of charge."
    DEFVAL { "" }
    ::= { nb7-fp8  21 }		
		
FP8BatteryTestStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery discharge test status, Active or Inactive. Set Value: Testing or Inactive"
    DEFVAL { "" }
    ::= { nb7-fp8  22 }

FP8BatteryLastTestDate OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test date."
    DEFVAL { "" }
    ::= { nb7-fp8  23 }

FP8BatteryLastTestDischargeTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test time."
    DEFVAL { "" }
    ::= { nb7-fp8  24 }
    
FP8RepeatTestInterval OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Repeat Test Interval."
    DEFVAL { "" }
    ::= { nb7-fp8  25 }
    
FP8Version	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "FP8 Ver."
    DEFVAL { "" }
    ::= { nb7-fp8  26 }  
    
FP8SystemFaultDescription	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Fault Description."
    DEFVAL { "" }
    ::= { nb7-fp8  27 }         
    
 FP8BatteryTestsPerformed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Performed."
    DEFVAL { "" }
    ::= { nb7-fp8  28 }   

FP8BatteryTestsFailed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Failed."
    DEFVAL { "" }
    ::= { nb7-fp8  29 }  

FP8RequiredBatteryRuntime	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS   read-write
    STATUS      current
    DESCRIPTION
    "Required Battery Runtime."
    DEFVAL { "" }
    ::= { nb7-fp8  30 }  

FP8ActualStandby	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Actual Standby."
    DEFVAL { "" }
    ::= { nb7-fp8  31 }  

FP8ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset output for AQL/FPV-G2/FPG/FPO-G2"
    DEFVAL { "" }
    ::= { nb7-fp8  32 }  

FP8BatteryScheduleTestDateTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "e.g. Enter '2020-01-01 23:01:59' to configure Battery Schedule Test DateTime"
    DEFVAL { "" }
    ::= { nb7-fp8  33 }  

FP8OutputResetDelay OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Output Reset Delay Seconds for AQL/FPV-G2/FPG/FPO-G2"
    DEFVAL { "" }
    ::= { nb7-fp8  34 }  



--
--	nb7-m8-1
--    		

m8-1-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { nb7-m8-1-1  1 }

m8-1-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { nb7-m8-1-1  2 }

m8-1-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { nb7-m8-1-1  3 }

m8-1-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { nb7-m8-1-1  4 }
	
m8-1-1PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- power supply."
    DEFVAL { "" }
    ::= { nb7-m8-1-1  5 }	
	
	
m8-1-1ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- Output response to control input, Active, Inactive or Disable."
    DEFVAL { "" }
    ::= { nb7-m8-1-1  6 }		
	
m8-1-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { nb7-m8-1-1  7 }		
	
	
m8-1-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { nb7-m8-1-1  8 }

m8-1-1CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- control Input Type, Normally Open, Normally Closed,
    Open Collector, Voltage, Disabled."
    DEFVAL { "" }
    ::= { nb7-m8-1-1  9 }	
	
	
m8-1-1OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- output load type, Maglock, Fail-safe Strike, 
    Fail-secure Strike, Constant ON."
    DEFVAL { "" }
    ::= { nb7-m8-1-1  10 }	
	
m8-1-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- unlock on FAI Activation, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-1-1  11 }	
	
	
m8-1-1UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- unlock on AC loss, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-1-1  12 }	
	
m8-1-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-1-1  13 }		
	
m8-1-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { nb7-m8-1-1  14 }		
	
m8-1-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { nb7-m8-1-1  15 }	
	
m8-1-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { nb7-m8-1-1  16 }	
	

m8-1-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { nb7-m8-1-1  17 }	

m8-1-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable M8 -."
    DEFVAL { "" }
    ::= { nb7-m8-1-1  18 }	

m8-1-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-1-1  19 }	

m8-1-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-1-1  20 }	

m8-1-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-1-1  21 }	
    
--
--	nb7-m8-1
--    



m8-1-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-2  1 }

m8-1-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-2  2 }

m8-1-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-2  3 }

m8-1-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-2  4 }
	
m8-1-2PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-2  5 }	
	
	
m8-1-2ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-2  6 }		
	
m8-1-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-2  7 }		
	
	
m8-1-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-2  8 }		

m8-1-2CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-2  9 }	
	
m8-1-2OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-2  10 }	

m8-1-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-2  11 }	
	
	
m8-1-2UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-2  12 }	
	
m8-1-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-2  13 }		
	
m8-1-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-2  14 }		
	
m8-1-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-2  15 }	
	
m8-1-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-2  16 }	
	

m8-1-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-2  17 }		

	
m8-1-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-2  18 }	

m8-1-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-1-2  19 }

m8-1-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-1-2  20 }	

m8-1-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-1-2  21 }		
	
--
--	nb7-m8-1
--    
	

m8-1-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-3  1 }

m8-1-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-3  2 }

m8-1-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-3  3 }

m8-1-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-3  4 }
	
m8-1-3PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-3  5 }	
	
	
m8-1-3ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-3  6 }		
	
m8-1-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-3  7 }		
	
	
m8-1-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-3  8 }
	

m8-1-3CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-3  9 }


m8-1-3OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-3  10 }	
	

m8-1-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-3  11 }	
	
	
m8-1-3UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-3  12 }	
	
m8-1-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-3  13 }		
	
m8-1-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-3  14 }		
	
m8-1-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-3  15 }	
	
m8-1-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-3  16 }	
	

m8-1-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-3  17 }	


m8-1-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-3  18 }	

m8-1-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-1-3  19 }	

m8-1-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-1-3  20 }	

m8-1-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-1-3  21 }	
	
--
--	nb7-m8-1
--    
	
	

m8-1-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-4  1 }

m8-1-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-4  2 }

m8-1-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-4  3 }

m8-1-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-4  4 }
	
m8-1-4PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-4  5 }	
	
	
m8-1-4ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-4  6 }		
	
m8-1-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-4  7 }		
	
	
m8-1-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-4  8 }		
	

m8-1-4CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-4  9 }	
	

m8-1-4OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-4  10 }	


m8-1-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-4  11 }	
	
	
m8-1-4UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-4  12 }	
	
m8-1-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-4  13 }		
	
m8-1-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-4  14 }		
	
m8-1-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-4  15 }	
	
m8-1-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-4  16 }	
	

m8-1-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-4  17 }	

	
m8-1-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-4  18 }	

m8-1-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-1-4  19 }	

m8-1-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-1-4  20 }	

m8-1-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-1-4  21 }	

	
--
--	nb7-m8-1
--    

	
	

m8-1-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-5  1 }

m8-1-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-5  2 }

m8-1-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-5  3 }

m8-1-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-5  4 }
	
m8-1-5PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-5  5 }	
	
	
m8-1-5ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-5  6 }		
	
m8-1-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-5  7 }		
	
	
m8-1-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-5  8 }	
	

m8-1-5CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-5  9 }
	
	
m8-1-5OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-5  10 }	
	
	
m8-1-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-5  11 }	
	
	
m8-1-5UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-5  12 }	
	
m8-1-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-5  13 }		
	
m8-1-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-5  14 }		
	
m8-1-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-5  15 }	
	
m8-1-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-5  16 }	
	

m8-1-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-5  17 }	

m8-1-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-5  18 }	

m8-1-5ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-1-5  19 }	

m8-1-5CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-1-5  20 }	

m8-1-5CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-1-5  21 }		
	
--
--	nb7-m8-1
--    
	

m8-1-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-6  1 }

m8-1-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-6  2 }

m8-1-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-6  3 }

m8-1-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-6  4 }
	
m8-1-6PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-6  5 }	
	
	
m8-1-6ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-6  6 }		
	
m8-1-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-6  7 }		
	
	
m8-1-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-6  8 }	


m8-1-6CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-6  9 }

	
m8-1-6OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-6  10 }	
	
m8-1-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-6  11 }	
	
	
m8-1-6UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-6  12 }	
	
m8-1-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-6  13 }		
	
m8-1-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-6  14 }		
	
m8-1-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-6  15 }	
	
m8-1-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-6  16 }	
	

m8-1-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-6  17 }	

	
m8-1-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-6  18 }	

m8-1-6ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-1-6  19 }	

m8-1-6CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-1-6  20 }	

m8-1-6CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-1-6  21 }		
	
--
--	nb7-m8-1
--    

m8-1-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-7  1 }

m8-1-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-7  2 }

m8-1-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-7  3 }

m8-1-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-7  4 }
	
m8-1-7PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-7  5 }	
	
	
m8-1-7ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-7  6 }		
	
m8-1-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-7  7 }		
	
	
m8-1-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-7  8 }	


m8-1-7CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-7  9 }

m8-1-7OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-7  10 }	

m8-1-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-7  11 }	
	
	
m8-1-7UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-7  12 }	
	
m8-1-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-7  13 }		
	
m8-1-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-7  14 }		
	
m8-1-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-7  15 }	
	
m8-1-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-7  16 }	
	

m8-1-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-7  17 }		

m8-1-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-7  18 }	

m8-1-7ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-1-7  19 }	

m8-1-7CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-1-7  20 }	

m8-1-7CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-1-7  21 }		
	
--
--	nb7-m8-1
--    	

m8-1-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-8  1 }

m8-1-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-8  2 }

m8-1-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-8  3 }

m8-1-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-8  4 }
	
m8-1-8PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-8  5 }	
	
	
m8-1-8ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-8  6 }		
	
m8-1-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-8  7 }		
	
	
m8-1-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-8  8 }		
	
	
m8-1-8CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-8  9 }


m8-1-8OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-8  10 }	

m8-1-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-8  11 }	
	
	
m8-1-8UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-8  12 }	
	
m8-1-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-8  13 }		
	
m8-1-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-8  14 }		
	
m8-1-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-8  15 }	
	
m8-1-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-8  16 }	
	

m8-1-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-8  17 }		

m8-1-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1-8  18 }	

m8-1-8ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-1-8  19 }	

m8-1-8CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-1-8  20 }	

m8-1-8CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-1-8  21 }	

	
	
m8-1Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1  9 }	
    
m8-1VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1  10 }

m8-1VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1  11 }

m8-1CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1  12 }

m8-1CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1  13 }
    
m8-1Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-1  14 }


--
--	nb7-m8-2
--    		

m8-2-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { nb7-m8-2-1  1 }

m8-2-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { nb7-m8-2-1  2 }

m8-2-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { nb7-m8-2-1  3 }

m8-2-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { nb7-m8-2-1  4 }
	
m8-2-1PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- power supply."
    DEFVAL { "" }
    ::= { nb7-m8-2-1  5 }	
	
	
m8-2-1ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- Output response to control input, Active, Inactive or Disable."
    DEFVAL { "" }
    ::= { nb7-m8-2-1  6 }		
	
m8-2-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { nb7-m8-2-1  7 }		
	
	
m8-2-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { nb7-m8-2-1  8 }

m8-2-1CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- control Input Type, Normally Open, Normally Closed,
    Open Collector, Voltage, Disabled."
    DEFVAL { "" }
    ::= { nb7-m8-2-1  9 }	
	
	
m8-2-1OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- output load type, Maglock, Fail-safe Strike, 
    Fail-secure Strike, Constant ON."
    DEFVAL { "" }
    ::= { nb7-m8-2-1  10 }	
	
m8-2-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- unlock on FAI Activation, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-2-1  11 }	
	
	
m8-2-1UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- unlock on AC loss, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-2-1  12 }	
	
m8-2-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-2-1  13 }		
	
m8-2-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { nb7-m8-2-1  14 }		
	
m8-2-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { nb7-m8-2-1  15 }	
	
m8-2-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { nb7-m8-2-1  16 }	
	

m8-2-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { nb7-m8-2-1  17 }	

m8-2-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable M8 -."
    DEFVAL { "" }
    ::= { nb7-m8-2-1  18 }	

m8-2-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-2-1  19 }	

m8-2-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-2-1  20 }	

m8-2-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-2-1  21 }		
    
--
--	nb7-m8-2
--    



m8-2-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-2  1 }

m8-2-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-2  2 }

m8-2-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-2  3 }

m8-2-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-2  4 }
	
m8-2-2PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-2  5 }	
	
	
m8-2-2ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-2  6 }		
	
m8-2-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-2  7 }		
	
	
m8-2-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-2  8 }		

m8-2-2CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-2  9 }	
	
m8-2-2OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-2  10 }	

m8-2-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-2  11 }	
	
	
m8-2-2UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-2  12 }	
	
m8-2-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-2  13 }		
	
m8-2-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-2  14 }		
	
m8-2-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-2  15 }	
	
m8-2-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-2  16 }	
	

m8-2-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-2  17 }		

	
m8-2-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-2  18 }	

m8-2-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-2-2  19 }	

m8-2-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-2-2  20 }	

m8-2-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-2-2  21 }	
	
--
--	nb7-m8-2
--    
	

m8-2-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-3  1 }

m8-2-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-3  2 }

m8-2-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-3  3 }

m8-2-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-3  4 }
	
m8-2-3PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-3  5 }	
	
	
m8-2-3ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-3  6 }		
	
m8-2-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-3  7 }		
	
	
m8-2-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-3  8 }
	

m8-2-3CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-3  9 }


m8-2-3OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-3  10 }	
	

m8-2-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-3  11 }	
	
	
m8-2-3UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-3  12 }	
	
m8-2-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-3  13 }		
	
m8-2-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-3  14 }		
	
m8-2-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-3  15 }	
	
m8-2-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-3  16 }	
	

m8-2-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-3  17 }	


m8-2-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-3  18 }	

m8-2-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-2-3  19 }	

m8-2-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-2-3  20 }	

m8-2-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-2-3  21 }	
	
--
--	nb7-m8-2
--    
	
	

m8-2-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-4  1 }

m8-2-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-4  2 }

m8-2-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-4  3 }

m8-2-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-4  4 }
	
m8-2-4PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-4  5 }	
	
	
m8-2-4ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-4  6 }		
	
m8-2-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-4  7 }		
	
	
m8-2-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-4  8 }		
	

m8-2-4CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-4  9 }	
	

m8-2-4OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-4  10 }	


m8-2-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-4  11 }	
	
	
m8-2-4UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-4  12 }	
	
m8-2-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-4  13 }		
	
m8-2-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-4  14 }		
	
m8-2-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-4  15 }	
	
m8-2-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-4  16 }	
	

m8-2-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-4  17 }	

	
m8-2-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-4  18 }	

m8-2-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-2-4  19 }	

m8-2-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-2-4  20 }	

m8-2-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-2-4  21 }	

	
--
--	nb7-m8-2
--    

	
	

m8-2-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-5  1 }

m8-2-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-5  2 }

m8-2-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-5  3 }

m8-2-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-5  4 }
	
m8-2-5PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-5  5 }	
	
	
m8-2-5ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-5  6 }		
	
m8-2-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-5  7 }		
	
	
m8-2-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-5  8 }	
	

m8-2-5CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-5  9 }
	
	
m8-2-5OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-5  10 }	
	
	
m8-2-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-5  11 }	
	
	
m8-2-5UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-5  12 }	
	
m8-2-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-5  13 }		
	
m8-2-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-5  14 }		
	
m8-2-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-5  15 }	
	
m8-2-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-5  16 }	
	

m8-2-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-5  17 }	

m8-2-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-5  18 }	

m8-2-5ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-2-5  19 }	

m8-2-5CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-2-5  20 }	

m8-2-5CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-2-5  21 }		
	
--
--	nb7-m8-2
--    
	

m8-2-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-6  1 }

m8-2-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-6  2 }

m8-2-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-6  3 }

m8-2-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-6  4 }
	
m8-2-6PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-6  5 }	
	
	
m8-2-6ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-6  6 }		
	
m8-2-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-6  7 }		
	
	
m8-2-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-6  8 }	


m8-2-6CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-6  9 }

	
m8-2-6OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-6  10 }	
	
m8-2-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-6  11 }	
	
	
m8-2-6UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-6  12 }	
	
m8-2-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-6  13 }		
	
m8-2-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-6  14 }		
	
m8-2-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-6  15 }	
	
m8-2-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-6  16 }	
	

m8-2-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-6  17 }	

	
m8-2-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-6  18 }	

m8-2-6ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-2-6  19 }	

m8-2-6CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-2-6  20 }	

m8-2-6CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-2-6  21 }		
	
--
--	nb7-m8-2
--    

m8-2-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-7  1 }

m8-2-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-7  2 }

m8-2-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-7  3 }

m8-2-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-7  4 }
	
m8-2-7PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-7  5 }	
	
	
m8-2-7ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-7  6 }		
	
m8-2-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-7  7 }		
	
	
m8-2-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-7  8 }	


m8-2-7CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-7  9 }

m8-2-7OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-7  10 }	

m8-2-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-7  11 }	
	
	
m8-2-7UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-7  12 }	
	
m8-2-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-7  13 }		
	
m8-2-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-7  14 }		
	
m8-2-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-7  15 }	
	
m8-2-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-7  16 }	
	

m8-2-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-7  17 }		

m8-2-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-7  18 }	

m8-2-7ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-2-7  19 }	

m8-2-7CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-2-7  20 }	

m8-2-7CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-2-7  21 }		
	
--
--	nb7-m8-2
--    	

m8-2-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-8  1 }

m8-2-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-8  2 }

m8-2-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-8  3 }

m8-2-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-8  4 }
	
m8-2-8PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-8  5 }	
	
	
m8-2-8ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-8  6 }		
	
m8-2-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-8  7 }		
	
	
m8-2-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-8  8 }		
	
	
m8-2-8CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-8  9 }


m8-2-8OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-8  10 }	

m8-2-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-8  11 }	
	
	
m8-2-8UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-8  12 }	
	
m8-2-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-8  13 }		
	
m8-2-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-8  14 }		
	
m8-2-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-8  15 }	
	
m8-2-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-8  16 }	
	

m8-2-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-8  17 }		

m8-2-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2-8  18 }	

m8-2-8ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-2-8  19 }	

m8-2-8CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-2-8  20 }	

m8-2-8CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-2-8  21 }	
	
	
m8-2Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2  9 }	
    
m8-2VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2  10 }

m8-2VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2  11 }

m8-2CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2  12 }

m8-2CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2  13 }
    
m8-2Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-2  14 }


--
--	nb7-m8-3
--    		

m8-3-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { nb7-m8-3-1  1 }

m8-3-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { nb7-m8-3-1  2 }

m8-3-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { nb7-m8-3-1  3 }

m8-3-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { nb7-m8-3-1  4 }
	
m8-3-1PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- power supply."
    DEFVAL { "" }
    ::= { nb7-m8-3-1  5 }	
	
	
m8-3-1ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- Output response to control input, Active, Inactive or Disable."
    DEFVAL { "" }
    ::= { nb7-m8-3-1  6 }		
	
m8-3-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { nb7-m8-3-1  7 }		
	
	
m8-3-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { nb7-m8-3-1  8 }

m8-3-1CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- control Input Type, Normally Open, Normally Closed,
    Open Collector, Voltage, Disabled."
    DEFVAL { "" }
    ::= { nb7-m8-3-1  9 }	
	
	
m8-3-1OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- output load type, Maglock, Fail-safe Strike, 
    Fail-secure Strike, Constant ON."
    DEFVAL { "" }
    ::= { nb7-m8-3-1  10 }	
	
m8-3-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- unlock on FAI Activation, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-3-1  11 }	
	
	
m8-3-1UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- unlock on AC loss, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-3-1  12 }	
	
m8-3-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-3-1  13 }		
	
m8-3-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { nb7-m8-3-1  14 }		
	
m8-3-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { nb7-m8-3-1  15 }	
	
m8-3-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { nb7-m8-3-1  16 }	
	

m8-3-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { nb7-m8-3-1  17 }	

m8-3-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable M8 -."
    DEFVAL { "" }
    ::= { nb7-m8-3-1  18 }	

m8-3-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-3-1  19 }	

m8-3-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-3-1  20 }	

m8-3-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-3-1  21 }		
    
--
--	nb7-m8-3
--    



m8-3-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-2  1 }

m8-3-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-2  2 }

m8-3-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-2  3 }

m8-3-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-2  4 }
	
m8-3-2PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-2  5 }	
	
	
m8-3-2ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-2  6 }		
	
m8-3-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-2  7 }		
	
	
m8-3-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-2  8 }		

m8-3-2CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-2  9 }	
	
m8-3-2OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-2  10 }	

m8-3-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-2  11 }	
	
	
m8-3-2UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-2  12 }	
	
m8-3-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-2  13 }		
	
m8-3-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-2  14 }		
	
m8-3-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-2  15 }	
	
m8-3-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-2  16 }	
	

m8-3-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-2  17 }		

	
m8-3-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-2  18 }	

m8-3-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-3-2  19 }	

m8-3-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-3-2  20 }	

m8-3-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-3-2  21 }	
	
--
--	nb7-m8-3
--    
	

m8-3-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-3  1 }

m8-3-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-3  2 }

m8-3-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-3  3 }

m8-3-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-3  4 }
	
m8-3-3PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-3  5 }	
	
	
m8-3-3ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-3  6 }		
	
m8-3-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-3  7 }		
	
	
m8-3-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-3  8 }
	

m8-3-3CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-3  9 }


m8-3-3OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-3  10 }	
	

m8-3-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-3  11 }	
	
	
m8-3-3UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-3  12 }	
	
m8-3-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-3  13 }		
	
m8-3-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-3  14 }		
	
m8-3-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-3  15 }	
	
m8-3-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-3  16 }	
	

m8-3-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-3  17 }	


m8-3-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-3  18 }	

m8-3-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-3-3  19 }	

m8-3-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-3-3  20 }	

m8-3-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-3-3  21 }	
	
--
--	nb7-m8-3
--    
	
	

m8-3-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-4  1 }

m8-3-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-4  2 }

m8-3-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-4  3 }

m8-3-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-4  4 }
	
m8-3-4PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-4  5 }	
	
	
m8-3-4ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-4  6 }		
	
m8-3-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-4  7 }		
	
	
m8-3-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-4  8 }		
	

m8-3-4CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-4  9 }	
	

m8-3-4OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-4  10 }	


m8-3-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-4  11 }	
	
	
m8-3-4UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-4  12 }	
	
m8-3-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-4  13 }		
	
m8-3-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-4  14 }		
	
m8-3-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-4  15 }	
	
m8-3-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-4  16 }	
	

m8-3-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-4  17 }	

	
m8-3-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-4  18 }	

m8-3-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-3-4  19 }	

m8-3-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-3-4  20 }	

m8-3-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-3-4  21 }	

	
--
--	nb7-m8-3
--    

	
	

m8-3-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-5  1 }

m8-3-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-5  2 }

m8-3-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-5  3 }

m8-3-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-5  4 }
	
m8-3-5PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-5  5 }	
	
	
m8-3-5ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-5  6 }		
	
m8-3-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-5  7 }		
	
	
m8-3-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-5  8 }	
	

m8-3-5CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-5  9 }
	
	
m8-3-5OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-5  10 }	
	
	
m8-3-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-5  11 }	
	
	
m8-3-5UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-5  12 }	
	
m8-3-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-5  13 }		
	
m8-3-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-5  14 }		
	
m8-3-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-5  15 }	
	
m8-3-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-5  16 }	
	

m8-3-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-5  17 }	

m8-3-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-5  18 }	

m8-3-5ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-3-5  19 }

m8-3-5CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-3-5  20 }	

m8-3-5CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-3-5  21 }			
	
--
--	nb7-m8-3
--    
	

m8-3-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-6  1 }

m8-3-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-6  2 }

m8-3-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-6  3 }

m8-3-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-6  4 }
	
m8-3-6PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-6  5 }	
	
	
m8-3-6ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-6  6 }		
	
m8-3-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-6  7 }		
	
	
m8-3-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-6  8 }	


m8-3-6CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-6  9 }

	
m8-3-6OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-6  10 }	
	
m8-3-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-6  11 }	
	
	
m8-3-6UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-6  12 }	
	
m8-3-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-6  13 }		
	
m8-3-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-6  14 }		
	
m8-3-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-6  15 }	
	
m8-3-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-6  16 }	
	

m8-3-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-6  17 }	

	
m8-3-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-6  18 }	

m8-3-6ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-3-6  19 }	


m8-3-6CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-3-6  20 }	

m8-3-6CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-3-6  21 }		
	
--
--	nb7-m8-3
--    

m8-3-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-7  1 }

m8-3-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-7  2 }

m8-3-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-7  3 }

m8-3-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-7  4 }
	
m8-3-7PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-7  5 }	
	
	
m8-3-7ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-7  6 }		
	
m8-3-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-7  7 }		
	
	
m8-3-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-7  8 }	


m8-3-7CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-7  9 }

m8-3-7OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-7  10 }	

m8-3-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-7  11 }	
	
	
m8-3-7UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-7  12 }	
	
m8-3-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-7  13 }		
	
m8-3-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-7  14 }		
	
m8-3-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-7  15 }	
	
m8-3-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-7  16 }	
	

m8-3-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-7  17 }		

m8-3-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-7  18 }	

m8-3-7ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-3-7  19 }	

m8-3-7CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-3-7  20 }	

m8-3-7CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-3-7  21 }		
	
--
--	nb7-m8-3
--    	

m8-3-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-8  1 }

m8-3-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-8  2 }

m8-3-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-8  3 }

m8-3-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-8  4 }
	
m8-3-8PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-8  5 }	
	
	
m8-3-8ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-8  6 }		
	
m8-3-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-8  7 }		
	
	
m8-3-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-8  8 }		
	
	
m8-3-8CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-8  9 }


m8-3-8OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-8  10 }	

m8-3-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-8  11 }	
	
	
m8-3-8UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-8  12 }	
	
m8-3-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-8  13 }		
	
m8-3-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-8  14 }		
	
m8-3-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-8  15 }	
	
m8-3-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-8  16 }	
	

m8-3-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-8  17 }		

m8-3-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3-8  18 }	

m8-3-8ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-3-8  19 }	

m8-3-8CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-3-8  20 }	

m8-3-8CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-3-8  21 }		
	
m8-3Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3  9 }	
    
m8-3VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3  10 }

m8-3VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3  11 }

m8-3CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3  12 }

m8-3CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3  13 }
    
m8-3Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-3  14 }


--
--	nb7-m8-4
--    		

m8-4-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { nb7-m8-4-1  1 }

m8-4-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { nb7-m8-4-1  2 }

m8-4-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { nb7-m8-4-1  3 }

m8-4-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { nb7-m8-4-1  4 }
	
m8-4-1PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- power supply."
    DEFVAL { "" }
    ::= { nb7-m8-4-1  5 }	
	
	
m8-4-1ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- Output response to control input, Active, Inactive or Disable."
    DEFVAL { "" }
    ::= { nb7-m8-4-1  6 }		
	
m8-4-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { nb7-m8-4-1  7 }		
	
	
m8-4-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { nb7-m8-4-1  8 }

m8-4-1CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- control Input Type, Normally Open, Normally Closed,
    Open Collector, Voltage, Disabled."
    DEFVAL { "" }
    ::= { nb7-m8-4-1  9 }	
	
	
m8-4-1OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- output load type, Maglock, Fail-safe Strike, 
    Fail-secure Strike, Constant ON."
    DEFVAL { "" }
    ::= { nb7-m8-4-1  10 }	
	
m8-4-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- unlock on FAI Activation, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-4-1  11 }	
	
	
m8-4-1UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- unlock on AC loss, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-4-1  12 }	
	
m8-4-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-4-1  13 }		
	
m8-4-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { nb7-m8-4-1  14 }		
	
m8-4-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { nb7-m8-4-1  15 }	
	
m8-4-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { nb7-m8-4-1  16 }	
	

m8-4-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { nb7-m8-4-1  17 }	

m8-4-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable M8 -."
    DEFVAL { "" }
    ::= { nb7-m8-4-1  18 }	

m8-4-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-4-1  19 }	

m8-4-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-4-1  20 }	

m8-4-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-4-1  21 }		
    
--
--	nb7-m8-4
--    



m8-4-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-2  1 }

m8-4-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-2  2 }

m8-4-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-2  3 }

m8-4-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-2  4 }
	
m8-4-2PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-2  5 }	
	
	
m8-4-2ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-2  6 }		
	
m8-4-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-2  7 }		
	
	
m8-4-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-2  8 }		

m8-4-2CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-2  9 }	
	
m8-4-2OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-2  10 }	

m8-4-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-2  11 }	
	
	
m8-4-2UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-2  12 }	
	
m8-4-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-2  13 }		
	
m8-4-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-2  14 }		
	
m8-4-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-2  15 }	
	
m8-4-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-2  16 }	
	

m8-4-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-2  17 }		

	
m8-4-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-2  18 }	

m8-4-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-4-2  19 }	

m8-4-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-4-2  20 }	

m8-4-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-4-2  21 }	
	
--
--	nb7-m8-4
--    
	

m8-4-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-3  1 }

m8-4-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-3  2 }

m8-4-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-3  3 }

m8-4-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-3  4 }
	
m8-4-3PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-3  5 }	
	
	
m8-4-3ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-3  6 }		
	
m8-4-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-3  7 }		
	
	
m8-4-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-3  8 }
	

m8-4-3CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-3  9 }


m8-4-3OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-3  10 }	
	

m8-4-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-3  11 }	
	
	
m8-4-3UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-3  12 }	
	
m8-4-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-3  13 }		
	
m8-4-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-3  14 }		
	
m8-4-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-3  15 }	
	
m8-4-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-3  16 }	
	

m8-4-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-3  17 }	


m8-4-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-3  18 }	

m8-4-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-4-3  19 }	

m8-4-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-4-3  20 }	

m8-4-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-4-3  21 }	
	
--
--	nb7-m8-4
--    
	
	

m8-4-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-4  1 }

m8-4-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-4  2 }

m8-4-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-4  3 }

m8-4-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-4  4 }
	
m8-4-4PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-4  5 }	
	
	
m8-4-4ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-4  6 }		
	
m8-4-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-4  7 }		
	
	
m8-4-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-4  8 }		
	

m8-4-4CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-4  9 }	
	

m8-4-4OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-4  10 }	


m8-4-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-4  11 }	
	
	
m8-4-4UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-4  12 }	
	
m8-4-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-4  13 }		
	
m8-4-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-4  14 }		
	
m8-4-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-4  15 }	
	
m8-4-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-4  16 }	
	

m8-4-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-4  17 }	

	
m8-4-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-4  18 }	

m8-4-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-4-4  19 }	

m8-4-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-4-4  20 }	

m8-4-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-4-4  21 }	

	
--
--	nb7-m8-4
--    

	
	

m8-4-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-5  1 }

m8-4-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-5  2 }

m8-4-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-5  3 }

m8-4-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-5  4 }
	
m8-4-5PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-5  5 }	
	
	
m8-4-5ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-5  6 }		
	
m8-4-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-5  7 }		
	
	
m8-4-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-5  8 }	
	

m8-4-5CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-5  9 }
	
	
m8-4-5OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-5  10 }	
	
	
m8-4-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-5  11 }	
	
	
m8-4-5UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-5  12 }	
	
m8-4-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-5  13 }		
	
m8-4-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-5  14 }		
	
m8-4-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-5  15 }	
	
m8-4-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-5  16 }	
	

m8-4-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-5  17 }	

m8-4-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-5  18 }	

m8-4-5ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-4-5  19 }	

m8-4-5CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-4-5  20 }	

m8-4-5CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-4-5  21 }		
	
--
--	nb7-m8-4
--    
	

m8-4-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-6  1 }

m8-4-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-6  2 }

m8-4-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-6  3 }

m8-4-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-6  4 }
	
m8-4-6PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-6  5 }	
	
	
m8-4-6ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-6  6 }		
	
m8-4-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-6  7 }		
	
	
m8-4-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-6  8 }	


m8-4-6CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-6  9 }

	
m8-4-6OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-6  10 }	
	
m8-4-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-6  11 }	
	
	
m8-4-6UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-6  12 }	
	
m8-4-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-6  13 }		
	
m8-4-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-6  14 }		
	
m8-4-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-6  15 }	
	
m8-4-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-6  16 }	
	

m8-4-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-6  17 }	

	
m8-4-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-6  18 }	

m8-4-6ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-4-6  19 }	

m8-4-6CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-4-6  20 }	

m8-4-6CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-4-6  21 }		
	
--
--	nb7-m8-4
--    

m8-4-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-7  1 }

m8-4-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-7  2 }

m8-4-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-7  3 }

m8-4-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-7  4 }
	
m8-4-7PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-7  5 }	
	
	
m8-4-7ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-7  6 }		
	
m8-4-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-7  7 }		
	
	
m8-4-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-7  8 }	


m8-4-7CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-7  9 }

m8-4-7OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-7  10 }	

m8-4-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-7  11 }	
	
	
m8-4-7UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-7  12 }	
	
m8-4-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-7  13 }		
	
m8-4-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-7  14 }		
	
m8-4-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-7  15 }	
	
m8-4-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-7  16 }	
	

m8-4-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-7  17 }		

m8-4-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-7  18 }	

m8-4-7ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-4-7  19 }	

m8-4-7CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-4-7  20 }	

m8-4-7CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-4-7  21 }		
	
--
--	nb7-m8-4
--    	

m8-4-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-8  1 }

m8-4-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-8  2 }

m8-4-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-8  3 }

m8-4-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-8  4 }
	
m8-4-8PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-8  5 }	
	
	
m8-4-8ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-8  6 }		
	
m8-4-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-8  7 }		
	
	
m8-4-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-8  8 }		
	
	
m8-4-8CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-8  9 }


m8-4-8OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-8  10 }	

m8-4-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-8  11 }	
	
	
m8-4-8UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-8  12 }	
	
m8-4-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-8  13 }		
	
m8-4-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-8  14 }		
	
m8-4-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-8  15 }	
	
m8-4-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-8  16 }	
	

m8-4-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-8  17 }		

m8-4-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4-8  18 }	

m8-4-8ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-4-8  19 }	

m8-4-8CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-4-8  20 }	

m8-4-8CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-4-8  21 }		
	
m8-4Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4  9 }	
    
m8-4VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4  10 }

m8-4VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4  11 }

m8-4CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4  12 }

m8-4CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4  13 }
    
m8-4Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-4  14 }


--
--	nb7-m8-5
--    		

m8-5-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { nb7-m8-5-1  1 }

m8-5-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { nb7-m8-5-1  2 }

m8-5-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { nb7-m8-5-1  3 }

m8-5-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { nb7-m8-5-1  4 }
	
m8-5-1PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- power supply."
    DEFVAL { "" }
    ::= { nb7-m8-5-1  5 }	
	
	
m8-5-1ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- Output response to control input, Active, Inactive or Disable."
    DEFVAL { "" }
    ::= { nb7-m8-5-1  6 }		
	
m8-5-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { nb7-m8-5-1  7 }		
	
	
m8-5-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { nb7-m8-5-1  8 }

m8-5-1CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- control Input Type, Normally Open, Normally Closed,
    Open Collector, Voltage, Disabled."
    DEFVAL { "" }
    ::= { nb7-m8-5-1  9 }	
	
	
m8-5-1OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- output load type, Maglock, Fail-safe Strike, 
    Fail-secure Strike, Constant ON."
    DEFVAL { "" }
    ::= { nb7-m8-5-1  10 }	
	
m8-5-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- unlock on FAI Activation, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-5-1  11 }	
	
	
m8-5-1UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- unlock on AC loss, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-5-1  12 }	
	
m8-5-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-5-1  13 }		
	
m8-5-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { nb7-m8-5-1  14 }		
	
m8-5-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { nb7-m8-5-1  15 }	
	
m8-5-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { nb7-m8-5-1  16 }	
	

m8-5-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { nb7-m8-5-1  17 }	

m8-5-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable M8 -."
    DEFVAL { "" }
    ::= { nb7-m8-5-1  18 }	

m8-5-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-5-1  19 }	

m8-5-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-5-1  20 }	

m8-5-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-5-1  21 }		
    
--
--	nb7-m8-5
--    



m8-5-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-2  1 }

m8-5-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-2  2 }

m8-5-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-2  3 }

m8-5-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-2  4 }
	
m8-5-2PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-2  5 }	
	
	
m8-5-2ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-2  6 }		
	
m8-5-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-2  7 }		
	
	
m8-5-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-2  8 }		

m8-5-2CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-2  9 }	
	
m8-5-2OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-2  10 }	

m8-5-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-2  11 }	
	
	
m8-5-2UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-2  12 }	
	
m8-5-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-2  13 }		
	
m8-5-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-2  14 }		
	
m8-5-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-2  15 }	
	
m8-5-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-2  16 }	
	

m8-5-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-2  17 }		

	
m8-5-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-2  18 }	

m8-5-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-5-2  19 }	

m8-5-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-5-2  20 }	

m8-5-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-5-2  21 }	
	
--
--	nb7-m8-5
--    
	

m8-5-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-3  1 }

m8-5-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-3  2 }

m8-5-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-3  3 }

m8-5-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-3  4 }
	
m8-5-3PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-3  5 }	
	
	
m8-5-3ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-3  6 }		
	
m8-5-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-3  7 }		
	
	
m8-5-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-3  8 }
	

m8-5-3CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-3  9 }


m8-5-3OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-3  10 }	
	

m8-5-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-3  11 }	
	
	
m8-5-3UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-3  12 }	
	
m8-5-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-3  13 }		
	
m8-5-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-3  14 }		
	
m8-5-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-3  15 }	
	
m8-5-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-3  16 }	
	

m8-5-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-3  17 }	


m8-5-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-3  18 }	

m8-5-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-5-3  19 }	

m8-5-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-5-3  20 }	

m8-5-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-5-3  21 }	
	
--
--	nb7-m8-5
--    
	
	

m8-5-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-4  1 }

m8-5-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-4  2 }

m8-5-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-4  3 }

m8-5-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-4  4 }
	
m8-5-4PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-4  5 }	
	
	
m8-5-4ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-4  6 }		
	
m8-5-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-4  7 }		
	
	
m8-5-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-4  8 }		
	

m8-5-4CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-4  9 }	
	

m8-5-4OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-4  10 }	


m8-5-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-4  11 }	
	
	
m8-5-4UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-4  12 }	
	
m8-5-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-4  13 }		
	
m8-5-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-4  14 }		
	
m8-5-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-4  15 }	
	
m8-5-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-4  16 }	
	

m8-5-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-4  17 }	

	
m8-5-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-4  18 }	

m8-5-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-5-4  19 }

m8-5-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-5-4  20 }	

m8-5-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-5-4  21 }		

	
--
--	nb7-m8-5
--    

	
	

m8-5-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-5  1 }

m8-5-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-5  2 }

m8-5-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-5  3 }

m8-5-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-5  4 }
	
m8-5-5PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-5  5 }	
	
	
m8-5-5ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-5  6 }		
	
m8-5-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-5  7 }		
	
	
m8-5-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-5  8 }	
	

m8-5-5CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-5  9 }
	
	
m8-5-5OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-5  10 }	
	
	
m8-5-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-5  11 }	
	
	
m8-5-5UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-5  12 }	
	
m8-5-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-5  13 }		
	
m8-5-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-5  14 }		
	
m8-5-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-5  15 }	
	
m8-5-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-5  16 }	
	

m8-5-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-5  17 }	

m8-5-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-5  18 }	

m8-5-5ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-5-5  19 }	

m8-5-5CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-5-5  20 }	

m8-5-5CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-5-5  21 }		
	
--
--	nb7-m8-5
--    
	

m8-5-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-6  1 }

m8-5-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-6  2 }

m8-5-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-6  3 }

m8-5-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-6  4 }
	
m8-5-6PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-6  5 }	
	
	
m8-5-6ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-6  6 }		
	
m8-5-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-6  7 }		
	
	
m8-5-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-6  8 }	


m8-5-6CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-6  9 }

	
m8-5-6OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-6  10 }	
	
m8-5-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-6  11 }	
	
	
m8-5-6UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-6  12 }	
	
m8-5-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-6  13 }		
	
m8-5-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-6  14 }		
	
m8-5-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-6  15 }	
	
m8-5-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-6  16 }	
	

m8-5-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-6  17 }	

	
m8-5-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-6  18 }	

m8-5-6ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-5-6  19 }	

m8-5-6CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-5-6  20 }	

m8-5-6CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-5-6  21 }		
	
--
--	nb7-m8-5
--    

m8-5-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-7  1 }

m8-5-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-7  2 }

m8-5-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-7  3 }

m8-5-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-7  4 }
	
m8-5-7PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-7  5 }	
	
	
m8-5-7ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-7  6 }		
	
m8-5-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-7  7 }		
	
	
m8-5-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-7  8 }	


m8-5-7CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-7  9 }

m8-5-7OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-7  10 }	

m8-5-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-7  11 }	
	
	
m8-5-7UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-7  12 }	
	
m8-5-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-7  13 }		
	
m8-5-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-7  14 }		
	
m8-5-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-7  15 }	
	
m8-5-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-7  16 }	
	

m8-5-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-7  17 }		

m8-5-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-7  18 }	

m8-5-7ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-5-7  19 }	

m8-5-7CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-5-7  20 }	

m8-5-7CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-5-7  21 }		
	
--
--	nb7-m8-5
--    	

m8-5-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-8  1 }

m8-5-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-8  2 }

m8-5-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-8  3 }

m8-5-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-8  4 }
	
m8-5-8PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-8  5 }	
	
	
m8-5-8ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-8  6 }		
	
m8-5-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-8  7 }		
	
	
m8-5-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-8  8 }		
	
	
m8-5-8CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-8  9 }


m8-5-8OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-8  10 }	

m8-5-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-8  11 }	
	
	
m8-5-8UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-8  12 }	
	
m8-5-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-8  13 }		
	
m8-5-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-8  14 }		
	
m8-5-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-8  15 }	
	
m8-5-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-8  16 }	
	

m8-5-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-8  17 }		

m8-5-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5-8  18 }	

m8-5-8ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-5-8  19 }	

m8-5-8CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-5-8  20 }	

m8-5-8CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-5-8  21 }		
	
m8-5Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5  9 }	
    
m8-5VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5  10 }

m8-5VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5  11 }

m8-5CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5  12 }

m8-5CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5  13 }
    
m8-5Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-5  14 }


--
--	nb7-m8-6
--    		

m8-6-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { nb7-m8-6-1  1 }

m8-6-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { nb7-m8-6-1  2 }

m8-6-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { nb7-m8-6-1  3 }

m8-6-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { nb7-m8-6-1  4 }
	
m8-6-1PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- power supply."
    DEFVAL { "" }
    ::= { nb7-m8-6-1  5 }	
	
	
m8-6-1ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- Output response to control input, Active, Inactive or Disable."
    DEFVAL { "" }
    ::= { nb7-m8-6-1  6 }		
	
m8-6-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { nb7-m8-6-1  7 }		
	
	
m8-6-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { nb7-m8-6-1  8 }

m8-6-1CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- control Input Type, Normally Open, Normally Closed,
    Open Collector, Voltage, Disabled."
    DEFVAL { "" }
    ::= { nb7-m8-6-1  9 }	
	
	
m8-6-1OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- output load type, Maglock, Fail-safe Strike, 
    Fail-secure Strike, Constant ON."
    DEFVAL { "" }
    ::= { nb7-m8-6-1  10 }	
	
m8-6-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- unlock on FAI Activation, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-6-1  11 }	
	
	
m8-6-1UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- unlock on AC loss, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-6-1  12 }	
	
m8-6-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-6-1  13 }		
	
m8-6-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { nb7-m8-6-1  14 }		
	
m8-6-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { nb7-m8-6-1  15 }	
	
m8-6-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { nb7-m8-6-1  16 }	
	

m8-6-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { nb7-m8-6-1  17 }	

m8-6-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable M8 -."
    DEFVAL { "" }
    ::= { nb7-m8-6-1  18 }	

m8-6-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-6-1  19 }

m8-6-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-6-1  20 }	

m8-6-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-6-1  21 }			
    
--
--	nb7-m8-6
--    



m8-6-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-2  1 }

m8-6-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-2  2 }

m8-6-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-2  3 }

m8-6-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-2  4 }
	
m8-6-2PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-2  5 }	
	
	
m8-6-2ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-2  6 }		
	
m8-6-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-2  7 }		
	
	
m8-6-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-2  8 }		

m8-6-2CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-2  9 }	
	
m8-6-2OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-2  10 }	

m8-6-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-2  11 }	
	
	
m8-6-2UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-2  12 }	
	
m8-6-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-2  13 }		
	
m8-6-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-2  14 }		
	
m8-6-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-2  15 }	
	
m8-6-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-2  16 }	
	

m8-6-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-2  17 }		

	
m8-6-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-2  18 }	

m8-6-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-6-2  19 }

m8-6-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-6-2  20 }	

m8-6-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-6-2  21 }	
	
--
--	nb7-m8-6
--    
	

m8-6-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-3  1 }

m8-6-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-3  2 }

m8-6-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-3  3 }

m8-6-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-3  4 }
	
m8-6-3PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-3  5 }	
	
	
m8-6-3ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-3  6 }		
	
m8-6-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-3  7 }		
	
	
m8-6-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-3  8 }
	

m8-6-3CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-3  9 }


m8-6-3OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-3  10 }	
	

m8-6-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-3  11 }	
	
	
m8-6-3UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-3  12 }	
	
m8-6-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-3  13 }		
	
m8-6-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-3  14 }		
	
m8-6-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-3  15 }	
	
m8-6-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-3  16 }	
	

m8-6-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-3  17 }	


m8-6-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-3  18 }	

m8-6-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-6-3  19 }	

m8-6-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-6-3  20 }	

m8-6-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-6-3  21 }
	
--
--	nb7-m8-6
--    
	
	

m8-6-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-4  1 }

m8-6-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-4  2 }

m8-6-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-4  3 }

m8-6-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-4  4 }
	
m8-6-4PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-4  5 }	
	
	
m8-6-4ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-4  6 }		
	
m8-6-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-4  7 }		
	
	
m8-6-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-4  8 }		
	

m8-6-4CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-4  9 }	
	

m8-6-4OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-4  10 }	


m8-6-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-4  11 }	
	
	
m8-6-4UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-4  12 }	
	
m8-6-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-4  13 }		
	
m8-6-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-4  14 }		
	
m8-6-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-4  15 }	
	
m8-6-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-4  16 }	
	

m8-6-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-4  17 }	

	
m8-6-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-4  18 }	

m8-6-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-6-4  19 }	

m8-6-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-6-4  20 }	

m8-6-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-6-4  21 }

	
--
--	nb7-m8-6
--    

	
	

m8-6-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-5  1 }

m8-6-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-5  2 }

m8-6-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-5  3 }

m8-6-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-5  4 }
	
m8-6-5PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-5  5 }	
	
	
m8-6-5ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-5  6 }		
	
m8-6-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-5  7 }		
	
	
m8-6-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-5  8 }	
	

m8-6-5CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-5  9 }
	
	
m8-6-5OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-5  10 }	
	
	
m8-6-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-5  11 }	
	
	
m8-6-5UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-5  12 }	
	
m8-6-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-5  13 }		
	
m8-6-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-5  14 }		
	
m8-6-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-5  15 }	
	
m8-6-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-5  16 }	
	

m8-6-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-5  17 }	

m8-6-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-5  18 }	

m8-6-5ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-6-5  19 }

m8-6-5CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-6-5  20 }	

m8-6-5CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-6-5  21 }		
	
--
--	nb7-m8-6
--    
	

m8-6-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-6  1 }

m8-6-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-6  2 }

m8-6-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-6  3 }

m8-6-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-6  4 }
	
m8-6-6PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-6  5 }	
	
	
m8-6-6ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-6  6 }		
	
m8-6-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-6  7 }		
	
	
m8-6-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-6  8 }	


m8-6-6CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-6  9 }

	
m8-6-6OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-6  10 }	
	
m8-6-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-6  11 }	
	
	
m8-6-6UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-6  12 }	
	
m8-6-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-6  13 }		
	
m8-6-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-6  14 }		
	
m8-6-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-6  15 }	
	
m8-6-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-6  16 }	
	

m8-6-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-6  17 }	

	
m8-6-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-6  18 }	

m8-6-6ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-6-6  19 }

m8-6-6CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-6-6  20 }	

m8-6-6CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-6-6  21 }		
	
--
--	nb7-m8-6
--    

m8-6-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-7  1 }

m8-6-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-7  2 }

m8-6-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-7  3 }

m8-6-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-7  4 }
	
m8-6-7PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-7  5 }	
	
	
m8-6-7ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-7  6 }		
	
m8-6-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-7  7 }		
	
	
m8-6-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-7  8 }	


m8-6-7CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-7  9 }

m8-6-7OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-7  10 }	

m8-6-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-7  11 }	
	
	
m8-6-7UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-7  12 }	
	
m8-6-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-7  13 }		
	
m8-6-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-7  14 }		
	
m8-6-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-7  15 }	
	
m8-6-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-7  16 }	
	

m8-6-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-7  17 }		

m8-6-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-7  18 }	

m8-6-7ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-6-7  19 }	

m8-6-7CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-6-7  20 }	

m8-6-7CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-6-7  21 }	
	
--
--	nb7-m8-6
--    	

m8-6-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-8  1 }

m8-6-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-8  2 }

m8-6-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-8  3 }

m8-6-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-8  4 }
	
m8-6-8PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-8  5 }	
	
	
m8-6-8ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-8  6 }		
	
m8-6-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-8  7 }		
	
	
m8-6-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-8  8 }		
	
	
m8-6-8CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-8  9 }


m8-6-8OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-8  10 }	

m8-6-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-8  11 }	
	
	
m8-6-8UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-8  12 }	
	
m8-6-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-8  13 }		
	
m8-6-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-8  14 }		
	
m8-6-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-8  15 }	
	
m8-6-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-8  16 }	
	

m8-6-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-8  17 }		

m8-6-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6-8  18 }	

m8-6-8ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-6-8  19 }	

m8-6-8CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-6-8  20 }	

m8-6-8CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-6-8  21 }	
	
m8-6Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6  9 }	
    
m8-6VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6  10 }

m8-6VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6  11 }

m8-6CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6  12 }

m8-6CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6  13 }
    
m8-6Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-6  14 }


--
--	nb7-m8-7
--    		

m8-7-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { nb7-m8-7-1  1 }

m8-7-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { nb7-m8-7-1  2 }

m8-7-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { nb7-m8-7-1  3 }

m8-7-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { nb7-m8-7-1  4 }
	
m8-7-1PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- power supply."
    DEFVAL { "" }
    ::= { nb7-m8-7-1  5 }	
	
	
m8-7-1ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- Output response to control input, Active, Inactive or Disable."
    DEFVAL { "" }
    ::= { nb7-m8-7-1  6 }		
	
m8-7-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { nb7-m8-7-1  7 }		
	
	
m8-7-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { nb7-m8-7-1  8 }

m8-7-1CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- control Input Type, Normally Open, Normally Closed,
    Open Collector, Voltage, Disabled."
    DEFVAL { "" }
    ::= { nb7-m8-7-1  9 }	
	
	
m8-7-1OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- output load type, Maglock, Fail-safe Strike, 
    Fail-secure Strike, Constant ON."
    DEFVAL { "" }
    ::= { nb7-m8-7-1  10 }	
	
m8-7-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- unlock on FAI Activation, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-7-1  11 }	
	
	
m8-7-1UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- unlock on AC loss, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-7-1  12 }	
	
m8-7-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-7-1  13 }		
	
m8-7-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { nb7-m8-7-1  14 }		
	
m8-7-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { nb7-m8-7-1  15 }	
	
m8-7-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { nb7-m8-7-1  16 }	
	

m8-7-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { nb7-m8-7-1  17 }	

m8-7-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable M8 -."
    DEFVAL { "" }
    ::= { nb7-m8-7-1  18 }	

m8-7-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-7-1  19 }	

m8-7-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-7-1  20 }	

m8-7-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-7-1  21 }	
    
--
--	nb7-m8-7
--    



m8-7-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-2  1 }

m8-7-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-2  2 }

m8-7-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-2  3 }

m8-7-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-2  4 }
	
m8-7-2PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-2  5 }	
	
	
m8-7-2ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-2  6 }		
	
m8-7-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-2  7 }		
	
	
m8-7-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-2  8 }		

m8-7-2CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-2  9 }	
	
m8-7-2OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-2  10 }	

m8-7-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-2  11 }	
	
	
m8-7-2UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-2  12 }	
	
m8-7-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-2  13 }		
	
m8-7-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-2  14 }		
	
m8-7-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-2  15 }	
	
m8-7-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-2  16 }	
	

m8-7-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-2  17 }		

	
m8-7-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-2  18 }	

m8-7-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-7-2  19 }	

m8-7-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-7-2  20 }	

m8-7-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-7-2  21 }
	
--
--	nb7-m8-7
--    
	

m8-7-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-3  1 }

m8-7-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-3  2 }

m8-7-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-3  3 }

m8-7-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-3  4 }
	
m8-7-3PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-3  5 }	
	
	
m8-7-3ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-3  6 }		
	
m8-7-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-3  7 }		
	
	
m8-7-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-3  8 }
	

m8-7-3CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-3  9 }


m8-7-3OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-3  10 }	
	

m8-7-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-3  11 }	
	
	
m8-7-3UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-3  12 }	
	
m8-7-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-3  13 }		
	
m8-7-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-3  14 }		
	
m8-7-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-3  15 }	
	
m8-7-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-3  16 }	
	

m8-7-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-3  17 }	


m8-7-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-3  18 }	

m8-7-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-7-3  19 }	

m8-7-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-7-3  20 }	

m8-7-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-7-3  21 }
	
--
--	nb7-m8-7
--    
	
	

m8-7-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-4  1 }

m8-7-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-4  2 }

m8-7-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-4  3 }

m8-7-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-4  4 }
	
m8-7-4PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-4  5 }	
	
	
m8-7-4ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-4  6 }		
	
m8-7-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-4  7 }		
	
	
m8-7-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-4  8 }		
	

m8-7-4CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-4  9 }	
	

m8-7-4OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-4  10 }	


m8-7-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-4  11 }	
	
	
m8-7-4UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-4  12 }	
	
m8-7-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-4  13 }		
	
m8-7-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-4  14 }		
	
m8-7-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-4  15 }	
	
m8-7-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-4  16 }	
	

m8-7-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-4  17 }	

	
m8-7-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-4  18 }	

m8-7-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-7-4  19 }	

m8-7-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-7-4  20 }	

m8-7-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-7-4  21 }

	
--
--	nb7-m8-7
--    

	
	

m8-7-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-5  1 }

m8-7-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-5  2 }

m8-7-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-5  3 }

m8-7-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-5  4 }
	
m8-7-5PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-5  5 }	
	
	
m8-7-5ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-5  6 }		
	
m8-7-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-5  7 }		
	
	
m8-7-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-5  8 }	
	

m8-7-5CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-5  9 }
	
	
m8-7-5OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-5  10 }	
	
	
m8-7-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-5  11 }	
	
	
m8-7-5UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-5  12 }	
	
m8-7-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-5  13 }		
	
m8-7-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-5  14 }		
	
m8-7-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-5  15 }	
	
m8-7-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-5  16 }	
	

m8-7-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-5  17 }	

m8-7-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-5  18 }	

m8-7-5ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-7-5  19 }	

m8-7-5CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-7-5  20 }	

m8-7-5CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-7-5  21 }	
	
--
--	nb7-m8-7
--    
	

m8-7-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-6  1 }

m8-7-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-6  2 }

m8-7-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-6  3 }

m8-7-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-6  4 }
	
m8-7-6PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-6  5 }	
	
	
m8-7-6ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-6  6 }		
	
m8-7-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-6  7 }		
	
	
m8-7-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-6  8 }	


m8-7-6CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-6  9 }

	
m8-7-6OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-6  10 }	
	
m8-7-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-6  11 }	
	
	
m8-7-6UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-6  12 }	
	
m8-7-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-6  13 }		
	
m8-7-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-6  14 }		
	
m8-7-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-6  15 }	
	
m8-7-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-6  16 }	
	

m8-7-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-6  17 }	

	
m8-7-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-6  18 }	

m8-7-6ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-7-6  19 }	

m8-7-6CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-7-6  20 }	

m8-7-6CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-7-6  21 }	
	
--
--	nb7-m8-7
--    

m8-7-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-7  1 }

m8-7-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-7  2 }

m8-7-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-7  3 }

m8-7-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-7  4 }
	
m8-7-7PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-7  5 }	
	
	
m8-7-7ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-7  6 }		
	
m8-7-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-7  7 }		
	
	
m8-7-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-7  8 }	


m8-7-7CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-7  9 }

m8-7-7OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-7  10 }	

m8-7-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-7  11 }	
	
	
m8-7-7UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-7  12 }	
	
m8-7-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-7  13 }		
	
m8-7-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-7  14 }		
	
m8-7-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-7  15 }	
	
m8-7-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-7  16 }	
	

m8-7-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-7  17 }		

m8-7-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-7  18 }	

m8-7-7ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-7-7  19 }	

m8-7-7CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-7-7  20 }	

m8-7-7CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-7-7  21 }	
	
--
--	nb7-m8-7
--    	

m8-7-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-8  1 }

m8-7-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-8  2 }

m8-7-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-8  3 }

m8-7-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-8  4 }
	
m8-7-8PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-8  5 }	
	
	
m8-7-8ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-8  6 }		
	
m8-7-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-8  7 }		
	
	
m8-7-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-8  8 }		
	
	
m8-7-8CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-8  9 }


m8-7-8OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-8  10 }	

m8-7-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-8  11 }	
	
	
m8-7-8UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-8  12 }	
	
m8-7-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-8  13 }		
	
m8-7-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-8  14 }		
	
m8-7-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-8  15 }	
	
m8-7-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-8  16 }	
	

m8-7-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-8  17 }		

m8-7-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7-8  18 }	

m8-7-8ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-7-8  19 }	

m8-7-8CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-7-8  20 }	

m8-7-8CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-7-8  21 }	
	
m8-7Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7  9 }	
    
m8-7VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7  10 }

m8-7VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7  11 }

m8-7CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7  12 }

m8-7CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7  13 }
    
m8-7Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-7  14 }


--
--	nb7-m8-8
--    		

m8-8-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { nb7-m8-8-1  1 }

m8-8-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { nb7-m8-8-1  2 }

m8-8-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { nb7-m8-8-1  3 }

m8-8-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { nb7-m8-8-1  4 }
	
m8-8-1PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- power supply."
    DEFVAL { "" }
    ::= { nb7-m8-8-1  5 }	
	
	
m8-8-1ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- Output response to control input, Active, Inactive or Disable."
    DEFVAL { "" }
    ::= { nb7-m8-8-1  6 }		
	
m8-8-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { nb7-m8-8-1  7 }		
	
	
m8-8-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { nb7-m8-8-1  8 }

m8-8-1CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- control Input Type, Normally Open, Normally Closed,
    Open Collector, Voltage, Disabled."
    DEFVAL { "" }
    ::= { nb7-m8-8-1  9 }	
	
	
m8-8-1OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- output load type, Maglock, Fail-safe Strike, 
    Fail-secure Strike, Constant ON."
    DEFVAL { "" }
    ::= { nb7-m8-8-1  10 }	
	
m8-8-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- unlock on FAI Activation, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-8-1  11 }	
	
	
m8-8-1UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- unlock on AC loss, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-8-1  12 }	
	
m8-8-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { nb7-m8-8-1  13 }		
	
m8-8-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { nb7-m8-8-1  14 }		
	
m8-8-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { nb7-m8-8-1  15 }	
	
m8-8-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { nb7-m8-8-1  16 }	
	

m8-8-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { nb7-m8-8-1  17 }	

m8-8-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable M8 -."
    DEFVAL { "" }
    ::= { nb7-m8-8-1  18 }	

m8-8-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-8-1  19 }	

m8-8-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-8-1  20 }	

m8-8-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-8-1  21 }	
    
--
--	nb7-m8-8
--    



m8-8-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-2  1 }

m8-8-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-2  2 }

m8-8-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-2  3 }

m8-8-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-2  4 }
	
m8-8-2PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-2  5 }	
	
	
m8-8-2ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-2  6 }		
	
m8-8-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-2  7 }		
	
	
m8-8-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-2  8 }		

m8-8-2CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-2  9 }	
	
m8-8-2OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-2  10 }	

m8-8-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-2  11 }	
	
	
m8-8-2UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-2  12 }	
	
m8-8-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-2  13 }		
	
m8-8-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-2  14 }		
	
m8-8-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-2  15 }	
	
m8-8-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-2  16 }	
	

m8-8-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-2  17 }		

	
m8-8-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-2  18 }	

m8-8-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-8-2  19 }	

m8-8-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-8-2  20 }	

m8-8-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-8-2  21 }	
	
--
--	nb7-m8-8
--    
	

m8-8-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-3  1 }

m8-8-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-3  2 }

m8-8-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-3  3 }

m8-8-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-3  4 }
	
m8-8-3PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-3  5 }	
	
	
m8-8-3ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-3  6 }		
	
m8-8-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-3  7 }		
	
	
m8-8-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-3  8 }
	

m8-8-3CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-3  9 }


m8-8-3OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-3  10 }	
	

m8-8-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-3  11 }	
	
	
m8-8-3UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-3  12 }	
	
m8-8-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-3  13 }		
	
m8-8-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-3  14 }		
	
m8-8-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-3  15 }	
	
m8-8-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-3  16 }	
	

m8-8-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-3  17 }	


m8-8-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-3  18 }	

m8-8-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-8-3  19 }	

m8-8-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-8-3  20 }	

m8-8-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-8-3  21 }	
	
--
--	nb7-m8-8
--    
	
	

m8-8-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-4  1 }

m8-8-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-4  2 }

m8-8-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-4  3 }

m8-8-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-4  4 }
	
m8-8-4PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-4  5 }	
	
	
m8-8-4ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-4  6 }		
	
m8-8-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-4  7 }		
	
	
m8-8-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-4  8 }		
	

m8-8-4CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-4  9 }	
	

m8-8-4OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-4  10 }	


m8-8-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-4  11 }	
	
	
m8-8-4UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-4  12 }	
	
m8-8-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-4  13 }		
	
m8-8-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-4  14 }		
	
m8-8-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-4  15 }	
	
m8-8-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-4  16 }	
	

m8-8-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-4  17 }	

	
m8-8-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-4  18 }	

m8-8-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-8-4  19 }	

m8-8-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-8-4  20 }	

m8-8-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-8-4  21 }	

	
--
--	nb7-m8-8
--    

	
	

m8-8-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-5  1 }

m8-8-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-5  2 }

m8-8-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-5  3 }

m8-8-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-5  4 }
	
m8-8-5PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-5  5 }	
	
	
m8-8-5ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-5  6 }		
	
m8-8-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-5  7 }		
	
	
m8-8-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-5  8 }	
	

m8-8-5CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-5  9 }
	
	
m8-8-5OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-5  10 }	
	
	
m8-8-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-5  11 }	
	
	
m8-8-5UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-5  12 }	
	
m8-8-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-5  13 }		
	
m8-8-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-5  14 }		
	
m8-8-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-5  15 }	
	
m8-8-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-5  16 }	
	

m8-8-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-5  17 }	

m8-8-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-5  18 }	

m8-8-5ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-8-5  19 }	

m8-8-5CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-8-5  20 }	

m8-8-5CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-8-5  21 }		
	
--
--	nb7-m8-8
--    
	

m8-8-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-6  1 }

m8-8-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-6  2 }

m8-8-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-6  3 }

m8-8-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-6  4 }
	
m8-8-6PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-6  5 }	
	
	
m8-8-6ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-6  6 }		
	
m8-8-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-6  7 }		
	
	
m8-8-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-6  8 }	


m8-8-6CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-6  9 }

	
m8-8-6OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-6  10 }	
	
m8-8-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-6  11 }	
	
	
m8-8-6UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-6  12 }	
	
m8-8-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-6  13 }		
	
m8-8-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-6  14 }		
	
m8-8-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-6  15 }	
	
m8-8-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-6  16 }	
	

m8-8-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-6  17 }	

	
m8-8-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-6  18 }	

m8-8-6ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-8-6  19 }

m8-8-6CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-8-6  20 }	

m8-8-6CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-8-6  21 }			
	
--
--	nb7-m8-8
--    

m8-8-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-7  1 }

m8-8-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-7  2 }

m8-8-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-7  3 }

m8-8-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-7  4 }
	
m8-8-7PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-7  5 }	
	
	
m8-8-7ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-7  6 }		
	
m8-8-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-7  7 }		
	
	
m8-8-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-7  8 }	


m8-8-7CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-7  9 }

m8-8-7OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-7  10 }	

m8-8-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-7  11 }	
	
	
m8-8-7UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-7  12 }	
	
m8-8-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-7  13 }		
	
m8-8-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-7  14 }		
	
m8-8-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-7  15 }	
	
m8-8-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-7  16 }	
	

m8-8-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-7  17 }		

m8-8-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-7  18 }	

m8-8-7ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-8-7  19 }	

m8-8-7CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-8-7  20 }	

m8-8-7CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-8-7  21 }		
	
--
--	nb7-m8-8
--    	

m8-8-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-8  1 }

m8-8-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-8  2 }

m8-8-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-8  3 }

m8-8-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-8  4 }
	
m8-8-8PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-8  5 }	
	
	
m8-8-8ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-8  6 }		
	
m8-8-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-8  7 }		
	
	
m8-8-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-8  8 }		
	
	
m8-8-8CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-8  9 }


m8-8-8OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-8  10 }	

m8-8-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-8  11 }	
	
	
m8-8-8UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-8  12 }	
	
m8-8-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-8  13 }		
	
m8-8-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-8  14 }		
	
m8-8-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-8  15 }	
	
m8-8-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-8  16 }	
	

m8-8-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-8  17 }		

m8-8-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8-8  18 }	

m8-8-8ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { nb7-m8-8-8  19 }	

m8-8-8CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-m8-8-8  20 }	

m8-8-8CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-m8-8-8  21 }		
	
m8-8Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8  9 }	
    
m8-8VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8  10 }

m8-8VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8  11 }

m8-8CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8  12 }

m8-8CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8  13 }
    
m8-8Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-m8-8  14 }



--
--	sd16-1
-- 
sd16-1-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { nb7-sd16-1-1  1 }

sd16-1-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { nb7-sd16-1-1  2 }

sd16-1-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { nb7-sd16-1-1  3 }

sd16-1-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { nb7-sd16-1-1  4 }
		
sd16-1-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { nb7-sd16-1-1  5 }		
	
	
sd16-1-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { nb7-sd16-1-1  6 }	
	
sd16-1-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { nb7-sd16-1-1  7 }		
	
sd16-1-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { nb7-sd16-1-1  8 }		
	
sd16-1-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { nb7-sd16-1-1  9 }	
	
sd16-1-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { nb7-sd16-1-1  10 }	
	

sd16-1-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { nb7-sd16-1-1  11 }	

sd16-1-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable nb7-sd16 -."
    DEFVAL { "" }
    ::= { nb7-sd16-1-1  12 }		
	
sd16-1-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-1-1  13 }	

sd16-1-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-1  14 }	

sd16-1-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-1-1  15 }	

sd16-1-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-1-1  16 }	
	
--
--	nb7-sd16-1
--    



sd16-1-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-2  1 }

sd16-1-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-2  2 }

sd16-1-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-2  3 }

sd16-1-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-2  4 }
	
	
sd16-1-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-2  5 }		
	
	
sd16-1-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-2  6 }		

	
sd16-1-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-2  7 }		
	
sd16-1-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-2  8 }		
	
sd16-1-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-2  9 }	
	
sd16-1-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-2  10 }	
	

sd16-1-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-2  11 }		

	
sd16-1-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-2  12 }	

sd16-1-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-1-2  13 }	

sd16-1-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-2  14 }	

sd16-1-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-1-2  15 }	

sd16-1-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-1-2  16 }	

	
--
--	nb7-sd16-1
--    
	

sd16-1-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-3  1 }

sd16-1-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-3  2 }

sd16-1-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-3  3 }

sd16-1-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-3  4 }
	
	
sd16-1-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-3  5 }		
	
	
sd16-1-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-3  6 }
	
	
sd16-1-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-3  7 }		
	
sd16-1-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-3  8 }		
	
sd16-1-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-3  9 }	
	
sd16-1-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-3  10 }	
	

sd16-1-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-3  11 }	


sd16-1-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-3  12 }	

sd16-1-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-1-3  13 }	

sd16-1-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-3  14 }	

sd16-1-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-1-3  15 }	

sd16-1-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-1-3  16 }	

	
--
--	nb7-sd16-1
--    
	
	

sd16-1-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-4  1 }

sd16-1-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-4  2 }

sd16-1-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-4  3 }

sd16-1-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-4  4 }
	
	
sd16-1-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-4  5 }		
	
	
sd16-1-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-4  6 }		
	
	
sd16-1-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-4  7 }		
	
sd16-1-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-4  8 }		
	
sd16-1-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-4  9 }	
	
sd16-1-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-4  10 }	
	

sd16-1-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-4  11 }	

	
sd16-1-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-4  12 }	

sd16-1-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-1-4  13 }	

sd16-1-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-4  14 }	

sd16-1-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-1-4  15 }	

sd16-1-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-1-4  16 }	


	
--
--	nb7-sd16-1
--    

	
	

sd16-1-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-5  1 }

sd16-1-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-5  2 }

sd16-1-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-5  3 }

sd16-1-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-5  4 }
	
	
sd16-1-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-5  5 }		
	
	
sd16-1-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-5  6 }	
	
	
sd16-1-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-5  7 }		
	
sd16-1-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-5  8 }		
	
sd16-1-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-5  9 }	
	
sd16-1-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-5  10 }	
	

sd16-1-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-5  11 }	

sd16-1-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-5  12 }	

sd16-1-5ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-1-5  13 }		

sd16-1-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-5  14 }	

sd16-1-5CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-1-5  15 }	

sd16-1-5CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-1-5  16 }	

	
--
--	nb7-sd16-1
--    
	

sd16-1-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-6  1 }

sd16-1-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-6  2 }

sd16-1-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-6  3 }

sd16-1-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-6  4 }
	
	
sd16-1-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-6  5 }		
	
	
sd16-1-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-6  6 }	

	
sd16-1-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-6  7 }		
	
sd16-1-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-6  8 }		
	
sd16-1-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-6  9 }	
	
sd16-1-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-6  10 }	
	

sd16-1-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-6  11 }	

	
sd16-1-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-6  12 }	

sd16-1-6ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-1-6  13 }		

sd16-1-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-6  14 }	

sd16-1-6CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-1-6  15 }	

sd16-1-6CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-1-6  16 }	

	
--
--	nb7-sd16-1
--    

sd16-1-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-7  1 }

sd16-1-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-7  2 }

sd16-1-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-7  3 }

sd16-1-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-7  4 }
	
	
sd16-1-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-7  5 }		
	
	
sd16-1-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-7  6 }	


	
sd16-1-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-7  7 }		
	
sd16-1-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-7  8 }		
	
sd16-1-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-7  9 }	
	
sd16-1-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-7  10 }	
	

sd16-1-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-7  11 }		

sd16-1-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-7  12 }	

sd16-1-7ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-1-7  13 }	

sd16-1-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-7  14 }	

sd16-1-7CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-1-7  15 }	

sd16-1-7CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-1-7  16 }	
	
	
--
--	nb7-sd16-1
--    	

sd16-1-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-8  1 }

sd16-1-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-8  2 }

sd16-1-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-8  3 }

sd16-1-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-8  4 }
	
	
sd16-1-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-8  5 }		
	
	
sd16-1-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-8  6 }		
	
	
	
sd16-1-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-8  7 }		
	
sd16-1-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-8  8 }		
	
sd16-1-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-8  9 }	
	
sd16-1-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-8  10 }	
	

sd16-1-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-8  11 }		

sd16-1-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-8  12 }	

sd16-1-8ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-1-8  13 }		

sd16-1-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-8  14 }	

sd16-1-8CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-1-8  15 }	

sd16-1-8CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-1-8  16 }	

	--
--	nb7-sd16-1
--    	

sd16-1-9Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-9  1 }

sd16-1-9Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-9  2 }

sd16-1-9Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-9  3 }

sd16-1-9Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-9  4 }
	
	
sd16-1-9FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-9  5 }		
	
	
sd16-1-9Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-9  6 }		
	
	
	
sd16-1-9EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-9  7 }		
	
sd16-1-9VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-9  8 }		
	
sd16-1-9VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-9  9 }	
	
sd16-1-9CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-9  10 }	
	

sd16-1-9CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-9  11 }		

sd16-1-9Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-9  12 }	

sd16-1-9ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-1-9  13 }		

sd16-1-9UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-9  14 }	

sd16-1-9CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-1-9  15 }	

sd16-1-9CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-1-9  16 }	

	
--
--	nb7-sd16-1
--    	

sd16-1-10Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-10  1 }

sd16-1-10Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-10  2 }

sd16-1-10Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-10  3 }

sd16-1-10Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-10  4 }
	
	
sd16-1-10FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-10  5 }		
	
	
sd16-1-10Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-10  6 }		
	
	
	
sd16-1-10EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-10  7 }		
	
sd16-1-10VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-10  8 }		
	
sd16-1-10VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-10  9 }	
	
sd16-1-10CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-10  10 }	
	

sd16-1-10CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-10  11 }		

sd16-1-10Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-10  12 }	

sd16-1-10ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-1-10  13 }		

sd16-1-10UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-10  14 }	

sd16-1-10CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-1-10  15 }	

sd16-1-10CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-1-10  16 }	

	
--
--	nb7-sd16-1
--    	

sd16-1-11Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-11  1 }

sd16-1-11Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-11  2 }

sd16-1-11Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-11  3 }

sd16-1-11Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-11  4 }
	
	
sd16-1-11FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-11  5 }		
	
	
sd16-1-11Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-11  6 }		
	
	
	
sd16-1-11EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-11  7 }		
	
sd16-1-11VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-11  8 }		
	
sd16-1-11VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-11  9 }	
	
sd16-1-11CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-11  10 }	
	

sd16-1-11CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-11  11 }		

sd16-1-11Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-11  12 }	

sd16-1-11ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-1-11  13 }		

sd16-1-11UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-11  14 }	

sd16-1-11CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-1-11  15 }	

sd16-1-11CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-1-11  16 }	

	
--
--	nb7-sd16-1
--    	

sd16-1-12Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-12  1 }

sd16-1-12Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-12  2 }

sd16-1-12Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-12  3 }

sd16-1-12Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-12  4 }
	
	
sd16-1-12FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-12  5 }		
	
	
sd16-1-12Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-12  6 }		
	
	
	
sd16-1-12EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-12  7 }		
	
sd16-1-12VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-12  8 }		
	
sd16-1-12VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-12  9 }	
	
sd16-1-12CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-12  10 }	
	

sd16-1-12CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-12  11 }		

sd16-1-12Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-12  12 }	

sd16-1-12ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-1-12  13 }		

sd16-1-12UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-12  14 }	

sd16-1-12CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-1-12  15 }	

sd16-1-12CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-1-12  16 }	

	
--
--	nb7-sd16-1
--    	

sd16-1-13Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-13  1 }

sd16-1-13Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-13  2 }

sd16-1-13Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-13  3 }

sd16-1-13Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-13  4 }
	
	
sd16-1-13FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-13  5 }		
	
	
sd16-1-13Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-13  6 }		
	
	
	
sd16-1-13EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-13  7 }		
	
sd16-1-13VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-13  8 }		
	
sd16-1-13VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-13  9 }	
	
sd16-1-13CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-13  10 }	
	

sd16-1-13CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-13  11 }		

sd16-1-13Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-13  12 }	

sd16-1-13ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-1-13  13 }		

sd16-1-13UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-13  14 }	

sd16-1-13CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-1-13  15 }	

sd16-1-13CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-1-13  16 }	

	
--
--	nb7-sd16-1
--    	

sd16-1-14Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-14  1 }

sd16-1-14Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-14  2 }

sd16-1-14Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-14  3 }

sd16-1-14Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-14  4 }
	
	
sd16-1-14FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-14  5 }		
	
	
sd16-1-14Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-14  6 }		
	
	
	
sd16-1-14EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-14  7 }		
	
sd16-1-14VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-14  8 }		
	
sd16-1-14VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-14  9 }	
	
sd16-1-14CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-14  10 }	
	

sd16-1-14CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-14  11 }		

sd16-1-14Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-14  12 }	

sd16-1-14ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-1-14  13 }		

sd16-1-14UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-14  14 }	

sd16-1-14CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-1-14  15 }	

sd16-1-14CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-1-14  16 }	

	
--
--	nb7-sd16-1
--    	

sd16-1-15Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-15  1 }

sd16-1-15Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-15  2 }

sd16-1-15Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-15  3 }

sd16-1-15Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-15  4 }
	
	
sd16-1-15FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-15  5 }		
	
	
sd16-1-15Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-15  6 }		
	
	
	
sd16-1-15EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-15  7 }		
	
sd16-1-15VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-15  8 }		
	
sd16-1-15VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-15  9 }	
	
sd16-1-15CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-15  10 }	
	

sd16-1-15CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-15  11 }		

sd16-1-15Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-15  12 }	

sd16-1-15ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-1-15  13 }		

sd16-1-15UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-15  14 }	

sd16-1-15CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-1-15  15 }	

sd16-1-15CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-1-15  16 }	

	
--
--	nb7-sd16-1
--    	

sd16-1-16Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-16  1 }

sd16-1-16Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-16  2 }

sd16-1-16Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-16  3 }

sd16-1-16Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-16  4 }
	
	
sd16-1-16FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-16  5 }		
	
	
sd16-1-16Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-16  6 }		
	
	
	
sd16-1-16EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-16  7 }		
	
sd16-1-16VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-16  8 }		
	
sd16-1-16VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-16  9 }	
	
sd16-1-16CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-16  10 }	
	

sd16-1-16CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-16  11 }		

sd16-1-16Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-16  12 }	

sd16-1-16ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-1-16  13 }		

sd16-1-16UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1-16  14 }	

sd16-1-16CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-1-16  15 }	

sd16-1-16CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-1-16  16 }	

	

sd16-1Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1  17 }	
    
sd16-1VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1  18 }

sd16-1VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1  19 }

sd16-1CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1  20 }

sd16-1CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1  21 }
    
sd16-1Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1  22 }

sd16-1Temperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1  23 }

sd16-1TemperatureLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1  24 }

sd16-1TemperatureUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1  25 }

sd16-1Humidity OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1  26 }

sd16-1HumidityLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1  27 }

sd16-1HumidityUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1  28 }

sd16-1Event1 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1  29 }

sd16-1Event2 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-1  30 }


--
--	sd16-2
-- 
sd16-2-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { nb7-sd16-2-1  1 }

sd16-2-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { nb7-sd16-2-1  2 }

sd16-2-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { nb7-sd16-2-1  3 }

sd16-2-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { nb7-sd16-2-1  4 }
		
sd16-2-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { nb7-sd16-2-1  5 }		
	
	
sd16-2-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { nb7-sd16-2-1  6 }	
	
sd16-2-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { nb7-sd16-2-1  7 }		
	
sd16-2-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { nb7-sd16-2-1  8 }		
	
sd16-2-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { nb7-sd16-2-1  9 }	
	
sd16-2-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { nb7-sd16-2-1  10 }	
	

sd16-2-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { nb7-sd16-2-1  11 }	

sd16-2-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable nb7-sd16 -."
    DEFVAL { "" }
    ::= { nb7-sd16-2-1  12 }		
	
sd16-2-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-2-1  13 }	

sd16-2-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-1  14 }	

sd16-2-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-2-1  15 }	

sd16-2-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-2-1  16 }	

	
--
--	nb7-sd16-2
--    



sd16-2-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-2  1 }

sd16-2-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-2  2 }

sd16-2-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-2  3 }

sd16-2-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-2  4 }
	
	
sd16-2-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-2  5 }		
	
	
sd16-2-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-2  6 }		

	
sd16-2-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-2  7 }		
	
sd16-2-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-2  8 }		
	
sd16-2-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-2  9 }	
	
sd16-2-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-2  10 }	
	

sd16-2-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-2  11 }		

	
sd16-2-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-2  12 }	

sd16-2-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-2-2  13 }	

sd16-2-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-2  14 }	

sd16-2-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-2-2  15 }	

sd16-2-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-2-2  16 }	

	
--
--	nb7-sd16-2
--    
	

sd16-2-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-3  1 }

sd16-2-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-3  2 }

sd16-2-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-3  3 }

sd16-2-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-3  4 }
	
	
sd16-2-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-3  5 }		
	
	
sd16-2-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-3  6 }
	
	
sd16-2-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-3  7 }		
	
sd16-2-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-3  8 }		
	
sd16-2-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-3  9 }	
	
sd16-2-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-3  10 }	
	

sd16-2-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-3  11 }	


sd16-2-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-3  12 }	

sd16-2-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-2-3  13 }	

sd16-2-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-3  14 }	

sd16-2-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-2-3  15 }	

sd16-2-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-2-3  16 }	

	
--
--	nb7-sd16-2
--    
	
	

sd16-2-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-4  1 }

sd16-2-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-4  2 }

sd16-2-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-4  3 }

sd16-2-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-4  4 }
	
	
sd16-2-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-4  5 }		
	
	
sd16-2-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-4  6 }		
	
	
sd16-2-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-4  7 }		
	
sd16-2-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-4  8 }		
	
sd16-2-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-4  9 }	
	
sd16-2-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-4  10 }	
	

sd16-2-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-4  11 }	

	
sd16-2-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-4  12 }	

sd16-2-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-2-4  13 }	

sd16-2-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-4  14 }	

sd16-2-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-2-4  15 }	

sd16-2-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-2-4  16 }	


	
--
--	nb7-sd16-2
--    

	
	

sd16-2-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-5  1 }

sd16-2-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-5  2 }

sd16-2-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-5  3 }

sd16-2-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-5  4 }
	
	
sd16-2-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-5  5 }		
	
	
sd16-2-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-5  6 }	
	
	
sd16-2-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-5  7 }		
	
sd16-2-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-5  8 }		
	
sd16-2-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-5  9 }	
	
sd16-2-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-5  10 }	
	

sd16-2-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-5  11 }	

sd16-2-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-5  12 }	

sd16-2-5ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-2-5  13 }		

sd16-2-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-5  14 }	

sd16-2-5CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-2-5  15 }	

sd16-2-5CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-2-5  16 }	

	
--
--	nb7-sd16-2
--    
	

sd16-2-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-6  1 }

sd16-2-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-6  2 }

sd16-2-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-6  3 }

sd16-2-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-6  4 }
	
	
sd16-2-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-6  5 }		
	
	
sd16-2-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-6  6 }	

	
sd16-2-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-6  7 }		
	
sd16-2-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-6  8 }		
	
sd16-2-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-6  9 }	
	
sd16-2-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-6  10 }	
	

sd16-2-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-6  11 }	

	
sd16-2-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-6  12 }	

sd16-2-6ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-2-6  13 }		

sd16-2-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-6  14 }	

sd16-2-6CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-2-6  15 }	

sd16-2-6CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-2-6  16 }	

	
--
--	nb7-sd16-2
--    

sd16-2-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-7  1 }

sd16-2-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-7  2 }

sd16-2-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-7  3 }

sd16-2-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-7  4 }
	
	
sd16-2-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-7  5 }		
	
	
sd16-2-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-7  6 }	


	
sd16-2-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-7  7 }		
	
sd16-2-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-7  8 }		
	
sd16-2-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-7  9 }	
	
sd16-2-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-7  10 }	
	

sd16-2-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-7  11 }		

sd16-2-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-7  12 }	

sd16-2-7ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-2-7  13 }	

sd16-2-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-7  14 }	

sd16-2-7CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-2-7  15 }	

sd16-2-7CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-2-7  16 }	
	
	
--
--	nb7-sd16-2
--    	

sd16-2-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-8  1 }

sd16-2-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-8  2 }

sd16-2-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-8  3 }

sd16-2-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-8  4 }
	
	
sd16-2-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-8  5 }		
	
	
sd16-2-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-8  6 }		
	
	
	
sd16-2-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-8  7 }		
	
sd16-2-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-8  8 }		
	
sd16-2-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-8  9 }	
	
sd16-2-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-8  10 }	
	

sd16-2-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-8  11 }		

sd16-2-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-8  12 }	

sd16-2-8ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-2-8  13 }		

sd16-2-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-8  14 }	

sd16-2-8CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-2-8  15 }	

sd16-2-8CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-2-8  16 }	

	--
--	nb7-sd16-2
--    	

sd16-2-9Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-9  1 }

sd16-2-9Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-9  2 }

sd16-2-9Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-9  3 }

sd16-2-9Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-9  4 }
	
	
sd16-2-9FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-9  5 }		
	
	
sd16-2-9Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-9  6 }		
	
	
	
sd16-2-9EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-9  7 }		
	
sd16-2-9VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-9  8 }		
	
sd16-2-9VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-9  9 }	
	
sd16-2-9CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-9  10 }	
	

sd16-2-9CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-9  11 }		

sd16-2-9Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-9  12 }	

sd16-2-9ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-2-9  13 }		

sd16-2-9UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-9  14 }	

sd16-2-9CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-2-9  15 }	

sd16-2-9CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-2-9  16 }	

	
--
--	nb7-sd16-2
--    	

sd16-2-10Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-10  1 }

sd16-2-10Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-10  2 }

sd16-2-10Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-10  3 }

sd16-2-10Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-10  4 }
	
	
sd16-2-10FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-10  5 }		
	
	
sd16-2-10Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-10  6 }		
	
	
	
sd16-2-10EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-10  7 }		
	
sd16-2-10VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-10  8 }		
	
sd16-2-10VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-10  9 }	
	
sd16-2-10CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-10  10 }	
	

sd16-2-10CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-10  11 }		

sd16-2-10Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-10  12 }	

sd16-2-10ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-2-10  13 }		

sd16-2-10UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-10  14 }	

sd16-2-10CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-2-10  15 }	

sd16-2-10CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-2-10  16 }	

	
--
--	nb7-sd16-2
--    	

sd16-2-11Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-11  1 }

sd16-2-11Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-11  2 }

sd16-2-11Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-11  3 }

sd16-2-11Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-11  4 }
	
	
sd16-2-11FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-11  5 }		
	
	
sd16-2-11Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-11  6 }		
	
	
	
sd16-2-11EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-11  7 }		
	
sd16-2-11VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-11  8 }		
	
sd16-2-11VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-11  9 }	
	
sd16-2-11CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-11  10 }	
	

sd16-2-11CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-11  11 }		

sd16-2-11Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-11  12 }	

sd16-2-11ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-2-11  13 }		

sd16-2-11UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-11  14 }	

sd16-2-11CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-2-11  15 }	

sd16-2-11CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-2-11  16 }	

	
--
--	nb7-sd16-2
--    	

sd16-2-12Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-12  1 }

sd16-2-12Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-12  2 }

sd16-2-12Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-12  3 }

sd16-2-12Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-12  4 }
	
	
sd16-2-12FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-12  5 }		
	
	
sd16-2-12Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-12  6 }		
	
	
	
sd16-2-12EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-12  7 }		
	
sd16-2-12VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-12  8 }		
	
sd16-2-12VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-12  9 }	
	
sd16-2-12CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-12  10 }	
	

sd16-2-12CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-12  11 }		

sd16-2-12Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-12  12 }	

sd16-2-12ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-2-12  13 }		

sd16-2-12UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-12  14 }	

sd16-2-12CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-2-12  15 }	

sd16-2-12CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-2-12  16 }	

	
--
--	nb7-sd16-2
--    	

sd16-2-13Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-13  1 }

sd16-2-13Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-13  2 }

sd16-2-13Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-13  3 }

sd16-2-13Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-13  4 }
	
	
sd16-2-13FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-13  5 }		
	
	
sd16-2-13Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-13  6 }		
	
	
	
sd16-2-13EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-13  7 }		
	
sd16-2-13VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-13  8 }		
	
sd16-2-13VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-13  9 }	
	
sd16-2-13CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-13  10 }	
	

sd16-2-13CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-13  11 }		

sd16-2-13Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-13  12 }	

sd16-2-13ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-2-13  13 }		

sd16-2-13UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-13  14 }	

sd16-2-13CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-2-13  15 }	

sd16-2-13CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-2-13  16 }	

	
--
--	nb7-sd16-2
--    	

sd16-2-14Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-14  1 }

sd16-2-14Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-14  2 }

sd16-2-14Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-14  3 }

sd16-2-14Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-14  4 }
	
	
sd16-2-14FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-14  5 }		
	
	
sd16-2-14Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-14  6 }		
	
	
	
sd16-2-14EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-14  7 }		
	
sd16-2-14VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-14  8 }		
	
sd16-2-14VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-14  9 }	
	
sd16-2-14CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-14  10 }	
	

sd16-2-14CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-14  11 }		

sd16-2-14Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-14  12 }	

sd16-2-14ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-2-14  13 }		

sd16-2-14UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-14  14 }	

sd16-2-14CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-2-14  15 }	

sd16-2-14CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-2-14  16 }	

	
--
--	nb7-sd16-2
--    	

sd16-2-15Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-15  1 }

sd16-2-15Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-15  2 }

sd16-2-15Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-15  3 }

sd16-2-15Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-15  4 }
	
	
sd16-2-15FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-15  5 }		
	
	
sd16-2-15Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-15  6 }		
	
	
	
sd16-2-15EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-15  7 }		
	
sd16-2-15VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-15  8 }		
	
sd16-2-15VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-15  9 }	
	
sd16-2-15CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-15  10 }	
	

sd16-2-15CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-15  11 }		

sd16-2-15Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-15  12 }	

sd16-2-15ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-2-15  13 }		

sd16-2-15UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-15  14 }	

sd16-2-15CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-2-15  15 }	

sd16-2-15CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-2-15  16 }	

	
--
--	nb7-sd16-2
--    	

sd16-2-16Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-16  1 }

sd16-2-16Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-16  2 }

sd16-2-16Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-16  3 }

sd16-2-16Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-16  4 }
	
	
sd16-2-16FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-16  5 }		
	
	
sd16-2-16Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-16  6 }		
	
	
	
sd16-2-16EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-16  7 }		
	
sd16-2-16VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-16  8 }		
	
sd16-2-16VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-16  9 }	
	
sd16-2-16CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-16  10 }	
	

sd16-2-16CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-16  11 }		

sd16-2-16Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-16  12 }	

sd16-2-16ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-2-16  13 }		

sd16-2-16UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2-16  14 }	

sd16-2-16CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-2-16  15 }	

sd16-2-16CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-2-16  16 }	

	

sd16-2Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2  17 }	
    
sd16-2VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2  18 }

sd16-2VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2  19 }

sd16-2CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2  20 }

sd16-2CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2  21 }
    
sd16-2Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2  22 }

sd16-2Temperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2  23 }

sd16-2TemperatureLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2  24 }

sd16-2TemperatureUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2  25 }

sd16-2Humidity OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2  26 }

sd16-2HumidityLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2  27 }

sd16-2HumidityUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2  28 }

sd16-2Event1 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2  29 }

sd16-2Event2 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-2  30 }


--
--	sd16-3
-- 
sd16-3-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { nb7-sd16-3-1  1 }

sd16-3-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { nb7-sd16-3-1  2 }

sd16-3-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { nb7-sd16-3-1  3 }

sd16-3-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { nb7-sd16-3-1  4 }
		
sd16-3-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { nb7-sd16-3-1  5 }		
	
	
sd16-3-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { nb7-sd16-3-1  6 }	
	
sd16-3-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { nb7-sd16-3-1  7 }		
	
sd16-3-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { nb7-sd16-3-1  8 }		
	
sd16-3-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { nb7-sd16-3-1  9 }	
	
sd16-3-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { nb7-sd16-3-1  10 }	
	

sd16-3-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { nb7-sd16-3-1  11 }	

sd16-3-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable nb7-sd16 -."
    DEFVAL { "" }
    ::= { nb7-sd16-3-1  12 }		
	
sd16-3-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-3-1  13 }	

sd16-3-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-1  14 }	

sd16-3-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-3-1  15 }	

sd16-3-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-3-1  16 }	


	
--
--	nb7-sd16-3
--    



sd16-3-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-2  1 }

sd16-3-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-2  2 }

sd16-3-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-2  3 }

sd16-3-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-2  4 }
	
	
sd16-3-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-2  5 }		
	
	
sd16-3-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-2  6 }		

	
sd16-3-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-2  7 }		
	
sd16-3-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-2  8 }		
	
sd16-3-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-2  9 }	
	
sd16-3-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-2  10 }	
	

sd16-3-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-2  11 }		

	
sd16-3-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-2  12 }	

sd16-3-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-3-2  13 }	

sd16-3-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-2  14 }	

sd16-3-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-3-2  15 }	

sd16-3-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-3-2  16 }	

	
--
--	nb7-sd16-3
--    
	

sd16-3-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-3  1 }

sd16-3-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-3  2 }

sd16-3-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-3  3 }

sd16-3-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-3  4 }
	
	
sd16-3-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-3  5 }		
	
	
sd16-3-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-3  6 }
	
	
sd16-3-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-3  7 }		
	
sd16-3-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-3  8 }		
	
sd16-3-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-3  9 }	
	
sd16-3-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-3  10 }	
	

sd16-3-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-3  11 }	


sd16-3-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-3  12 }	

sd16-3-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-3-3  13 }	

sd16-3-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-3  14 }	

sd16-3-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-3-3  15 }	

sd16-3-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-3-3  16 }	

	
--
--	nb7-sd16-3
--    
	
	

sd16-3-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-4  1 }

sd16-3-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-4  2 }

sd16-3-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-4  3 }

sd16-3-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-4  4 }
	
	
sd16-3-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-4  5 }		
	
	
sd16-3-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-4  6 }		
	
	
sd16-3-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-4  7 }		
	
sd16-3-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-4  8 }		
	
sd16-3-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-4  9 }	
	
sd16-3-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-4  10 }	
	

sd16-3-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-4  11 }	

	
sd16-3-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-4  12 }	

sd16-3-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-3-4  13 }	

sd16-3-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-4  14 }	

sd16-3-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-3-4  15 }	

sd16-3-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-3-4  16 }	


	
--
--	nb7-sd16-3
--    

	
	

sd16-3-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-5  1 }

sd16-3-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-5  2 }

sd16-3-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-5  3 }

sd16-3-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-5  4 }
	
	
sd16-3-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-5  5 }		
	
	
sd16-3-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-5  6 }	
	
	
sd16-3-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-5  7 }		
	
sd16-3-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-5  8 }		
	
sd16-3-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-5  9 }	
	
sd16-3-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-5  10 }	
	

sd16-3-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-5  11 }	

sd16-3-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-5  12 }	

sd16-3-5ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-3-5  13 }		

sd16-3-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-5  14 }	

sd16-3-5CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-3-5  15 }	

sd16-3-5CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-3-5  16 }	

	
--
--	nb7-sd16-3
--    
	

sd16-3-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-6  1 }

sd16-3-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-6  2 }

sd16-3-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-6  3 }

sd16-3-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-6  4 }
	
	
sd16-3-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-6  5 }		
	
	
sd16-3-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-6  6 }	

	
sd16-3-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-6  7 }		
	
sd16-3-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-6  8 }		
	
sd16-3-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-6  9 }	
	
sd16-3-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-6  10 }	
	

sd16-3-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-6  11 }	

	
sd16-3-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-6  12 }	

sd16-3-6ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-3-6  13 }		

sd16-3-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-6  14 }	

sd16-3-6CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-3-6  15 }	

sd16-3-6CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-3-6  16 }	

	
--
--	nb7-sd16-3
--    

sd16-3-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-7  1 }

sd16-3-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-7  2 }

sd16-3-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-7  3 }

sd16-3-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-7  4 }
	
	
sd16-3-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-7  5 }		
	
	
sd16-3-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-7  6 }	


	
sd16-3-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-7  7 }		
	
sd16-3-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-7  8 }		
	
sd16-3-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-7  9 }	
	
sd16-3-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-7  10 }	
	

sd16-3-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-7  11 }		

sd16-3-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-7  12 }	

sd16-3-7ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-3-7  13 }	

sd16-3-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-7  14 }	

sd16-3-7CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-3-7  15 }	

sd16-3-7CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-3-7  16 }	
	
	
--
--	nb7-sd16-3
--    	

sd16-3-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-8  1 }

sd16-3-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-8  2 }

sd16-3-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-8  3 }

sd16-3-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-8  4 }
	
	
sd16-3-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-8  5 }		
	
	
sd16-3-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-8  6 }		
	
	
	
sd16-3-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-8  7 }		
	
sd16-3-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-8  8 }		
	
sd16-3-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-8  9 }	
	
sd16-3-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-8  10 }	
	

sd16-3-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-8  11 }		

sd16-3-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-8  12 }	

sd16-3-8ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-3-8  13 }		

sd16-3-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-8  14 }	

sd16-3-8CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-3-8  15 }	

sd16-3-8CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-3-8  16 }	

	--
--	nb7-sd16-3
--    	

sd16-3-9Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-9  1 }

sd16-3-9Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-9  2 }

sd16-3-9Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-9  3 }

sd16-3-9Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-9  4 }
	
	
sd16-3-9FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-9  5 }		
	
	
sd16-3-9Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-9  6 }		
	
	
	
sd16-3-9EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-9  7 }		
	
sd16-3-9VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-9  8 }		
	
sd16-3-9VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-9  9 }	
	
sd16-3-9CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-9  10 }	
	

sd16-3-9CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-9  11 }		

sd16-3-9Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-9  12 }	

sd16-3-9ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-3-9  13 }		

sd16-3-9UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-9  14 }	

sd16-3-9CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-3-9  15 }	

sd16-3-9CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-3-9  16 }	

	
--
--	nb7-sd16-3
--    	

sd16-3-10Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-10  1 }

sd16-3-10Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-10  2 }

sd16-3-10Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-10  3 }

sd16-3-10Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-10  4 }
	
	
sd16-3-10FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-10  5 }		
	
	
sd16-3-10Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-10  6 }		
	
	
	
sd16-3-10EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-10  7 }		
	
sd16-3-10VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-10  8 }		
	
sd16-3-10VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-10  9 }	
	
sd16-3-10CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-10  10 }	
	

sd16-3-10CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-10  11 }		

sd16-3-10Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-10  12 }	

sd16-3-10ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-3-10  13 }		

sd16-3-10UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-10  14 }	

sd16-3-10CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-3-10  15 }	

sd16-3-10CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-3-10  16 }	

	
--
--	nb7-sd16-3
--    	

sd16-3-11Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-11  1 }

sd16-3-11Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-11  2 }

sd16-3-11Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-11  3 }

sd16-3-11Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-11  4 }
	
	
sd16-3-11FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-11  5 }		
	
	
sd16-3-11Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-11  6 }		
	
	
	
sd16-3-11EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-11  7 }		
	
sd16-3-11VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-11  8 }		
	
sd16-3-11VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-11  9 }	
	
sd16-3-11CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-11  10 }	
	

sd16-3-11CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-11  11 }		

sd16-3-11Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-11  12 }	

sd16-3-11ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-3-11  13 }		

sd16-3-11UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-11  14 }	

sd16-3-11CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-3-11  15 }	

sd16-3-11CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-3-11  16 }	

	
--
--	nb7-sd16-3
--    	

sd16-3-12Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-12  1 }

sd16-3-12Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-12  2 }

sd16-3-12Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-12  3 }

sd16-3-12Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-12  4 }
	
	
sd16-3-12FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-12  5 }		
	
	
sd16-3-12Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-12  6 }		
	
	
	
sd16-3-12EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-12  7 }		
	
sd16-3-12VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-12  8 }		
	
sd16-3-12VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-12  9 }	
	
sd16-3-12CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-12  10 }	
	

sd16-3-12CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-12  11 }		

sd16-3-12Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-12  12 }	

sd16-3-12ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-3-12  13 }		

sd16-3-12UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-12  14 }	

sd16-3-12CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-3-12  15 }	

sd16-3-12CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-3-12  16 }	

	
--
--	nb7-sd16-3
--    	

sd16-3-13Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-13  1 }

sd16-3-13Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-13  2 }

sd16-3-13Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-13  3 }

sd16-3-13Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-13  4 }
	
	
sd16-3-13FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-13  5 }		
	
	
sd16-3-13Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-13  6 }		
	
	
	
sd16-3-13EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-13  7 }		
	
sd16-3-13VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-13  8 }		
	
sd16-3-13VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-13  9 }	
	
sd16-3-13CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-13  10 }	
	

sd16-3-13CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-13  11 }		

sd16-3-13Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-13  12 }	

sd16-3-13ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-3-13  13 }		

sd16-3-13UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-13  14 }	

sd16-3-13CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-3-13  15 }	

sd16-3-13CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-3-13  16 }	

	
--
--	nb7-sd16-3
--    	

sd16-3-14Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-14  1 }

sd16-3-14Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-14  2 }

sd16-3-14Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-14  3 }

sd16-3-14Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-14  4 }
	
	
sd16-3-14FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-14  5 }		
	
	
sd16-3-14Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-14  6 }		
	
	
	
sd16-3-14EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-14  7 }		
	
sd16-3-14VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-14  8 }		
	
sd16-3-14VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-14  9 }	
	
sd16-3-14CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-14  10 }	
	

sd16-3-14CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-14  11 }		

sd16-3-14Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-14  12 }	

sd16-3-14ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-3-14  13 }		

sd16-3-14UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-14  14 }	

sd16-3-14CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-3-14  15 }	

sd16-3-14CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-3-14  16 }	

	
--
--	nb7-sd16-3
--    	

sd16-3-15Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-15  1 }

sd16-3-15Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-15  2 }

sd16-3-15Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-15  3 }

sd16-3-15Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-15  4 }
	
	
sd16-3-15FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-15  5 }		
	
	
sd16-3-15Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-15  6 }		
	
	
	
sd16-3-15EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-15  7 }		
	
sd16-3-15VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-15  8 }		
	
sd16-3-15VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-15  9 }	
	
sd16-3-15CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-15  10 }	
	

sd16-3-15CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-15  11 }		

sd16-3-15Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-15  12 }	

sd16-3-15ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-3-15  13 }		

sd16-3-15UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-15  14 }	

sd16-3-15CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-3-15  15 }	

sd16-3-15CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-3-15  16 }	

	
--
--	nb7-sd16-3
--    	

sd16-3-16Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-16  1 }

sd16-3-16Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-16  2 }

sd16-3-16Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-16  3 }

sd16-3-16Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-16  4 }
	
	
sd16-3-16FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-16  5 }		
	
	
sd16-3-16Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-16  6 }		
	
	
	
sd16-3-16EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-16  7 }		
	
sd16-3-16VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-16  8 }		
	
sd16-3-16VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-16  9 }	
	
sd16-3-16CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-16  10 }	
	

sd16-3-16CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-16  11 }		

sd16-3-16Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-16  12 }	

sd16-3-16ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-3-16  13 }		

sd16-3-16UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3-16  14 }	

sd16-3-16CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-3-16  15 }	

sd16-3-16CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-3-16  16 }	

	

sd16-3Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3  17 }	
    
sd16-3VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3  18 }

sd16-3VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3  19 }

sd16-3CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3  20 }

sd16-3CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3  21 }
    
sd16-3Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3  22 }

sd16-3Temperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3  23 }

sd16-3TemperatureLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3  24 }

sd16-3TemperatureUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3  25 }

sd16-3Humidity OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3  26 }

sd16-3HumidityLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3  27 }

sd16-3HumidityUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3  28 }

sd16-3Event1 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3  29 }

sd16-3Event2 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-3  30 }


--
--	sd16-4
-- 

sd16-4-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { nb7-sd16-4-1  1 }

sd16-4-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { nb7-sd16-4-1  2 }

sd16-4-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { nb7-sd16-4-1  3 }

sd16-4-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { nb7-sd16-4-1  4 }
		
sd16-4-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { nb7-sd16-4-1  5 }		
	
	
sd16-4-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { nb7-sd16-4-1  6 }	
	
sd16-4-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { nb7-sd16-4-1  7 }		
	
sd16-4-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { nb7-sd16-4-1  8 }		
	
sd16-4-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { nb7-sd16-4-1  9 }	
	
sd16-4-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { nb7-sd16-4-1  10 }	
	

sd16-4-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { nb7-sd16-4-1  11 }	

sd16-4-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable nb7-sd16 -."
    DEFVAL { "" }
    ::= { nb7-sd16-4-1  12 }		
	
sd16-4-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-4-1  13 }	

sd16-4-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-1  14 }	

sd16-4-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-4-1  15 }	

sd16-4-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-4-1  16 }	


	
--
--	nb7-sd16-4
--    



sd16-4-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-2  1 }

sd16-4-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-2  2 }

sd16-4-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-2  3 }

sd16-4-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-2  4 }
	
	
sd16-4-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-2  5 }		
	
	
sd16-4-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-2  6 }		

	
sd16-4-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-2  7 }		
	
sd16-4-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-2  8 }		
	
sd16-4-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-2  9 }	
	
sd16-4-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-2  10 }	
	

sd16-4-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-2  11 }		

	
sd16-4-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-2  12 }	

sd16-4-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-4-2  13 }	

sd16-4-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-2  14 }	

sd16-4-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-4-2  15 }	

sd16-4-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-4-2  16 }	

	
--
--	nb7-sd16-4
--    
	

sd16-4-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-3  1 }

sd16-4-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-3  2 }

sd16-4-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-3  3 }

sd16-4-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-3  4 }
	
	
sd16-4-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-3  5 }		
	
	
sd16-4-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-3  6 }
	
	
sd16-4-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-3  7 }		
	
sd16-4-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-3  8 }		
	
sd16-4-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-3  9 }	
	
sd16-4-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-3  10 }	
	

sd16-4-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-3  11 }	


sd16-4-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-3  12 }	

sd16-4-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-4-3  13 }	

sd16-4-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-3  14 }	

sd16-4-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-4-3  15 }	

sd16-4-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-4-3  16 }	

	
--
--	nb7-sd16-4
--    
	
	

sd16-4-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-4  1 }

sd16-4-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-4  2 }

sd16-4-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-4  3 }

sd16-4-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-4  4 }
	
	
sd16-4-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-4  5 }		
	
	
sd16-4-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-4  6 }		
	
	
sd16-4-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-4  7 }		
	
sd16-4-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-4  8 }		
	
sd16-4-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-4  9 }	
	
sd16-4-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-4  10 }	
	

sd16-4-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-4  11 }	

	
sd16-4-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-4  12 }	

sd16-4-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-4-4  13 }	

sd16-4-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-4  14 }	

sd16-4-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-4-4  15 }	

sd16-4-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-4-4  16 }	


	
--
--	nb7-sd16-4
--    

	
	

sd16-4-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-5  1 }

sd16-4-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-5  2 }

sd16-4-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-5  3 }

sd16-4-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-5  4 }
	
	
sd16-4-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-5  5 }		
	
	
sd16-4-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-5  6 }	
	
	
sd16-4-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-5  7 }		
	
sd16-4-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-5  8 }		
	
sd16-4-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-5  9 }	
	
sd16-4-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-5  10 }	
	

sd16-4-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-5  11 }	

sd16-4-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-5  12 }	

sd16-4-5ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-4-5  13 }		

sd16-4-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-5  14 }	

sd16-4-5CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-4-5  15 }	

sd16-4-5CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-4-5  16 }	

	
--
--	nb7-sd16-4
--    
	

sd16-4-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-6  1 }

sd16-4-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-6  2 }

sd16-4-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-6  3 }

sd16-4-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-6  4 }
	
	
sd16-4-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-6  5 }		
	
	
sd16-4-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-6  6 }	

	
sd16-4-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-6  7 }		
	
sd16-4-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-6  8 }		
	
sd16-4-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-6  9 }	
	
sd16-4-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-6  10 }	
	

sd16-4-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-6  11 }	

	
sd16-4-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-6  12 }	

sd16-4-6ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-4-6  13 }		

sd16-4-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-6  14 }	

sd16-4-6CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-4-6  15 }	

sd16-4-6CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-4-6  16 }	

	
--
--	nb7-sd16-4
--    

sd16-4-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-7  1 }

sd16-4-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-7  2 }

sd16-4-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-7  3 }

sd16-4-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-7  4 }
	
	
sd16-4-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-7  5 }		
	
	
sd16-4-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-7  6 }	


	
sd16-4-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-7  7 }		
	
sd16-4-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-7  8 }		
	
sd16-4-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-7  9 }	
	
sd16-4-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-7  10 }	
	

sd16-4-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-7  11 }		

sd16-4-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-7  12 }	

sd16-4-7ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-4-7  13 }	

sd16-4-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-7  14 }	

sd16-4-7CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-4-7  15 }	

sd16-4-7CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-4-7  16 }	
	
	
--
--	nb7-sd16-4
--    	

sd16-4-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-8  1 }

sd16-4-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-8  2 }

sd16-4-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-8  3 }

sd16-4-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-8  4 }
	
	
sd16-4-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-8  5 }		
	
	
sd16-4-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-8  6 }		
	
	
	
sd16-4-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-8  7 }		
	
sd16-4-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-8  8 }		
	
sd16-4-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-8  9 }	
	
sd16-4-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-8  10 }	
	

sd16-4-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-8  11 }		

sd16-4-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-8  12 }	

sd16-4-8ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-4-8  13 }		

sd16-4-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-8  14 }	

sd16-4-8CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-4-8  15 }	

sd16-4-8CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-4-8  16 }	

	--
--	nb7-sd16-4
--    	

sd16-4-9Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-9  1 }

sd16-4-9Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-9  2 }

sd16-4-9Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-9  3 }

sd16-4-9Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-9  4 }
	
	
sd16-4-9FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-9  5 }		
	
	
sd16-4-9Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-9  6 }		
	
	
	
sd16-4-9EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-9  7 }		
	
sd16-4-9VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-9  8 }		
	
sd16-4-9VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-9  9 }	
	
sd16-4-9CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-9  10 }	
	

sd16-4-9CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-9  11 }		

sd16-4-9Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-9  12 }	

sd16-4-9ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-4-9  13 }		

sd16-4-9UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-9  14 }	

sd16-4-9CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-4-9  15 }	

sd16-4-9CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-4-9  16 }	

	
--
--	nb7-sd16-4
--    	

sd16-4-10Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-10  1 }

sd16-4-10Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-10  2 }

sd16-4-10Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-10  3 }

sd16-4-10Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-10  4 }
	
	
sd16-4-10FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-10  5 }		
	
	
sd16-4-10Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-10  6 }		
	
	
	
sd16-4-10EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-10  7 }		
	
sd16-4-10VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-10  8 }		
	
sd16-4-10VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-10  9 }	
	
sd16-4-10CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-10  10 }	
	

sd16-4-10CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-10  11 }		

sd16-4-10Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-10  12 }	

sd16-4-10ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-4-10  13 }		

sd16-4-10UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-10  14 }	

sd16-4-10CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-4-10  15 }	

sd16-4-10CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-4-10  16 }	

	
--
--	nb7-sd16-4
--    	

sd16-4-11Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-11  1 }

sd16-4-11Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-11  2 }

sd16-4-11Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-11  3 }

sd16-4-11Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-11  4 }
	
	
sd16-4-11FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-11  5 }		
	
	
sd16-4-11Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-11  6 }		
	
	
	
sd16-4-11EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-11  7 }		
	
sd16-4-11VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-11  8 }		
	
sd16-4-11VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-11  9 }	
	
sd16-4-11CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-11  10 }	
	

sd16-4-11CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-11  11 }		

sd16-4-11Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-11  12 }	

sd16-4-11ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-4-11  13 }		

sd16-4-11UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-11  14 }	

sd16-4-11CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-4-11  15 }	

sd16-4-11CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-4-11  16 }	

	
--
--	nb7-sd16-4
--    	

sd16-4-12Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-12  1 }

sd16-4-12Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-12  2 }

sd16-4-12Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-12  3 }

sd16-4-12Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-12  4 }
	
	
sd16-4-12FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-12  5 }		
	
	
sd16-4-12Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-12  6 }		
	
	
	
sd16-4-12EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-12  7 }		
	
sd16-4-12VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-12  8 }		
	
sd16-4-12VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-12  9 }	
	
sd16-4-12CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-12  10 }	
	

sd16-4-12CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-12  11 }		

sd16-4-12Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-12  12 }	

sd16-4-12ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-4-12  13 }		

sd16-4-12UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-12  14 }	

sd16-4-12CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-4-12  15 }	

sd16-4-12CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-4-12  16 }	

	
--
--	nb7-sd16-4
--    	

sd16-4-13Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-13  1 }

sd16-4-13Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-13  2 }

sd16-4-13Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-13  3 }

sd16-4-13Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-13  4 }
	
	
sd16-4-13FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-13  5 }		
	
	
sd16-4-13Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-13  6 }		
	
	
	
sd16-4-13EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-13  7 }		
	
sd16-4-13VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-13  8 }		
	
sd16-4-13VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-13  9 }	
	
sd16-4-13CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-13  10 }	
	

sd16-4-13CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-13  11 }		

sd16-4-13Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-13  12 }	

sd16-4-13ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-4-13  13 }		

sd16-4-13UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-13  14 }	

sd16-4-13CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-4-13  15 }	

sd16-4-13CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-4-13  16 }	

	
--
--	nb7-sd16-4
--    	

sd16-4-14Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-14  1 }

sd16-4-14Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-14  2 }

sd16-4-14Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-14  3 }

sd16-4-14Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-14  4 }
	
	
sd16-4-14FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-14  5 }		
	
	
sd16-4-14Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-14  6 }		
	
	
	
sd16-4-14EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-14  7 }		
	
sd16-4-14VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-14  8 }		
	
sd16-4-14VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-14  9 }	
	
sd16-4-14CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-14  10 }	
	

sd16-4-14CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-14  11 }		

sd16-4-14Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-14  12 }	

sd16-4-14ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-4-14  13 }		

sd16-4-14UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-14  14 }	

sd16-4-14CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-4-14  15 }	

sd16-4-14CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-4-14  16 }	

	
--
--	nb7-sd16-4
--    	

sd16-4-15Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-15  1 }

sd16-4-15Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-15  2 }

sd16-4-15Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-15  3 }

sd16-4-15Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-15  4 }
	
	
sd16-4-15FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-15  5 }		
	
	
sd16-4-15Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-15  6 }		
	
	
	
sd16-4-15EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-15  7 }		
	
sd16-4-15VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-15  8 }		
	
sd16-4-15VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-15  9 }	
	
sd16-4-15CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-15  10 }	
	

sd16-4-15CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-15  11 }		

sd16-4-15Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-15  12 }	

sd16-4-15ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-4-15  13 }		

sd16-4-15UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-15  14 }	

sd16-4-15CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-4-15  15 }	

sd16-4-15CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-4-15  16 }	

	
--
--	nb7-sd16-4
--    	

sd16-4-16Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-16  1 }

sd16-4-16Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-16  2 }

sd16-4-16Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-16  3 }

sd16-4-16Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-16  4 }
	
	
sd16-4-16FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-16  5 }		
	
	
sd16-4-16Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-16  6 }		
	
	
	
sd16-4-16EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-16  7 }		
	
sd16-4-16VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-16  8 }		
	
sd16-4-16VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-16  9 }	
	
sd16-4-16CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-16  10 }	
	

sd16-4-16CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-16  11 }		

sd16-4-16Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-16  12 }	

sd16-4-16ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-4-16  13 }		

sd16-4-16UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4-16  14 }	

sd16-4-16CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-4-16  15 }	

sd16-4-16CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-4-16  16 }	

	

sd16-4Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4  17 }	
    
sd16-4VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4  18 }

sd16-4VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4  19 }

sd16-4CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4  20 }

sd16-4CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4  21 }
    
sd16-4Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4  22 }

sd16-4Temperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4  23 }

sd16-4TemperatureLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4  24 }

sd16-4TemperatureUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4  25 }

sd16-4Humidity OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4  26 }

sd16-4HumidityLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4  27 }

sd16-4HumidityUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4  28 }

sd16-4Event1 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4  29 }

sd16-4Event2 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-4  30 }

--
--	sd16-5
-- 

sd16-5-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { nb7-sd16-5-1  1 }

sd16-5-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { nb7-sd16-5-1  2 }

sd16-5-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { nb7-sd16-5-1  3 }

sd16-5-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { nb7-sd16-5-1  4 }
		
sd16-5-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { nb7-sd16-5-1  5 }		
	
	
sd16-5-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { nb7-sd16-5-1  6 }	
	
sd16-5-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { nb7-sd16-5-1  7 }		
	
sd16-5-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { nb7-sd16-5-1  8 }		
	
sd16-5-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { nb7-sd16-5-1  9 }	
	
sd16-5-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { nb7-sd16-5-1  10 }	
	

sd16-5-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { nb7-sd16-5-1  11 }	

sd16-5-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable nb7-sd16 -."
    DEFVAL { "" }
    ::= { nb7-sd16-5-1  12 }		
	
sd16-5-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-5-1  13 }	

sd16-5-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-1  14 }	

sd16-5-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-5-1  15 }	

sd16-5-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-5-1  16 }	


	
--
--	nb7-sd16-5
--    



sd16-5-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-2  1 }

sd16-5-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-2  2 }

sd16-5-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-2  3 }

sd16-5-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-2  4 }
	
	
sd16-5-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-2  5 }		
	
	
sd16-5-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-2  6 }		

	
sd16-5-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-2  7 }		
	
sd16-5-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-2  8 }		
	
sd16-5-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-2  9 }	
	
sd16-5-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-2  10 }	
	

sd16-5-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-2  11 }		

	
sd16-5-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-2  12 }	

sd16-5-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-5-2  13 }	

sd16-5-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-2  14 }	

sd16-5-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-5-2  15 }	

sd16-5-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-5-2  16 }	

	
--
--	nb7-sd16-5
--    
	

sd16-5-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-3  1 }

sd16-5-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-3  2 }

sd16-5-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-3  3 }

sd16-5-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-3  4 }
	
	
sd16-5-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-3  5 }		
	
	
sd16-5-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-3  6 }
	
	
sd16-5-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-3  7 }		
	
sd16-5-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-3  8 }		
	
sd16-5-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-3  9 }	
	
sd16-5-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-3  10 }	
	

sd16-5-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-3  11 }	


sd16-5-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-3  12 }	

sd16-5-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-5-3  13 }	

sd16-5-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-3  14 }	

sd16-5-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-5-3  15 }	

sd16-5-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-5-3  16 }	

	
--
--	nb7-sd16-5
--    
	
	

sd16-5-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-4  1 }

sd16-5-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-4  2 }

sd16-5-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-4  3 }

sd16-5-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-4  4 }
	
	
sd16-5-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-4  5 }		
	
	
sd16-5-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-4  6 }		
	
	
sd16-5-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-4  7 }		
	
sd16-5-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-4  8 }		
	
sd16-5-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-4  9 }	
	
sd16-5-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-4  10 }	
	

sd16-5-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-4  11 }	

	
sd16-5-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-4  12 }	

sd16-5-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-5-4  13 }	

sd16-5-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-4  14 }	

sd16-5-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-5-4  15 }	

sd16-5-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-5-4  16 }	


	
--
--	nb7-sd16-5
--    

	
	

sd16-5-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-5  1 }

sd16-5-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-5  2 }

sd16-5-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-5  3 }

sd16-5-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-5  4 }
	
	
sd16-5-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-5  5 }		
	
	
sd16-5-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-5  6 }	
	
	
sd16-5-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-5  7 }		
	
sd16-5-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-5  8 }		
	
sd16-5-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-5  9 }	
	
sd16-5-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-5  10 }	
	

sd16-5-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-5  11 }	

sd16-5-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-5  12 }	

sd16-5-5ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-5-5  13 }		

sd16-5-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-5  14 }	

sd16-5-5CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-5-5  15 }	

sd16-5-5CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-5-5  16 }	

	
--
--	nb7-sd16-5
--    
	

sd16-5-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-6  1 }

sd16-5-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-6  2 }

sd16-5-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-6  3 }

sd16-5-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-6  4 }
	
	
sd16-5-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-6  5 }		
	
	
sd16-5-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-6  6 }	

	
sd16-5-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-6  7 }		
	
sd16-5-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-6  8 }		
	
sd16-5-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-6  9 }	
	
sd16-5-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-6  10 }	
	

sd16-5-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-6  11 }	

	
sd16-5-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-6  12 }	

sd16-5-6ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-5-6  13 }		

sd16-5-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-6  14 }	

sd16-5-6CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-5-6  15 }	

sd16-5-6CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-5-6  16 }	

	
--
--	nb7-sd16-5
--    

sd16-5-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-7  1 }

sd16-5-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-7  2 }

sd16-5-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-7  3 }

sd16-5-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-7  4 }
	
	
sd16-5-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-7  5 }		
	
	
sd16-5-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-7  6 }	


	
sd16-5-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-7  7 }		
	
sd16-5-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-7  8 }		
	
sd16-5-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-7  9 }	
	
sd16-5-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-7  10 }	
	

sd16-5-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-7  11 }		

sd16-5-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-7  12 }	

sd16-5-7ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-5-7  13 }	

sd16-5-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-7  14 }	

sd16-5-7CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-5-7  15 }	

sd16-5-7CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-5-7  16 }	
	
	
--
--	nb7-sd16-5
--    	

sd16-5-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-8  1 }

sd16-5-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-8  2 }

sd16-5-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-8  3 }

sd16-5-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-8  4 }
	
	
sd16-5-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-8  5 }		
	
	
sd16-5-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-8  6 }		
	
	
	
sd16-5-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-8  7 }		
	
sd16-5-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-8  8 }		
	
sd16-5-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-8  9 }	
	
sd16-5-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-8  10 }	
	

sd16-5-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-8  11 }		

sd16-5-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-8  12 }	

sd16-5-8ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-5-8  13 }		

sd16-5-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-8  14 }	

sd16-5-8CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-5-8  15 }	

sd16-5-8CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-5-8  16 }	

	--
--	nb7-sd16-5
--    	

sd16-5-9Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-9  1 }

sd16-5-9Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-9  2 }

sd16-5-9Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-9  3 }

sd16-5-9Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-9  4 }
	
	
sd16-5-9FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-9  5 }		
	
	
sd16-5-9Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-9  6 }		
	
	
	
sd16-5-9EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-9  7 }		
	
sd16-5-9VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-9  8 }		
	
sd16-5-9VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-9  9 }	
	
sd16-5-9CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-9  10 }	
	

sd16-5-9CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-9  11 }		

sd16-5-9Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-9  12 }	

sd16-5-9ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-5-9  13 }		

sd16-5-9UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-9  14 }	

sd16-5-9CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-5-9  15 }	

sd16-5-9CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-5-9  16 }	

	
--
--	nb7-sd16-5
--    	

sd16-5-10Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-10  1 }

sd16-5-10Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-10  2 }

sd16-5-10Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-10  3 }

sd16-5-10Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-10  4 }
	
	
sd16-5-10FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-10  5 }		
	
	
sd16-5-10Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-10  6 }		
	
	
	
sd16-5-10EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-10  7 }		
	
sd16-5-10VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-10  8 }		
	
sd16-5-10VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-10  9 }	
	
sd16-5-10CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-10  10 }	
	

sd16-5-10CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-10  11 }		

sd16-5-10Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-10  12 }	

sd16-5-10ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-5-10  13 }		

sd16-5-10UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-10  14 }	

sd16-5-10CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-5-10  15 }	

sd16-5-10CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-5-10  16 }	

	
--
--	nb7-sd16-5
--    	

sd16-5-11Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-11  1 }

sd16-5-11Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-11  2 }

sd16-5-11Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-11  3 }

sd16-5-11Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-11  4 }
	
	
sd16-5-11FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-11  5 }		
	
	
sd16-5-11Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-11  6 }		
	
	
	
sd16-5-11EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-11  7 }		
	
sd16-5-11VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-11  8 }		
	
sd16-5-11VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-11  9 }	
	
sd16-5-11CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-11  10 }	
	

sd16-5-11CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-11  11 }		

sd16-5-11Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-11  12 }	

sd16-5-11ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-5-11  13 }		

sd16-5-11UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-11  14 }	

sd16-5-11CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-5-11  15 }	

sd16-5-11CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-5-11  16 }	

	
--
--	nb7-sd16-5
--    	

sd16-5-12Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-12  1 }

sd16-5-12Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-12  2 }

sd16-5-12Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-12  3 }

sd16-5-12Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-12  4 }
	
	
sd16-5-12FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-12  5 }		
	
	
sd16-5-12Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-12  6 }		
	
	
	
sd16-5-12EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-12  7 }		
	
sd16-5-12VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-12  8 }		
	
sd16-5-12VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-12  9 }	
	
sd16-5-12CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-12  10 }	
	

sd16-5-12CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-12  11 }		

sd16-5-12Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-12  12 }	

sd16-5-12ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-5-12  13 }		

sd16-5-12UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-12  14 }	

sd16-5-12CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-5-12  15 }	

sd16-5-12CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-5-12  16 }	

	
--
--	nb7-sd16-5
--    	

sd16-5-13Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-13  1 }

sd16-5-13Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-13  2 }

sd16-5-13Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-13  3 }

sd16-5-13Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-13  4 }
	
	
sd16-5-13FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-13  5 }		
	
	
sd16-5-13Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-13  6 }		
	
	
	
sd16-5-13EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-13  7 }		
	
sd16-5-13VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-13  8 }		
	
sd16-5-13VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-13  9 }	
	
sd16-5-13CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-13  10 }	
	

sd16-5-13CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-13  11 }		

sd16-5-13Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-13  12 }	

sd16-5-13ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-5-13  13 }		

sd16-5-13UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-13  14 }	

sd16-5-13CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-5-13  15 }	

sd16-5-13CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-5-13  16 }	

	
--
--	nb7-sd16-5
--    	

sd16-5-14Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-14  1 }

sd16-5-14Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-14  2 }

sd16-5-14Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-14  3 }

sd16-5-14Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-14  4 }
	
	
sd16-5-14FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-14  5 }		
	
	
sd16-5-14Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-14  6 }		
	
	
	
sd16-5-14EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-14  7 }		
	
sd16-5-14VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-14  8 }		
	
sd16-5-14VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-14  9 }	
	
sd16-5-14CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-14  10 }	
	

sd16-5-14CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-14  11 }		

sd16-5-14Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-14  12 }	

sd16-5-14ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-5-14  13 }		

sd16-5-14UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-14  14 }	

sd16-5-14CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-5-14  15 }	

sd16-5-14CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-5-14  16 }	

	
--
--	nb7-sd16-5
--    	

sd16-5-15Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-15  1 }

sd16-5-15Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-15  2 }

sd16-5-15Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-15  3 }

sd16-5-15Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-15  4 }
	
	
sd16-5-15FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-15  5 }		
	
	
sd16-5-15Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-15  6 }		
	
	
	
sd16-5-15EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-15  7 }		
	
sd16-5-15VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-15  8 }		
	
sd16-5-15VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-15  9 }	
	
sd16-5-15CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-15  10 }	
	

sd16-5-15CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-15  11 }		

sd16-5-15Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-15  12 }	

sd16-5-15ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-5-15  13 }		

sd16-5-15UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-15  14 }	

sd16-5-15CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-5-15  15 }	

sd16-5-15CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-5-15  16 }	

	
--
--	nb7-sd16-5
--    	

sd16-5-16Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-16  1 }

sd16-5-16Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-16  2 }

sd16-5-16Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-16  3 }

sd16-5-16Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-16  4 }
	
	
sd16-5-16FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-16  5 }		
	
	
sd16-5-16Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-16  6 }		
	
	
	
sd16-5-16EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-16  7 }		
	
sd16-5-16VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-16  8 }		
	
sd16-5-16VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-16  9 }	
	
sd16-5-16CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-16  10 }	
	

sd16-5-16CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-16  11 }		

sd16-5-16Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-16  12 }	

sd16-5-16ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-5-16  13 }		

sd16-5-16UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5-16  14 }	

sd16-5-16CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-5-16  15 }	

sd16-5-16CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-5-16  16 }	

	

sd16-5Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5  17 }	
    
sd16-5VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5  18 }

sd16-5VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5  19 }

sd16-5CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5  20 }

sd16-5CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5  21 }
    
sd16-5Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5  22 }

sd16-5Temperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5  23 }

sd16-5TemperatureLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5  24 }

sd16-5TemperatureUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5  25 }

sd16-5Humidity OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5  26 }

sd16-5HumidityLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5  27 }

sd16-5HumidityUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5  28 }

sd16-5Event1 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5  29 }

sd16-5Event2 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-5  30 }

--
--	sd16-6
-- 

sd16-6-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { nb7-sd16-6-1  1 }

sd16-6-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { nb7-sd16-6-1  2 }

sd16-6-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { nb7-sd16-6-1  3 }

sd16-6-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { nb7-sd16-6-1  4 }
		
sd16-6-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { nb7-sd16-6-1  5 }		
	
	
sd16-6-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { nb7-sd16-6-1  6 }	
	
sd16-6-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { nb7-sd16-6-1  7 }		
	
sd16-6-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { nb7-sd16-6-1  8 }		
	
sd16-6-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { nb7-sd16-6-1  9 }	
	
sd16-6-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { nb7-sd16-6-1  10 }	
	

sd16-6-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { nb7-sd16-6-1  11 }	

sd16-6-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable nb7-sd16 -."
    DEFVAL { "" }
    ::= { nb7-sd16-6-1  12 }		
	
sd16-6-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-6-1  13 }	

sd16-6-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-1  14 }	

sd16-6-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-6-1  15 }	

sd16-6-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-6-1  16 }	


	
--
--	nb7-sd16-6
--    



sd16-6-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-2  1 }

sd16-6-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-2  2 }

sd16-6-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-2  3 }

sd16-6-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-2  4 }
	
	
sd16-6-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-2  5 }		
	
	
sd16-6-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-2  6 }		

	
sd16-6-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-2  7 }		
	
sd16-6-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-2  8 }		
	
sd16-6-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-2  9 }	
	
sd16-6-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-2  10 }	
	

sd16-6-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-2  11 }		

	
sd16-6-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-2  12 }	

sd16-6-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-6-2  13 }	

sd16-6-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-2  14 }	

sd16-6-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-6-2  15 }	

sd16-6-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-6-2  16 }	

	
--
--	nb7-sd16-6
--    
	

sd16-6-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-3  1 }

sd16-6-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-3  2 }

sd16-6-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-3  3 }

sd16-6-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-3  4 }
	
	
sd16-6-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-3  5 }		
	
	
sd16-6-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-3  6 }
	
	
sd16-6-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-3  7 }		
	
sd16-6-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-3  8 }		
	
sd16-6-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-3  9 }	
	
sd16-6-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-3  10 }	
	

sd16-6-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-3  11 }	


sd16-6-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-3  12 }	

sd16-6-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-6-3  13 }	

sd16-6-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-3  14 }	

sd16-6-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-6-3  15 }	

sd16-6-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-6-3  16 }	

	
--
--	nb7-sd16-6
--    
	
	

sd16-6-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-4  1 }

sd16-6-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-4  2 }

sd16-6-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-4  3 }

sd16-6-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-4  4 }
	
	
sd16-6-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-4  5 }		
	
	
sd16-6-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-4  6 }		
	
	
sd16-6-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-4  7 }		
	
sd16-6-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-4  8 }		
	
sd16-6-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-4  9 }	
	
sd16-6-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-4  10 }	
	

sd16-6-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-4  11 }	

	
sd16-6-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-4  12 }	

sd16-6-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-6-4  13 }	

sd16-6-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-4  14 }	

sd16-6-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-6-4  15 }	

sd16-6-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-6-4  16 }	


	
--
--	nb7-sd16-6
--    

	
	

sd16-6-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-5  1 }

sd16-6-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-5  2 }

sd16-6-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-5  3 }

sd16-6-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-5  4 }
	
	
sd16-6-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-5  5 }		
	
	
sd16-6-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-5  6 }	
	
	
sd16-6-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-5  7 }		
	
sd16-6-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-5  8 }		
	
sd16-6-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-5  9 }	
	
sd16-6-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-5  10 }	
	

sd16-6-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-5  11 }	

sd16-6-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-5  12 }	

sd16-6-5ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-6-5  13 }		

sd16-6-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-5  14 }	

sd16-6-5CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-6-5  15 }	

sd16-6-5CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-6-5  16 }	

	
--
--	nb7-sd16-6
--    
	

sd16-6-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-6  1 }

sd16-6-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-6  2 }

sd16-6-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-6  3 }

sd16-6-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-6  4 }
	
	
sd16-6-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-6  5 }		
	
	
sd16-6-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-6  6 }	

	
sd16-6-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-6  7 }		
	
sd16-6-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-6  8 }		
	
sd16-6-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-6  9 }	
	
sd16-6-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-6  10 }	
	

sd16-6-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-6  11 }	

	
sd16-6-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-6  12 }	

sd16-6-6ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-6-6  13 }		

sd16-6-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-6  14 }	

sd16-6-6CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-6-6  15 }	

sd16-6-6CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-6-6  16 }	

	
--
--	nb7-sd16-6
--    

sd16-6-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-7  1 }

sd16-6-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-7  2 }

sd16-6-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-7  3 }

sd16-6-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-7  4 }
	
	
sd16-6-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-7  5 }		
	
	
sd16-6-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-7  6 }	


	
sd16-6-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-7  7 }		
	
sd16-6-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-7  8 }		
	
sd16-6-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-7  9 }	
	
sd16-6-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-7  10 }	
	

sd16-6-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-7  11 }		

sd16-6-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-7  12 }	

sd16-6-7ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-6-7  13 }	

sd16-6-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-7  14 }	

sd16-6-7CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-6-7  15 }	

sd16-6-7CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-6-7  16 }	
	
	
--
--	nb7-sd16-6
--    	

sd16-6-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-8  1 }

sd16-6-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-8  2 }

sd16-6-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-8  3 }

sd16-6-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-8  4 }
	
	
sd16-6-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-8  5 }		
	
	
sd16-6-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-8  6 }		
	
	
	
sd16-6-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-8  7 }		
	
sd16-6-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-8  8 }		
	
sd16-6-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-8  9 }	
	
sd16-6-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-8  10 }	
	

sd16-6-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-8  11 }		

sd16-6-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-8  12 }	

sd16-6-8ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-6-8  13 }		

sd16-6-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-8  14 }	

sd16-6-8CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-6-8  15 }	

sd16-6-8CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-6-8  16 }	

	--
--	nb7-sd16-6
--    	

sd16-6-9Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-9  1 }

sd16-6-9Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-9  2 }

sd16-6-9Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-9  3 }

sd16-6-9Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-9  4 }
	
	
sd16-6-9FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-9  5 }		
	
	
sd16-6-9Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-9  6 }		
	
	
	
sd16-6-9EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-9  7 }		
	
sd16-6-9VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-9  8 }		
	
sd16-6-9VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-9  9 }	
	
sd16-6-9CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-9  10 }	
	

sd16-6-9CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-9  11 }		

sd16-6-9Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-9  12 }	

sd16-6-9ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-6-9  13 }		

sd16-6-9UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-9  14 }	

sd16-6-9CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-6-9  15 }	

sd16-6-9CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-6-9  16 }	

	
--
--	nb7-sd16-6
--    	

sd16-6-10Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-10  1 }

sd16-6-10Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-10  2 }

sd16-6-10Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-10  3 }

sd16-6-10Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-10  4 }
	
	
sd16-6-10FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-10  5 }		
	
	
sd16-6-10Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-10  6 }		
	
	
	
sd16-6-10EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-10  7 }		
	
sd16-6-10VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-10  8 }		
	
sd16-6-10VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-10  9 }	
	
sd16-6-10CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-10  10 }	
	

sd16-6-10CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-10  11 }		

sd16-6-10Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-10  12 }	

sd16-6-10ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-6-10  13 }		

sd16-6-10UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-10  14 }	

sd16-6-10CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-6-10  15 }	

sd16-6-10CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-6-10  16 }	

	
--
--	nb7-sd16-6
--    	

sd16-6-11Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-11  1 }

sd16-6-11Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-11  2 }

sd16-6-11Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-11  3 }

sd16-6-11Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-11  4 }
	
	
sd16-6-11FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-11  5 }		
	
	
sd16-6-11Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-11  6 }		
	
	
	
sd16-6-11EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-11  7 }		
	
sd16-6-11VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-11  8 }		
	
sd16-6-11VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-11  9 }	
	
sd16-6-11CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-11  10 }	
	

sd16-6-11CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-11  11 }		

sd16-6-11Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-11  12 }	

sd16-6-11ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-6-11  13 }		

sd16-6-11UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-11  14 }	

sd16-6-11CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-6-11  15 }	

sd16-6-11CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-6-11  16 }	

	
--
--	nb7-sd16-6
--    	

sd16-6-12Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-12  1 }

sd16-6-12Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-12  2 }

sd16-6-12Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-12  3 }

sd16-6-12Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-12  4 }
	
	
sd16-6-12FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-12  5 }		
	
	
sd16-6-12Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-12  6 }		
	
	
	
sd16-6-12EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-12  7 }		
	
sd16-6-12VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-12  8 }		
	
sd16-6-12VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-12  9 }	
	
sd16-6-12CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-12  10 }	
	

sd16-6-12CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-12  11 }		

sd16-6-12Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-12  12 }	

sd16-6-12ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-6-12  13 }		

sd16-6-12UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-12  14 }	

sd16-6-12CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-6-12  15 }	

sd16-6-12CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-6-12  16 }	

	
--
--	nb7-sd16-6
--    	

sd16-6-13Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-13  1 }

sd16-6-13Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-13  2 }

sd16-6-13Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-13  3 }

sd16-6-13Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-13  4 }
	
	
sd16-6-13FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-13  5 }		
	
	
sd16-6-13Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-13  6 }		
	
	
	
sd16-6-13EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-13  7 }		
	
sd16-6-13VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-13  8 }		
	
sd16-6-13VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-13  9 }	
	
sd16-6-13CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-13  10 }	
	

sd16-6-13CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-13  11 }		

sd16-6-13Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-13  12 }	

sd16-6-13ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-6-13  13 }		

sd16-6-13UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-13  14 }	

sd16-6-13CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-6-13  15 }	

sd16-6-13CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-6-13  16 }	

	
--
--	nb7-sd16-6
--    	

sd16-6-14Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-14  1 }

sd16-6-14Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-14  2 }

sd16-6-14Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-14  3 }

sd16-6-14Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-14  4 }
	
	
sd16-6-14FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-14  5 }		
	
	
sd16-6-14Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-14  6 }		
	
	
	
sd16-6-14EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-14  7 }		
	
sd16-6-14VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-14  8 }		
	
sd16-6-14VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-14  9 }	
	
sd16-6-14CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-14  10 }	
	

sd16-6-14CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-14  11 }		

sd16-6-14Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-14  12 }	

sd16-6-14ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-6-14  13 }		

sd16-6-14UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-14  14 }	

sd16-6-14CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-6-14  15 }	

sd16-6-14CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-6-14  16 }	

	
--
--	nb7-sd16-6
--    	

sd16-6-15Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-15  1 }

sd16-6-15Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-15  2 }

sd16-6-15Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-15  3 }

sd16-6-15Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-15  4 }
	
	
sd16-6-15FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-15  5 }		
	
	
sd16-6-15Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-15  6 }		
	
	
	
sd16-6-15EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-15  7 }		
	
sd16-6-15VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-15  8 }		
	
sd16-6-15VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-15  9 }	
	
sd16-6-15CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-15  10 }	
	

sd16-6-15CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-15  11 }		

sd16-6-15Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-15  12 }	

sd16-6-15ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-6-15  13 }		

sd16-6-15UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-15  14 }	

sd16-6-15CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-6-15  15 }	

sd16-6-15CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-6-15  16 }	

	
--
--	nb7-sd16-6
--    	

sd16-6-16Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-16  1 }

sd16-6-16Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-16  2 }

sd16-6-16Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-16  3 }

sd16-6-16Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-16  4 }
	
	
sd16-6-16FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-16  5 }		
	
	
sd16-6-16Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-16  6 }		
	
	
	
sd16-6-16EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-16  7 }		
	
sd16-6-16VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-16  8 }		
	
sd16-6-16VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-16  9 }	
	
sd16-6-16CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-16  10 }	
	

sd16-6-16CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-16  11 }		

sd16-6-16Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-16  12 }	

sd16-6-16ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-6-16  13 }		

sd16-6-16UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6-16  14 }	

sd16-6-16CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-6-16  15 }	

sd16-6-16CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-6-16  16 }	

	

sd16-6Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6  17 }	
    
sd16-6VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6  18 }

sd16-6VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6  19 }

sd16-6CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6  20 }

sd16-6CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6  21 }
    
sd16-6Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6  22 }

sd16-6Temperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6  23 }

sd16-6TemperatureLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6  24 }

sd16-6TemperatureUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6  25 }

sd16-6Humidity OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6  26 }

sd16-6HumidityLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6  27 }

sd16-6HumidityUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6  28 }

sd16-6Event1 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6  29 }

sd16-6Event2 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-6  30 }

--
--	sd16-7
-- 

sd16-7-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { nb7-sd16-7-1  1 }

sd16-7-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { nb7-sd16-7-1  2 }

sd16-7-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { nb7-sd16-7-1  3 }

sd16-7-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { nb7-sd16-7-1  4 }
		
sd16-7-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { nb7-sd16-7-1  5 }		
	
	
sd16-7-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { nb7-sd16-7-1  6 }	
	
sd16-7-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { nb7-sd16-7-1  7 }		
	
sd16-7-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { nb7-sd16-7-1  8 }		
	
sd16-7-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { nb7-sd16-7-1  9 }	
	
sd16-7-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { nb7-sd16-7-1  10 }	
	

sd16-7-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { nb7-sd16-7-1  11 }	

sd16-7-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable nb7-sd16 -."
    DEFVAL { "" }
    ::= { nb7-sd16-7-1  12 }		
	
sd16-7-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-7-1  13 }	

sd16-7-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-1  14 }	

sd16-7-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-7-1  15 }	

sd16-7-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-7-1  16 }	


	
--
--	nb7-sd16-7
--    



sd16-7-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-2  1 }

sd16-7-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-2  2 }

sd16-7-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-2  3 }

sd16-7-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-2  4 }
	
	
sd16-7-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-2  5 }		
	
	
sd16-7-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-2  6 }		

	
sd16-7-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-2  7 }		
	
sd16-7-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-2  8 }		
	
sd16-7-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-2  9 }	
	
sd16-7-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-2  10 }	
	

sd16-7-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-2  11 }		

	
sd16-7-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-2  12 }	

sd16-7-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-7-2  13 }	

sd16-7-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-2  14 }	

sd16-7-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-7-2  15 }	

sd16-7-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-7-2  16 }	

	
--
--	nb7-sd16-7
--    
	

sd16-7-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-3  1 }

sd16-7-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-3  2 }

sd16-7-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-3  3 }

sd16-7-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-3  4 }
	
	
sd16-7-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-3  5 }		
	
	
sd16-7-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-3  6 }
	
	
sd16-7-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-3  7 }		
	
sd16-7-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-3  8 }		
	
sd16-7-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-3  9 }	
	
sd16-7-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-3  10 }	
	

sd16-7-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-3  11 }	


sd16-7-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-3  12 }	

sd16-7-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-7-3  13 }	

sd16-7-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-3  14 }	

sd16-7-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-7-3  15 }	

sd16-7-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-7-3  16 }	

	
--
--	nb7-sd16-7
--    
	
	

sd16-7-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-4  1 }

sd16-7-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-4  2 }

sd16-7-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-4  3 }

sd16-7-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-4  4 }
	
	
sd16-7-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-4  5 }		
	
	
sd16-7-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-4  6 }		
	
	
sd16-7-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-4  7 }		
	
sd16-7-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-4  8 }		
	
sd16-7-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-4  9 }	
	
sd16-7-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-4  10 }	
	

sd16-7-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-4  11 }	

	
sd16-7-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-4  12 }	

sd16-7-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-7-4  13 }	

sd16-7-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-4  14 }	

sd16-7-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-7-4  15 }	

sd16-7-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-7-4  16 }	


	
--
--	nb7-sd16-7
--    

	
	

sd16-7-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-5  1 }

sd16-7-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-5  2 }

sd16-7-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-5  3 }

sd16-7-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-5  4 }
	
	
sd16-7-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-5  5 }		
	
	
sd16-7-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-5  6 }	
	
	
sd16-7-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-5  7 }		
	
sd16-7-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-5  8 }		
	
sd16-7-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-5  9 }	
	
sd16-7-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-5  10 }	
	

sd16-7-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-5  11 }	

sd16-7-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-5  12 }	

sd16-7-5ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-7-5  13 }		

sd16-7-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-5  14 }	

sd16-7-5CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-7-5  15 }	

sd16-7-5CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-7-5  16 }	

	
--
--	nb7-sd16-7
--    
	

sd16-7-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-6  1 }

sd16-7-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-6  2 }

sd16-7-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-6  3 }

sd16-7-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-6  4 }
	
	
sd16-7-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-6  5 }		
	
	
sd16-7-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-6  6 }	

	
sd16-7-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-6  7 }		
	
sd16-7-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-6  8 }		
	
sd16-7-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-6  9 }	
	
sd16-7-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-6  10 }	
	

sd16-7-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-6  11 }	

	
sd16-7-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-6  12 }	

sd16-7-6ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-7-6  13 }		

sd16-7-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-6  14 }	

sd16-7-6CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-7-6  15 }	

sd16-7-6CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-7-6  16 }	

	
--
--	nb7-sd16-7
--    

sd16-7-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-7  1 }

sd16-7-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-7  2 }

sd16-7-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-7  3 }

sd16-7-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-7  4 }
	
	
sd16-7-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-7  5 }		
	
	
sd16-7-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-7  6 }	


	
sd16-7-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-7  7 }		
	
sd16-7-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-7  8 }		
	
sd16-7-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-7  9 }	
	
sd16-7-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-7  10 }	
	

sd16-7-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-7  11 }		

sd16-7-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-7  12 }	

sd16-7-7ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-7-7  13 }	

sd16-7-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-7  14 }	

sd16-7-7CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-7-7  15 }	

sd16-7-7CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-7-7  16 }	
	
	
--
--	nb7-sd16-7
--    	

sd16-7-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-8  1 }

sd16-7-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-8  2 }

sd16-7-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-8  3 }

sd16-7-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-8  4 }
	
	
sd16-7-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-8  5 }		
	
	
sd16-7-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-8  6 }		
	
	
	
sd16-7-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-8  7 }		
	
sd16-7-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-8  8 }		
	
sd16-7-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-8  9 }	
	
sd16-7-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-8  10 }	
	

sd16-7-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-8  11 }		

sd16-7-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-8  12 }	

sd16-7-8ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-7-8  13 }		

sd16-7-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-8  14 }	

sd16-7-8CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-7-8  15 }	

sd16-7-8CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-7-8  16 }	

	--
--	nb7-sd16-7
--    	

sd16-7-9Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-9  1 }

sd16-7-9Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-9  2 }

sd16-7-9Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-9  3 }

sd16-7-9Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-9  4 }
	
	
sd16-7-9FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-9  5 }		
	
	
sd16-7-9Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-9  6 }		
	
	
	
sd16-7-9EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-9  7 }		
	
sd16-7-9VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-9  8 }		
	
sd16-7-9VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-9  9 }	
	
sd16-7-9CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-9  10 }	
	

sd16-7-9CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-9  11 }		

sd16-7-9Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-9  12 }	

sd16-7-9ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-7-9  13 }		

sd16-7-9UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-9  14 }	

sd16-7-9CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-7-9  15 }	

sd16-7-9CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-7-9  16 }	

	
--
--	nb7-sd16-7
--    	

sd16-7-10Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-10  1 }

sd16-7-10Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-10  2 }

sd16-7-10Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-10  3 }

sd16-7-10Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-10  4 }
	
	
sd16-7-10FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-10  5 }		
	
	
sd16-7-10Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-10  6 }		
	
	
	
sd16-7-10EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-10  7 }		
	
sd16-7-10VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-10  8 }		
	
sd16-7-10VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-10  9 }	
	
sd16-7-10CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-10  10 }	
	

sd16-7-10CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-10  11 }		

sd16-7-10Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-10  12 }	

sd16-7-10ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-7-10  13 }		

sd16-7-10UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-10  14 }	

sd16-7-10CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-7-10  15 }	

sd16-7-10CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-7-10  16 }	

	
--
--	nb7-sd16-7
--    	

sd16-7-11Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-11  1 }

sd16-7-11Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-11  2 }

sd16-7-11Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-11  3 }

sd16-7-11Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-11  4 }
	
	
sd16-7-11FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-11  5 }		
	
	
sd16-7-11Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-11  6 }		
	
	
	
sd16-7-11EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-11  7 }		
	
sd16-7-11VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-11  8 }		
	
sd16-7-11VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-11  9 }	
	
sd16-7-11CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-11  10 }	
	

sd16-7-11CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-11  11 }		

sd16-7-11Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-11  12 }	

sd16-7-11ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-7-11  13 }		

sd16-7-11UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-11  14 }	

sd16-7-11CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-7-11  15 }	

sd16-7-11CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-7-11  16 }	

	
--
--	nb7-sd16-7
--    	

sd16-7-12Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-12  1 }

sd16-7-12Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-12  2 }

sd16-7-12Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-12  3 }

sd16-7-12Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-12  4 }
	
	
sd16-7-12FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-12  5 }		
	
	
sd16-7-12Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-12  6 }		
	
	
	
sd16-7-12EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-12  7 }		
	
sd16-7-12VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-12  8 }		
	
sd16-7-12VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-12  9 }	
	
sd16-7-12CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-12  10 }	
	

sd16-7-12CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-12  11 }		

sd16-7-12Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-12  12 }	

sd16-7-12ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-7-12  13 }		

sd16-7-12UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-12  14 }	

sd16-7-12CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-7-12  15 }	

sd16-7-12CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-7-12  16 }	

	
--
--	nb7-sd16-7
--    	

sd16-7-13Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-13  1 }

sd16-7-13Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-13  2 }

sd16-7-13Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-13  3 }

sd16-7-13Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-13  4 }
	
	
sd16-7-13FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-13  5 }		
	
	
sd16-7-13Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-13  6 }		
	
	
	
sd16-7-13EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-13  7 }		
	
sd16-7-13VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-13  8 }		
	
sd16-7-13VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-13  9 }	
	
sd16-7-13CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-13  10 }	
	

sd16-7-13CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-13  11 }		

sd16-7-13Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-13  12 }	

sd16-7-13ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-7-13  13 }		

sd16-7-13UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-13  14 }	

sd16-7-13CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-7-13  15 }	

sd16-7-13CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-7-13  16 }	

	
--
--	nb7-sd16-7
--    	

sd16-7-14Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-14  1 }

sd16-7-14Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-14  2 }

sd16-7-14Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-14  3 }

sd16-7-14Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-14  4 }
	
	
sd16-7-14FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-14  5 }		
	
	
sd16-7-14Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-14  6 }		
	
	
	
sd16-7-14EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-14  7 }		
	
sd16-7-14VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-14  8 }		
	
sd16-7-14VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-14  9 }	
	
sd16-7-14CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-14  10 }	
	

sd16-7-14CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-14  11 }		

sd16-7-14Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-14  12 }	

sd16-7-14ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-7-14  13 }		

sd16-7-14UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-14  14 }	

sd16-7-14CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-7-14  15 }	

sd16-7-14CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-7-14  16 }	

	
--
--	nb7-sd16-7
--    	

sd16-7-15Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-15  1 }

sd16-7-15Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-15  2 }

sd16-7-15Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-15  3 }

sd16-7-15Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-15  4 }
	
	
sd16-7-15FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-15  5 }		
	
	
sd16-7-15Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-15  6 }		
	
	
	
sd16-7-15EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-15  7 }		
	
sd16-7-15VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-15  8 }		
	
sd16-7-15VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-15  9 }	
	
sd16-7-15CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-15  10 }	
	

sd16-7-15CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-15  11 }		

sd16-7-15Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-15  12 }	

sd16-7-15ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-7-15  13 }		

sd16-7-15UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-15  14 }	

sd16-7-15CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-7-15  15 }	

sd16-7-15CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-7-15  16 }	

	
--
--	nb7-sd16-7
--    	

sd16-7-16Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-16  1 }

sd16-7-16Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-16  2 }

sd16-7-16Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-16  3 }

sd16-7-16Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-16  4 }
	
	
sd16-7-16FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-16  5 }		
	
	
sd16-7-16Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-16  6 }		
	
	
	
sd16-7-16EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-16  7 }		
	
sd16-7-16VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-16  8 }		
	
sd16-7-16VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-16  9 }	
	
sd16-7-16CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-16  10 }	
	

sd16-7-16CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-16  11 }		

sd16-7-16Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-16  12 }	

sd16-7-16ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-7-16  13 }		

sd16-7-16UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7-16  14 }	

sd16-7-16CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-7-16  15 }	

sd16-7-16CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-7-16  16 }	

	

sd16-7Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7  17 }	
    
sd16-7VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7  18 }

sd16-7VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7  19 }

sd16-7CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7  20 }

sd16-7CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7  21 }
    
sd16-7Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7  22 }

sd16-7Temperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7  23 }

sd16-7TemperatureLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7  24 }

sd16-7TemperatureUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7  25 }

sd16-7Humidity OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7  26 }

sd16-7HumidityLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7  27 }

sd16-7HumidityUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7  28 }

sd16-7Event1 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7  29 }

sd16-7Event2 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-7  30 }
--
--	sd16-8
-- 
sd16-8-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { nb7-sd16-8-1  1 }

sd16-8-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { nb7-sd16-8-1  2 }

sd16-8-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { nb7-sd16-8-1  3 }

sd16-8-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { nb7-sd16-8-1  4 }
		
sd16-8-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { nb7-sd16-8-1  5 }		
	
	
sd16-8-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { nb7-sd16-8-1  6 }	
	
sd16-8-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { nb7-sd16-8-1  7 }		
	
sd16-8-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { nb7-sd16-8-1  8 }		
	
sd16-8-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { nb7-sd16-8-1  9 }	
	
sd16-8-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { nb7-sd16-8-1  10 }	
	

sd16-8-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { nb7-sd16-8-1  11 }	

sd16-8-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable nb7-sd16 -."
    DEFVAL { "" }
    ::= { nb7-sd16-8-1  12 }		
	
sd16-8-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-8-1  13 }	

sd16-8-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-1  14 }

sd16-8-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-8-1  15 }	

sd16-8-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-8-1  16 }		


	
--
--	nb7-sd16-8
--    



sd16-8-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-2  1 }

sd16-8-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-2  2 }

sd16-8-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-2  3 }

sd16-8-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-2  4 }
	
	
sd16-8-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-2  5 }		
	
	
sd16-8-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-2  6 }		

	
sd16-8-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-2  7 }		
	
sd16-8-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-2  8 }		
	
sd16-8-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-2  9 }	
	
sd16-8-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-2  10 }	
	

sd16-8-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-2  11 }		

	
sd16-8-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-2  12 }	

sd16-8-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-8-2  13 }	

sd16-8-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-2  14 }	

sd16-8-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-8-2  15 }	

sd16-8-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-8-2  16 }	

	
--
--	nb7-sd16-8
--    
	

sd16-8-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-3  1 }

sd16-8-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-3  2 }

sd16-8-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-3  3 }

sd16-8-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-3  4 }
	
	
sd16-8-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-3  5 }		
	
	
sd16-8-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-3  6 }
	
	
sd16-8-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-3  7 }		
	
sd16-8-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-3  8 }		
	
sd16-8-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-3  9 }	
	
sd16-8-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-3  10 }	
	

sd16-8-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-3  11 }	


sd16-8-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-3  12 }	

sd16-8-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-8-3  13 }	

sd16-8-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-3  14 }	

sd16-8-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-8-3  15 }	

sd16-8-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-8-3  16 }	

	
--
--	nb7-sd16-8
--    
	
	

sd16-8-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-4  1 }

sd16-8-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-4  2 }

sd16-8-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-4  3 }

sd16-8-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-4  4 }
	
	
sd16-8-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-4  5 }		
	
	
sd16-8-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-4  6 }		
	
	
sd16-8-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-4  7 }		
	
sd16-8-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-4  8 }		
	
sd16-8-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-4  9 }	
	
sd16-8-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-4  10 }	
	

sd16-8-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-4  11 }	

	
sd16-8-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-4  12 }	

sd16-8-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-8-4  13 }	

sd16-8-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-4  14 }	

sd16-8-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-8-4  15 }	

sd16-8-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-8-4  16 }	


	
--
--	nb7-sd16-8
--    

	
	

sd16-8-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-5  1 }

sd16-8-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-5  2 }

sd16-8-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-5  3 }

sd16-8-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-5  4 }
	
	
sd16-8-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-5  5 }		
	
	
sd16-8-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-5  6 }	
	
	
sd16-8-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-5  7 }		
	
sd16-8-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-5  8 }		
	
sd16-8-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-5  9 }	
	
sd16-8-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-5  10 }	
	

sd16-8-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-5  11 }	

sd16-8-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-5  12 }	

sd16-8-5ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-8-5  13 }		

sd16-8-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-5  14 }	

sd16-8-5CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-8-5  15 }	

sd16-8-5CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-8-5  16 }	

	
--
--	nb7-sd16-8
--    
	

sd16-8-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-6  1 }

sd16-8-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-6  2 }

sd16-8-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-6  3 }

sd16-8-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-6  4 }
	
	
sd16-8-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-6  5 }		
	
	
sd16-8-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-6  6 }	

	
sd16-8-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-6  7 }		
	
sd16-8-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-6  8 }		
	
sd16-8-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-6  9 }	
	
sd16-8-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-6  10 }	
	

sd16-8-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-6  11 }	

	
sd16-8-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-6  12 }	

sd16-8-6ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-8-6  13 }		

sd16-8-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-6  14 }	

sd16-8-6CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-8-6  15 }	

sd16-8-6CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-8-6  16 }	

	
--
--	nb7-sd16-8
--    

sd16-8-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-7  1 }

sd16-8-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-7  2 }

sd16-8-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-7  3 }

sd16-8-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-7  4 }
	
	
sd16-8-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-7  5 }		
	
	
sd16-8-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-7  6 }	


	
sd16-8-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-7  7 }		
	
sd16-8-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-7  8 }		
	
sd16-8-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-7  9 }	
	
sd16-8-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-7  10 }	
	

sd16-8-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-7  11 }		

sd16-8-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-7  12 }	

sd16-8-7ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-8-7  13 }	

sd16-8-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-7  14 }	

sd16-8-7CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-8-7  15 }	

sd16-8-7CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-8-7  16 }	
	
	
--
--	nb7-sd16-8
--    	

sd16-8-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-8  1 }

sd16-8-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-8  2 }

sd16-8-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-8  3 }

sd16-8-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-8  4 }
	
	
sd16-8-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-8  5 }		
	
	
sd16-8-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-8  6 }		
	
	
	
sd16-8-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-8  7 }		
	
sd16-8-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-8  8 }		
	
sd16-8-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-8  9 }	
	
sd16-8-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-8  10 }	
	

sd16-8-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-8  11 }		

sd16-8-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-8  12 }	

sd16-8-8ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-8-8  13 }		

sd16-8-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-8  14 }	

sd16-8-8CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-8-8  15 }	

sd16-8-8CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-8-8  16 }	

	--
--	nb7-sd16-8
--    	

sd16-8-9Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-9  1 }

sd16-8-9Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-9  2 }

sd16-8-9Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-9  3 }

sd16-8-9Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-9  4 }
	
	
sd16-8-9FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-9  5 }		
	
	
sd16-8-9Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-9  6 }		
	
	
	
sd16-8-9EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-9  7 }		
	
sd16-8-9VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-9  8 }		
	
sd16-8-9VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-9  9 }	
	
sd16-8-9CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-9  10 }	
	

sd16-8-9CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-9  11 }		

sd16-8-9Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-9  12 }	

sd16-8-9ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-8-9  13 }		

sd16-8-9UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-9  14 }

sd16-8-9CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-8-9  15 }	

sd16-8-9CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-8-9  16 }		

	
--
--	nb7-sd16-8
--    	

sd16-8-10Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-10  1 }

sd16-8-10Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-10  2 }

sd16-8-10Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-10  3 }

sd16-8-10Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-10  4 }
	
	
sd16-8-10FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-10  5 }		
	
	
sd16-8-10Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-10  6 }		
	
	
	
sd16-8-10EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-10  7 }		
	
sd16-8-10VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-10  8 }		
	
sd16-8-10VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-10  9 }	
	
sd16-8-10CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-10  10 }	
	

sd16-8-10CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-10  11 }		

sd16-8-10Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-10  12 }	

sd16-8-10ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-8-10  13 }		

sd16-8-10UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-10  14 }	

sd16-8-10CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-8-10  15 }	

sd16-8-10CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-8-10  16 }	

	
--
--	nb7-sd16-8
--    	

sd16-8-11Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-11  1 }

sd16-8-11Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-11  2 }

sd16-8-11Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-11  3 }

sd16-8-11Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-11  4 }
	
	
sd16-8-11FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-11  5 }		
	
	
sd16-8-11Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-11  6 }		
	
	
	
sd16-8-11EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-11  7 }		
	
sd16-8-11VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-11  8 }		
	
sd16-8-11VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-11  9 }	
	
sd16-8-11CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-11  10 }	
	

sd16-8-11CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-11  11 }		

sd16-8-11Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-11  12 }	

sd16-8-11ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-8-11  13 }		

sd16-8-11UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-11  14 }	

sd16-8-11CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-8-11  15 }	

sd16-8-11CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-8-11  16 }	

	
--
--	nb7-sd16-8
--    	

sd16-8-12Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-12  1 }

sd16-8-12Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-12  2 }

sd16-8-12Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-12  3 }

sd16-8-12Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-12  4 }
	
	
sd16-8-12FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-12  5 }		
	
	
sd16-8-12Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-12  6 }		
	
	
	
sd16-8-12EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-12  7 }		
	
sd16-8-12VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-12  8 }		
	
sd16-8-12VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-12  9 }	
	
sd16-8-12CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-12  10 }	
	

sd16-8-12CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-12  11 }		

sd16-8-12Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-12  12 }	

sd16-8-12ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-8-12  13 }		

sd16-8-12UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-12  14 }	

sd16-8-12CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-8-12  15 }	

sd16-8-12CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-8-12  16 }	

	
--
--	nb7-sd16-8
--    	

sd16-8-13Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-13  1 }

sd16-8-13Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-13  2 }

sd16-8-13Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-13  3 }

sd16-8-13Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-13  4 }
	
	
sd16-8-13FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-13  5 }		
	
	
sd16-8-13Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-13  6 }		
	
	
	
sd16-8-13EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-13  7 }		
	
sd16-8-13VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-13  8 }		
	
sd16-8-13VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-13  9 }	
	
sd16-8-13CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-13  10 }	
	

sd16-8-13CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-13  11 }		

sd16-8-13Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-13  12 }	

sd16-8-13ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-8-13  13 }		

sd16-8-13UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-13  14 }	

sd16-8-13CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-8-13  15 }	

sd16-8-13CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-8-13  16 }	

	
--
--	nb7-sd16-8
--    	

sd16-8-14Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-14  1 }

sd16-8-14Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-14  2 }

sd16-8-14Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-14  3 }

sd16-8-14Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-14  4 }
	
	
sd16-8-14FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-14  5 }		
	
	
sd16-8-14Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-14  6 }		
	
	
	
sd16-8-14EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-14  7 }		
	
sd16-8-14VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-14  8 }		
	
sd16-8-14VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-14  9 }	
	
sd16-8-14CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-14  10 }	
	

sd16-8-14CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-14  11 }		

sd16-8-14Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-14  12 }	

sd16-8-14ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-8-14  13 }		

sd16-8-14UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-14  14 }	

sd16-8-14CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-8-14  15 }	

sd16-8-14CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-8-14  16 }	

	
--
--	nb7-sd16-8
--    	

sd16-8-15Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-15  1 }

sd16-8-15Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-15  2 }

sd16-8-15Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-15  3 }

sd16-8-15Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-15  4 }
	
	
sd16-8-15FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-15  5 }		
	
	
sd16-8-15Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-15  6 }		
	
	
	
sd16-8-15EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-15  7 }		
	
sd16-8-15VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-15  8 }		
	
sd16-8-15VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-15  9 }	
	
sd16-8-15CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-15  10 }	
	

sd16-8-15CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-15  11 }		

sd16-8-15Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-15  12 }	

sd16-8-15ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-8-15  13 }		

sd16-8-15UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-15  14 }	

sd16-8-15CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-8-15  15 }	

sd16-8-15CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-8-15  16 }	

	
--
--	nb7-sd16-8
--    	

sd16-8-16Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-16  1 }

sd16-8-16Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-16  2 }

sd16-8-16Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-16  3 }

sd16-8-16Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-16  4 }
	
	
sd16-8-16FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-16  5 }		
	
	
sd16-8-16Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-16  6 }		
	
	
	
sd16-8-16EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-16  7 }		
	
sd16-8-16VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-16  8 }		
	
sd16-8-16VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-16  9 }	
	
sd16-8-16CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-16  10 }	
	

sd16-8-16CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-16  11 }		

sd16-8-16Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-16  12 }	

sd16-8-16ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd16-8-16  13 }		

sd16-8-16UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8-16  14 }	

sd16-8-16CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd16-8-16  15 }	

sd16-8-16CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd16-8-16  16 }	

	

sd16-8Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8  17 }	
    
sd16-8VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8  18 }

sd16-8VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8  19 }

sd16-8CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8  20 }

sd16-8CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8  21 }
    
sd16-8Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8  22 }

sd16-8Temperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8  23 }

sd16-8TemperatureLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8  24 }

sd16-8TemperatureUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8  25 }

sd16-8Humidity OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8  26 }

sd16-8HumidityLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8  27 }

sd16-8HumidityUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8  28 }

sd16-8Event1 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8  29 }

sd16-8Event2 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd16-8  30 }




--
--	nb7-sd4-1
--    
	
	

sd4-1-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-1  1 }

sd4-1-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-1  2 }

sd4-1-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-1  3 }

sd4-1-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-1  4 }
	
	
sd4-1-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-1  5 }		
	
	
sd4-1-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-1  6 }		
	
	
sd4-1-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-1  7 }		
	
sd4-1-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-1  8 }		
	
sd4-1-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-1  9 }	
	
sd4-1-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-1  10 }	
	

sd4-1-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-1  11 }	

	
sd4-1-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-1  12 }	

sd4-1-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-1-1  13 }	

sd4-1-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-1  14 }	

sd4-1-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-1-1  15 }	

sd4-1-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-1-1  16 }	


--
--	nb7-sd4-1
--    
	
	

sd4-1-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-2  1 }

sd4-1-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-2  2 }

sd4-1-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-2  3 }

sd4-1-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-2  4 }
	
	
sd4-1-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-2  5 }		
	
	
sd4-1-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-2  6 }		
	
	
sd4-1-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-2  7 }		
	
sd4-1-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-2  8 }		
	
sd4-1-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-2  9 }	
	
sd4-1-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-2  10 }	
	

sd4-1-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-2  11 }	

	
sd4-1-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-2  12 }	

sd4-1-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-1-2  13 }	

sd4-1-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-2  14 }	

sd4-1-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-1-2  15 }	

sd4-1-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-1-2  16 }	



--
--	nb7-sd4-1
--    
	
	

sd4-1-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-3  1 }

sd4-1-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-3  2 }

sd4-1-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-3  3 }

sd4-1-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-3  4 }
	
	
sd4-1-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-3  5 }		
	
	
sd4-1-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-3  6 }		
	
	
sd4-1-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-3  7 }		
	
sd4-1-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-3  8 }		
	
sd4-1-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-3  9 }	
	
sd4-1-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-3  10 }	
	

sd4-1-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-3  11 }	

	
sd4-1-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-3  12 }	

sd4-1-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-1-3  13 }	

sd4-1-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-3  14 }	

sd4-1-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-1-3  15 }	

sd4-1-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-1-3  16 }	





--
--	nb7-sd4-1
--    
	
	

sd4-1-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-4  1 }

sd4-1-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-4  2 }

sd4-1-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-4  3 }

sd4-1-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-4  4 }
	
	
sd4-1-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-4  5 }		
	
	
sd4-1-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-4  6 }		
	
	
sd4-1-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-4  7 }		
	
sd4-1-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-4  8 }		
	
sd4-1-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-4  9 }	
	
sd4-1-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-4  10 }	
	

sd4-1-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-4  11 }	

	
sd4-1-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-4  12 }	

sd4-1-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-1-4  13 }	

sd4-1-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1-4  14 }	

sd4-1-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-1-4  15 }	

sd4-1-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-1-4  16 }	



sd4-1Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1  17 }	
    
sd4-1VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1  18 }

sd4-1VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1  19 }

sd4-1CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1  20 }

sd4-1CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1  21 }
    
sd4-1Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1  22 }

sd4-1Temperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1  23 }

sd4-1TemperatureLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1  24 }

sd4-1TemperatureUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1  25 }

sd4-1Humidity OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1  26 }

sd4-1HumidityLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1  27 }

sd4-1HumidityUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1  28 }

sd4-1Event1 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-1  29 }





--
--	nb7-sd4-2
--    		

sd4-2-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { nb7-sd4-2-1  1 }

sd4-2-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { nb7-sd4-2-1  2 }

sd4-2-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { nb7-sd4-2-1  3 }

sd4-2-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { nb7-sd4-2-1  4 }
		
sd4-2-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { nb7-sd4-2-1  5 }		
	
	
sd4-2-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { nb7-sd4-2-1  6 }	
	
sd4-2-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { nb7-sd4-2-1  7 }		
	
sd4-2-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { nb7-sd4-2-1  8 }		
	
sd4-2-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { nb7-sd4-2-1  9 }	
	
sd4-2-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { nb7-sd4-2-1  10 }	
	

sd4-2-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { nb7-sd4-2-1  11 }	

sd4-2-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable nb7-sd4 -."
    DEFVAL { "" }
    ::= { nb7-sd4-2-1  12 }		
	
sd4-2-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-2-1  13 }	

sd4-2-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-1  14 }	

sd4-2-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-2-1  15 }	

sd4-2-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-2-1  16 }	



	
--
--	nb7-sd4-2
--    



sd4-2-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-2  1 }

sd4-2-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-2  2 }

sd4-2-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-2  3 }

sd4-2-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-2  4 }
	
	
sd4-2-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-2  5 }		
	
	
sd4-2-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-2  6 }		

	
sd4-2-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-2  7 }		
	
sd4-2-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-2  8 }		
	
sd4-2-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-2  9 }	
	
sd4-2-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-2  10 }	
	

sd4-2-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-2  11 }		

	
sd4-2-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-2  12 }	

sd4-2-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-2-2  13 }	

sd4-2-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-2  14 }	

sd4-2-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-2-2  15 }	

sd4-2-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-2-2  16 }	



	
--
--	nb7-sd4-2
--    
	

sd4-2-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-3  1 }

sd4-2-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-3  2 }

sd4-2-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-3  3 }

sd4-2-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-3  4 }
	
	
sd4-2-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-3  5 }		
	
	
sd4-2-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-3  6 }
	
	
sd4-2-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-3  7 }		
	
sd4-2-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-3  8 }		
	
sd4-2-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-3  9 }	
	
sd4-2-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-3  10 }	
	

sd4-2-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-3  11 }	


sd4-2-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-3  12 }	

sd4-2-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-2-3  13 }	

sd4-2-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-3  14 }	

sd4-2-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-2-3  15 }	

sd4-2-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-2-3  16 }	



	
--
--	nb7-sd4-2
--    
	
	

sd4-2-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-4  1 }

sd4-2-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-4  2 }

sd4-2-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-4  3 }

sd4-2-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-4  4 }
	
	
sd4-2-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-4  5 }		
	
	
sd4-2-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-4  6 }		
	
	
sd4-2-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-4  7 }		
	
sd4-2-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-4  8 }		
	
sd4-2-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-4  9 }	
	
sd4-2-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-4  10 }	
	

sd4-2-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-4  11 }	

	
sd4-2-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-4  12 }	

sd4-2-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-2-4  13 }	

sd4-2-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2-4  14 }	

sd4-2-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-2-4  15 }	

sd4-2-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-2-4  16 }	




sd4-2Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2  17 }	
    
sd4-2VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2  18 }

sd4-2VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2  19 }

sd4-2CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2  20 }

sd4-2CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2  21 }
    
sd4-2Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2  22 }

sd4-2Temperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2  23 }

sd4-2TemperatureLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2  24 }

sd4-2TemperatureUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2  25 }

sd4-2Humidity OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2  26 }

sd4-2HumidityLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2  27 }

sd4-2HumidityUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2  28 }

sd4-2Event1 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-2  29 }



--
--	nb7-sd4-3
--    		

sd4-3-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { nb7-sd4-3-1  1 }

sd4-3-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { nb7-sd4-3-1  2 }

sd4-3-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { nb7-sd4-3-1  3 }

sd4-3-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { nb7-sd4-3-1  4 }
		
sd4-3-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { nb7-sd4-3-1  5 }		
	
	
sd4-3-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { nb7-sd4-3-1  6 }	
	
sd4-3-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { nb7-sd4-3-1  7 }		
	
sd4-3-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { nb7-sd4-3-1  8 }		
	
sd4-3-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { nb7-sd4-3-1  9 }	
	
sd4-3-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { nb7-sd4-3-1  10 }	
	

sd4-3-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { nb7-sd4-3-1  11 }	

sd4-3-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable nb7-sd4 -."
    DEFVAL { "" }
    ::= { nb7-sd4-3-1  12 }		
	
sd4-3-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-3-1  13 }	

sd4-3-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-1  14 }	

sd4-3-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-3-1  15 }	

sd4-3-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-3-1  16 }	




	
--
--	nb7-sd4-3
--    



sd4-3-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-2  1 }

sd4-3-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-2  2 }

sd4-3-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-2  3 }

sd4-3-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-2  4 }
	
	
sd4-3-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-2  5 }		
	
	
sd4-3-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-2  6 }		

	
sd4-3-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-2  7 }		
	
sd4-3-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-2  8 }		
	
sd4-3-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-2  9 }	
	
sd4-3-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-2  10 }	
	

sd4-3-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-2  11 }		

	
sd4-3-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-2  12 }	

sd4-3-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-3-2  13 }	

sd4-3-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-2  14 }	

sd4-3-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-3-2  15 }	

sd4-3-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-3-2  16 }	




	
--
--	nb7-sd4-3
--    
	

sd4-3-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-3  1 }

sd4-3-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-3  2 }

sd4-3-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-3  3 }

sd4-3-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-3  4 }
	
	
sd4-3-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-3  5 }		
	
	
sd4-3-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-3  6 }
	
	
sd4-3-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-3  7 }		
	
sd4-3-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-3  8 }		
	
sd4-3-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-3  9 }	
	
sd4-3-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-3  10 }	
	

sd4-3-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-3  11 }	


sd4-3-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-3  12 }	

sd4-3-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-3-3  13 }	

sd4-3-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-3  14 }	

sd4-3-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-3-3  15 }	

sd4-3-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-3-3  16 }	




	
--
--	nb7-sd4-3
--    
	
	

sd4-3-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-4  1 }

sd4-3-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-4  2 }

sd4-3-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-4  3 }

sd4-3-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-4  4 }
	
	
sd4-3-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-4  5 }		
	
	
sd4-3-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-4  6 }		
	
	
sd4-3-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-4  7 }		
	
sd4-3-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-4  8 }		
	
sd4-3-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-4  9 }	
	
sd4-3-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-4  10 }	
	

sd4-3-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-4  11 }	

	
sd4-3-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-4  12 }	

sd4-3-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-3-4  13 }	

sd4-3-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3-4  14 }	

sd4-3-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-3-4  15 }	

sd4-3-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-3-4  16 }	





sd4-3Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3  17 }	
    
sd4-3VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3  18 }

sd4-3VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3  19 }

sd4-3CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3  20 }

sd4-3CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3  21 }
    
sd4-3Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3  22 }

sd4-3Temperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3  23 }

sd4-3TemperatureLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3  24 }

sd4-3TemperatureUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3  25 }

sd4-3Humidity OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3  26 }

sd4-3HumidityLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3  27 }

sd4-3HumidityUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3  28 }

sd4-3Event1 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-3  29 }



--
--	nb7-sd4-4
--    		

sd4-4-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { nb7-sd4-4-1  1 }

sd4-4-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { nb7-sd4-4-1  2 }

sd4-4-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { nb7-sd4-4-1  3 }

sd4-4-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { nb7-sd4-4-1  4 }
		
sd4-4-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { nb7-sd4-4-1  5 }		
	
	
sd4-4-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { nb7-sd4-4-1  6 }	
	
sd4-4-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { nb7-sd4-4-1  7 }		
	
sd4-4-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { nb7-sd4-4-1  8 }		
	
sd4-4-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { nb7-sd4-4-1  9 }	
	
sd4-4-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { nb7-sd4-4-1  10 }	
	

sd4-4-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { nb7-sd4-4-1  11 }	

sd4-4-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable nb7-sd4 -."
    DEFVAL { "" }
    ::= { nb7-sd4-4-1  12 }		
	
sd4-4-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-4-1  13 }	

sd4-4-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-1  14 }	

sd4-4-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-4-1  15 }	

sd4-4-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-4-1  16 }	





	
--
--	nb7-sd4-4
--    



sd4-4-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-2  1 }

sd4-4-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-2  2 }

sd4-4-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-2  3 }

sd4-4-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-2  4 }
	
	
sd4-4-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-2  5 }		
	
	
sd4-4-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-2  6 }		

	
sd4-4-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-2  7 }		
	
sd4-4-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-2  8 }		
	
sd4-4-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-2  9 }	
	
sd4-4-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-2  10 }	
	

sd4-4-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-2  11 }		

	
sd4-4-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-2  12 }	

sd4-4-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-4-2  13 }	

sd4-4-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-2  14 }	

sd4-4-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-4-2  15 }	

sd4-4-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-4-2  16 }	



	
--
--	nb7-sd4-4
--    
	

sd4-4-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-3  1 }

sd4-4-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-3  2 }

sd4-4-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-3  3 }

sd4-4-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-3  4 }
	
	
sd4-4-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-3  5 }		
	
	
sd4-4-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-3  6 }
	
	
sd4-4-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-3  7 }		
	
sd4-4-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-3  8 }		
	
sd4-4-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-3  9 }	
	
sd4-4-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-3  10 }	
	

sd4-4-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-3  11 }	


sd4-4-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-3  12 }	

sd4-4-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-4-3  13 }	

sd4-4-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-3  14 }	

sd4-4-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-4-3  15 }	

sd4-4-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-4-3  16 }	



	
--
--	nb7-sd4-4
--    
	
	

sd4-4-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-4  1 }

sd4-4-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-4  2 }

sd4-4-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-4  3 }

sd4-4-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-4  4 }
	
	
sd4-4-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-4  5 }		
	
	
sd4-4-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-4  6 }		
	
	
sd4-4-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-4  7 }		
	
sd4-4-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-4  8 }		
	
sd4-4-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-4  9 }	
	
sd4-4-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-4  10 }	
	

sd4-4-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-4  11 }	

	
sd4-4-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-4  12 }	

sd4-4-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-4-4  13 }	

sd4-4-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4-4  14 }	

sd4-4-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-4-4  15 }	

sd4-4-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-4-4  16 }	




sd4-4Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4  17 }	
    
sd4-4VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4  18 }

sd4-4VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4  19 }

sd4-4CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4  20 }

sd4-4CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4  21 }
    
sd4-4Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4  22 }

sd4-4Temperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4  23 }

sd4-4TemperatureLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4  24 }

sd4-4TemperatureUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4  25 }

sd4-4Humidity OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4  26 }

sd4-4HumidityLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4  27 }

sd4-4HumidityUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4  28 }

sd4-4Event1 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-4  29 }




--
--	nb7-sd4-5
--    		

sd4-5-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { nb7-sd4-5-1  1 }

sd4-5-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { nb7-sd4-5-1  2 }

sd4-5-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { nb7-sd4-5-1  3 }

sd4-5-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { nb7-sd4-5-1  4 }
		
sd4-5-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { nb7-sd4-5-1  5 }		
	
	
sd4-5-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { nb7-sd4-5-1  6 }	
	
sd4-5-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { nb7-sd4-5-1  7 }		
	
sd4-5-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { nb7-sd4-5-1  8 }		
	
sd4-5-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { nb7-sd4-5-1  9 }	
	
sd4-5-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { nb7-sd4-5-1  10 }	
	

sd4-5-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { nb7-sd4-5-1  11 }	

sd4-5-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable nb7-sd4 -."
    DEFVAL { "" }
    ::= { nb7-sd4-5-1  12 }		
	
sd4-5-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-5-1  13 }	

sd4-5-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-1  14 }	

sd4-5-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-5-1  15 }	

sd4-5-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-5-1  16 }	




	
--
--	nb7-sd4-5
--    



sd4-5-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-2  1 }

sd4-5-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-2  2 }

sd4-5-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-2  3 }

sd4-5-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-2  4 }
	
	
sd4-5-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-2  5 }		
	
	
sd4-5-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-2  6 }		

	
sd4-5-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-2  7 }		
	
sd4-5-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-2  8 }		
	
sd4-5-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-2  9 }	
	
sd4-5-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-2  10 }	
	

sd4-5-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-2  11 }		

	
sd4-5-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-2  12 }	

sd4-5-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-5-2  13 }	

sd4-5-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-2  14 }	

sd4-5-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-5-2  15 }	

sd4-5-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-5-2  16 }	



	
--
--	nb7-sd4-5
--    
	

sd4-5-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-3  1 }

sd4-5-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-3  2 }

sd4-5-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-3  3 }

sd4-5-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-3  4 }
	
	
sd4-5-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-3  5 }		
	
	
sd4-5-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-3  6 }
	
	
sd4-5-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-3  7 }		
	
sd4-5-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-3  8 }		
	
sd4-5-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-3  9 }	
	
sd4-5-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-3  10 }	
	

sd4-5-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-3  11 }	


sd4-5-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-3  12 }	

sd4-5-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-5-3  13 }	

sd4-5-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-3  14 }	

sd4-5-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-5-3  15 }	

sd4-5-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-5-3  16 }	



	
--
--	nb7-sd4-5
--    
	
	

sd4-5-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-4  1 }

sd4-5-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-4  2 }

sd4-5-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-4  3 }

sd4-5-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-4  4 }
	
	
sd4-5-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-4  5 }		
	
	
sd4-5-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-4  6 }		
	
	
sd4-5-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-4  7 }		
	
sd4-5-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-4  8 }		
	
sd4-5-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-4  9 }	
	
sd4-5-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-4  10 }	
	

sd4-5-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-4  11 }	

	
sd4-5-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-4  12 }	

sd4-5-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-5-4  13 }	

sd4-5-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5-4  14 }	

sd4-5-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-5-4  15 }	

sd4-5-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-5-4  16 }	




sd4-5Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5  17 }	
    
sd4-5VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5  18 }

sd4-5VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5  19 }

sd4-5CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5  20 }

sd4-5CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5  21 }
    
sd4-5Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5  22 }

sd4-5Temperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5  23 }

sd4-5TemperatureLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5  24 }

sd4-5TemperatureUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5  25 }

sd4-5Humidity OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5  26 }

sd4-5HumidityLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5  27 }

sd4-5HumidityUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5  28 }

sd4-5Event1 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-5  29 }




--
--	nb7-sd4-6
--    		

sd4-6-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { nb7-sd4-6-1  1 }

sd4-6-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { nb7-sd4-6-1  2 }

sd4-6-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { nb7-sd4-6-1  3 }

sd4-6-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { nb7-sd4-6-1  4 }
		
sd4-6-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { nb7-sd4-6-1  5 }		
	
	
sd4-6-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { nb7-sd4-6-1  6 }	
	
sd4-6-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { nb7-sd4-6-1  7 }		
	
sd4-6-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { nb7-sd4-6-1  8 }		
	
sd4-6-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { nb7-sd4-6-1  9 }	
	
sd4-6-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { nb7-sd4-6-1  10 }	
	

sd4-6-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { nb7-sd4-6-1  11 }	

sd4-6-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable nb7-sd4 -."
    DEFVAL { "" }
    ::= { nb7-sd4-6-1  12 }		
	
sd4-6-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-6-1  13 }	

sd4-6-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-1  14 }	

sd4-6-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-6-1  15 }	

sd4-6-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-6-1  16 }	




	
--
--	nb7-sd4-6
--    



sd4-6-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-2  1 }

sd4-6-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-2  2 }

sd4-6-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-2  3 }

sd4-6-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-2  4 }
	
	
sd4-6-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-2  5 }		
	
	
sd4-6-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-2  6 }		

	
sd4-6-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-2  7 }		
	
sd4-6-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-2  8 }		
	
sd4-6-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-2  9 }	
	
sd4-6-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-2  10 }	
	

sd4-6-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-2  11 }		

	
sd4-6-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-2  12 }	

sd4-6-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-6-2  13 }	

sd4-6-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-2  14 }	

sd4-6-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-6-2  15 }	

sd4-6-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-6-2  16 }	




	
--
--	nb7-sd4-6
--    
	

sd4-6-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-3  1 }

sd4-6-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-3  2 }

sd4-6-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-3  3 }

sd4-6-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-3  4 }
	
	
sd4-6-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-3  5 }		
	
	
sd4-6-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-3  6 }
	
	
sd4-6-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-3  7 }		
	
sd4-6-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-3  8 }		
	
sd4-6-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-3  9 }	
	
sd4-6-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-3  10 }	
	

sd4-6-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-3  11 }	


sd4-6-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-3  12 }	

sd4-6-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-6-3  13 }	

sd4-6-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-3  14 }	

sd4-6-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-6-3  15 }	

sd4-6-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-6-3  16 }	




	
--
--	nb7-sd4-6
--    
	
	

sd4-6-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-4  1 }

sd4-6-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-4  2 }

sd4-6-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-4  3 }

sd4-6-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-4  4 }
	
	
sd4-6-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-4  5 }		
	
	
sd4-6-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-4  6 }		
	
	
sd4-6-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-4  7 }		
	
sd4-6-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-4  8 }		
	
sd4-6-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-4  9 }	
	
sd4-6-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-4  10 }	
	

sd4-6-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-4  11 }	

	
sd4-6-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-4  12 }	

sd4-6-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-6-4  13 }	

sd4-6-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6-4  14 }	

sd4-6-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-6-4  15 }	

sd4-6-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-6-4  16 }	





sd4-6Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6  17 }	
    
sd4-6VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6  18 }

sd4-6VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6  19 }

sd4-6CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6  20 }

sd4-6CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6  21 }
    
sd4-6Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6  22 }

sd4-6Temperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6  23 }

sd4-6TemperatureLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6  24 }

sd4-6TemperatureUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6  25 }

sd4-6Humidity OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6  26 }

sd4-6HumidityLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6  27 }

sd4-6HumidityUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6  28 }

sd4-6Event1 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-6  29 }



--
--	nb7-sd4-7
--    		

sd4-7-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { nb7-sd4-7-1  1 }

sd4-7-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { nb7-sd4-7-1  2 }

sd4-7-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { nb7-sd4-7-1  3 }

sd4-7-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { nb7-sd4-7-1  4 }
		
sd4-7-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { nb7-sd4-7-1  5 }		
	
	
sd4-7-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { nb7-sd4-7-1  6 }	
	
sd4-7-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { nb7-sd4-7-1  7 }		
	
sd4-7-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { nb7-sd4-7-1  8 }		
	
sd4-7-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { nb7-sd4-7-1  9 }	
	
sd4-7-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { nb7-sd4-7-1  10 }	
	

sd4-7-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { nb7-sd4-7-1  11 }	

sd4-7-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable nb7-sd4 -."
    DEFVAL { "" }
    ::= { nb7-sd4-7-1  12 }		
	
sd4-7-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-7-1  13 }	

sd4-7-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-1  14 }	

sd4-7-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-7-1  15 }	

sd4-7-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-7-1  16 }	





	
--
--	nb7-sd4-7
--    



sd4-7-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-2  1 }

sd4-7-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-2  2 }

sd4-7-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-2  3 }

sd4-7-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-2  4 }
	
	
sd4-7-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-2  5 }		
	
	
sd4-7-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-2  6 }		

	
sd4-7-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-2  7 }		
	
sd4-7-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-2  8 }		
	
sd4-7-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-2  9 }	
	
sd4-7-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-2  10 }	
	

sd4-7-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-2  11 }		

	
sd4-7-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-2  12 }	

sd4-7-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-7-2  13 }	

sd4-7-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-2  14 }	

sd4-7-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-7-2  15 }	

sd4-7-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-7-2  16 }	



	
--
--	nb7-sd4-7
--    
	

sd4-7-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-3  1 }

sd4-7-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-3  2 }

sd4-7-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-3  3 }

sd4-7-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-3  4 }
	
	
sd4-7-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-3  5 }		
	
	
sd4-7-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-3  6 }
	
	
sd4-7-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-3  7 }		
	
sd4-7-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-3  8 }		
	
sd4-7-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-3  9 }	
	
sd4-7-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-3  10 }	
	

sd4-7-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-3  11 }	


sd4-7-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-3  12 }	

sd4-7-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-7-3  13 }	

sd4-7-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-3  14 }	

sd4-7-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-7-3  15 }	

sd4-7-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-7-3  16 }	



	
--
--	nb7-sd4-7
--    
	
	

sd4-7-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-4  1 }

sd4-7-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-4  2 }

sd4-7-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-4  3 }

sd4-7-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-4  4 }
	
	
sd4-7-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-4  5 }		
	
	
sd4-7-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-4  6 }		
	
	
sd4-7-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-4  7 }		
	
sd4-7-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-4  8 }		
	
sd4-7-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-4  9 }	
	
sd4-7-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-4  10 }	
	

sd4-7-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-4  11 }	

	
sd4-7-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-4  12 }	

sd4-7-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-7-4  13 }	

sd4-7-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7-4  14 }	

sd4-7-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-7-4  15 }	

sd4-7-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-7-4  16 }	




sd4-7Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7  17 }	
    
sd4-7VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7  18 }

sd4-7VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7  19 }

sd4-7CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7  20 }

sd4-7CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7  21 }
    
sd4-7Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7  22 }

sd4-7Temperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7  23 }

sd4-7TemperatureLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7  24 }

sd4-7TemperatureUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7  25 }

sd4-7Humidity OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7  26 }

sd4-7HumidityLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7  27 }

sd4-7HumidityUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7  28 }

sd4-7Event1 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-7  29 }




--
--	nb7-sd4-8
--    		

sd4-8-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { nb7-sd4-8-1  1 }

sd4-8-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { nb7-sd4-8-1  2 }

sd4-8-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { nb7-sd4-8-1  3 }

sd4-8-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { nb7-sd4-8-1  4 }
		
sd4-8-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { nb7-sd4-8-1  5 }		
	
	
sd4-8-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { nb7-sd4-8-1  6 }	
	
sd4-8-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { nb7-sd4-8-1  7 }		
	
sd4-8-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { nb7-sd4-8-1  8 }		
	
sd4-8-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { nb7-sd4-8-1  9 }	
	
sd4-8-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { nb7-sd4-8-1  10 }	
	

sd4-8-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { nb7-sd4-8-1  11 }	

sd4-8-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable nb7-sd4 -."
    DEFVAL { "" }
    ::= { nb7-sd4-8-1  12 }		
	
sd4-8-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-8-1  13 }	

sd4-8-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-1  14 }	

sd4-8-1CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-8-1  15 }	

sd4-8-1CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-8-1  16 }	




	
--
--	nb7-sd4-8
--    



sd4-8-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-2  1 }

sd4-8-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-2  2 }

sd4-8-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-2  3 }

sd4-8-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-2  4 }
	
	
sd4-8-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-2  5 }		
	
	
sd4-8-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-2  6 }		

	
sd4-8-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-2  7 }		
	
sd4-8-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-2  8 }		
	
sd4-8-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-2  9 }	
	
sd4-8-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-2  10 }	
	

sd4-8-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-2  11 }		

	
sd4-8-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-2  12 }	

sd4-8-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-8-2  13 }	

sd4-8-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-2  14 }	

sd4-8-2CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-8-2  15 }	

sd4-8-2CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-8-2  16 }	



	
--
--	nb7-sd4-8
--    
	

sd4-8-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-3  1 }

sd4-8-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-3  2 }

sd4-8-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-3  3 }

sd4-8-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-3  4 }
	
	
sd4-8-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-3  5 }		
	
	
sd4-8-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-3  6 }
	
	
sd4-8-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-3  7 }		
	
sd4-8-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-3  8 }		
	
sd4-8-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-3  9 }	
	
sd4-8-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-3  10 }	
	

sd4-8-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-3  11 }	


sd4-8-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-3  12 }	

sd4-8-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-8-3  13 }	

sd4-8-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-3  14 }	

sd4-8-3CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-8-3  15 }	

sd4-8-3CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-8-3  16 }	



	
--
--	nb7-sd4-8
--    
	
	

sd4-8-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-4  1 }

sd4-8-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-4  2 }

sd4-8-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-4  3 }

sd4-8-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-4  4 }
	
	
sd4-8-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-4  5 }		
	
	
sd4-8-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-4  6 }		
	
	
sd4-8-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-4  7 }		
	
sd4-8-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-4  8 }		
	
sd4-8-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-4  9 }	
	
sd4-8-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-4  10 }	
	

sd4-8-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-4  11 }	

	
sd4-8-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-4  12 }	

sd4-8-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset channel output."
    DEFVAL { "" }
    ::= { nb7-sd4-8-4  13 }	

sd4-8-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8-4  14 }	

sd4-8-4CycleCount OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Cycle Count."
    DEFVAL { "" }
    ::= { nb7-sd4-8-4  15 }	

sd4-8-4CycleCountLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Cycle Count Limit."
    DEFVAL { "" }
    ::= { nb7-sd4-8-4  16 }	




sd4-8Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8  17 }	
    
sd4-8VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8  18 }

sd4-8VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8  19 }

sd4-8CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8  20 }

sd4-8CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8  21 }
    
sd4-8Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8  22 }

sd4-8Temperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8  23 }

sd4-8TemperatureLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8  24 }

sd4-8TemperatureUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8  25 }

sd4-8Humidity OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8  26 }

sd4-8HumidityLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8  27 }

sd4-8HumidityUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8  28 }

sd4-8Event1 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-sd4-8  29 }






--
--	nb7-b150-1
--    

b150-1Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  1}	

b150-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  2}	

b150-1OutputStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  3}	

b150-1InputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  4}	

b150-1InputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  5}	

b150-1InputPower OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  6}	

b150-1OutputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  7}	

b150-1OutputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  8}	

b150-1OutputPower OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  9}	


    
b150-1InputVoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  10}

b150-1InputVoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  11}

b150-1InputCurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  12}

 b150-1InputCurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  13}
    

b150-1InputVoltageLowerLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  14}

b150-1InputVoltageUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  15}


 b150-1InputCurrentUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  16}
    
    
b150-1OutputVoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  17}

b150-1OutputVoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  18}

b150-1OutputCurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  19}

 b150-1OutputCurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  20}
    

b150-1OutputVoltageLowerLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  21}

b150-1OutputVoltageUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  22}


b150-1OutputCurrentUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  23}
   
b150-1ResetOutput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  24} 

b150-1DisableOutputOnFAI OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  25} 

b150-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-1  26} 

    


--
--	nb7-b150-2
--    

b150-2Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  1}	

b150-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  2}	

b150-2OutputStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  3}	

b150-2InputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  4}	

b150-2InputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  5}	

b150-2InputPower OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  6}	

b150-2OutputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  7}	

b150-2OutputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  8}	

b150-2OutputPower OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  9}	


    
b150-2InputVoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  10}

b150-2InputVoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  11}

b150-2InputCurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  12}

 b150-2InputCurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  13}
    

b150-2InputVoltageLowerLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  14}

b150-2InputVoltageUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  15}


 b150-2InputCurrentUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  16}
    
    
b150-2OutputVoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  17}

b150-2OutputVoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  18}

b150-2OutputCurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  19}

 b150-2OutputCurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  20}
    

b150-2OutputVoltageLowerLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  21}

b150-2OutputVoltageUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  22}


b150-2OutputCurrentUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  23}
   
b150-2ResetOutput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  24} 

b150-2DisableOutputOnFAI OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  25} 

b150-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-2  26} 



--
--	nb7-b150-3
--    

b150-3Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  1}	

b150-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  2}	

b150-3OutputStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  3}	

b150-3InputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  4}	

b150-3InputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  5}	

b150-3InputPower OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  6}	

b150-3OutputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  7}	

b150-3OutputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  8}	

b150-3OutputPower OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  9}	


    
b150-3InputVoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  10}

b150-3InputVoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  11}

b150-3InputCurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  12}

 b150-3InputCurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  13}
    

b150-3InputVoltageLowerLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  14}

b150-3InputVoltageUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  15}


 b150-3InputCurrentUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  16}
    
    
b150-3OutputVoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  17}

b150-3OutputVoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  18}

b150-3OutputCurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  19}

 b150-3OutputCurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  20}
    

b150-3OutputVoltageLowerLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  21}

b150-3OutputVoltageUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  22}


b150-3OutputCurrentUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  23}
   
b150-3ResetOutput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  24} 

b150-3DisableOutputOnFAI OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  25} 

b150-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-3  26} 



--
--	nb7-b150-4
--    

b150-4Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  1}	

b150-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  2}	

b150-4OutputStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  3}	

b150-4InputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  4}	

b150-4InputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  5}	

b150-4InputPower OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  6}	

b150-4OutputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  7}	

b150-4OutputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  8}	

b150-4OutputPower OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  9}	


    
b150-4InputVoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  10}

b150-4InputVoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  11}

b150-4InputCurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  12}

 b150-4InputCurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  13}
    

b150-4InputVoltageLowerLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  14}

b150-4InputVoltageUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  15}


 b150-4InputCurrentUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  16}
    
    
b150-4OutputVoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  17}

b150-4OutputVoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  18}

b150-4OutputCurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  19}

 b150-4OutputCurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  20}
    

b150-4OutputVoltageLowerLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  21}

b150-4OutputVoltageUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  22}


b150-4OutputCurrentUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  23}
   
b150-4ResetOutput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  24} 

b150-4DisableOutputOnFAI OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  25} 

b150-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-4  26} 



--
--	nb7-b150-5
--    

b150-5Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  1}	

b150-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  2}	

b150-5OutputStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  3}	

b150-5InputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  4}	

b150-5InputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  5}	

b150-5InputPower OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  6}	

b150-5OutputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  7}	

b150-5OutputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  8}	

b150-5OutputPower OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  9}	


    
b150-5InputVoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  10}

b150-5InputVoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  11}

b150-5InputCurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  12}

 b150-5InputCurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  13}
    

b150-5InputVoltageLowerLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  14}

b150-5InputVoltageUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  15}


 b150-5InputCurrentUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  16}
    
    
b150-5OutputVoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  17}

b150-5OutputVoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  18}

b150-5OutputCurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  19}

 b150-5OutputCurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  20}
    

b150-5OutputVoltageLowerLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  21}

b150-5OutputVoltageUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  22}


b150-5OutputCurrentUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  23}
   
b150-5ResetOutput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  24} 

b150-5DisableOutputOnFAI OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  25} 

b150-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-5  26} 



--
--	nb7-b150-6
--    

b150-6Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  1}	

b150-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  2}	

b150-6OutputStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  3}	

b150-6InputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  4}	

b150-6InputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  5}	

b150-6InputPower OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  6}	

b150-6OutputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  7}	

b150-6OutputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  8}	

b150-6OutputPower OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  9}	


    
b150-6InputVoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  10}

b150-6InputVoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  11}

b150-6InputCurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  12}

 b150-6InputCurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  13}
    

b150-6InputVoltageLowerLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  14}

b150-6InputVoltageUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  15}


 b150-6InputCurrentUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  16}
    
    
b150-6OutputVoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  17}

b150-6OutputVoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  18}

b150-6OutputCurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  19}

 b150-6OutputCurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  20}
    

b150-6OutputVoltageLowerLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  21}

b150-6OutputVoltageUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  22}


b150-6OutputCurrentUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  23}
   
b150-6ResetOutput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  24} 

b150-6DisableOutputOnFAI OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  25} 

b150-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-6  26} 



--
--	nb7-b150-7
--    

b150-7Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  1}	

b150-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  2}	

b150-7OutputStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  3}	

b150-7InputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  4}	

b150-7InputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  5}	

b150-7InputPower OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  6}	

b150-7OutputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  7}	

b150-7OutputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  8}	

b150-7OutputPower OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  9}	


    
b150-7InputVoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  10}

b150-7InputVoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  11}

b150-7InputCurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  12}

 b150-7InputCurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  13}
    

b150-7InputVoltageLowerLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  14}

b150-7InputVoltageUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  15}


 b150-7InputCurrentUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  16}
    
    
b150-7OutputVoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  17}

b150-7OutputVoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  18}

b150-7OutputCurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  19}

 b150-7OutputCurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  20}
    

b150-7OutputVoltageLowerLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  21}

b150-7OutputVoltageUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  22}


b150-7OutputCurrentUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  23}
   
b150-7ResetOutput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  24} 

b150-7DisableOutputOnFAI OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  25} 

b150-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-7  26} 



--
--	nb7-b150-8
--    

b150-8Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  1}	

b150-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  2}	

b150-8OutputStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  3}	

b150-8InputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  4}	

b150-8InputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  5}	

b150-8InputPower OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  6}	

b150-8OutputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  7}	

b150-8OutputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  8}	

b150-8OutputPower OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  9}	


    
b150-8InputVoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  10}

b150-8InputVoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  11}

b150-8InputCurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  12}

 b150-8InputCurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  13}
    

b150-8InputVoltageLowerLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  14}

b150-8InputVoltageUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  15}


 b150-8InputCurrentUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  16}
    
    
b150-8OutputVoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  17}

b150-8OutputVoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  18}

b150-8OutputCurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  19}

 b150-8OutputCurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  20}
    

b150-8OutputVoltageLowerLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  21}

b150-8OutputVoltageUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  22}


b150-8OutputCurrentUpperLimitOfCutoff OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  23}
   
b150-8ResetOutput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  24} 

b150-8DisableOutputOnFAI OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  25} 

b150-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nb7-b150-8  26} 
    
END