lspnlcMIB DEFINITIONS ::= BEGIN

--
-- Top-level infrastructure of the Net-SNMP project enterprise MIB tree
--

IMPORTS
    MODULE-IDENTITY, enterprises          	FROM SNMPv2-SMI
    MODULE-IDENTITY, OBJECT-TYPE, Integer32,
    NOTIFICATION-TYPE                       FROM SNMPv2-SMI
    SnmpAdminString                         FROM SNMP-FRAMEWORK-MIB
    netSnmp                                 FROM NET-SNMP-MIB
    RowStatus, StorageType, DisplayString   FROM SNMPv2-TC
    InetAddressType, InetAddress            FROM INET-ADDRESS-MIB
;
lspnlcMIB MODULE-IDENTITY
    LAST-UPDATED "202103011010Z"
    ORGANIZATION "LifeSafety Power, Inc. "
    CONTACT-INFO    
     "http://www.lifesafetypower.com/
	 
	  EMail: gliu@lifesafetypower.com
	 "
    DESCRIPTION
    "This is the MIB Module for NLC objects for managing NLC device."

	REVISION	"202103011010Z"
	DESCRIPTION
	"Updated to support Net-SNMP compile."
    ::= { enterprises 42520}

nlcMIB 		OBJECT IDENTIFIER ::= {lspnlcMIB 10}

netlink		OBJECT IDENTIFIER ::= { nlcMIB 1}

nlcTraps       	OBJECT IDENTIFIER ::= { lspnlcMIB 11}

--
--	MCU
--    
Time OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Time."
    DEFVAL { "" }
    ::= { netlink  1 }

SiteID OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Site ID, it is entered by user from GUI."
    DEFVAL { "" }
    ::= { netlink  2 }

DeviceDetectCnt OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System device detected."
    DEFVAL { "" }
    ::= { netlink  3 }

NextServicedue OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Service due, NO or Yes. Service date is entered by user from GUI."
    DEFVAL { "" }
    ::= { netlink  4 }
    
Status   OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "MCU  Current Status."
    DEFVAL { "" }
    ::= { netlink  5 }
    


SystemVersion  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System  Version."
    DEFVAL { "" }
    ::= { netlink  6 }    




END