**REVIT FILE – READ ME**

1.       All enclosure heights are set such that the top of the enclosure is six feet, zero inches above the floor. The floor must be the reference plane to avoid placing the enclosure at the wrong height.

2.       Devices are classified as OmniClass 23. Specifically 23.85.xx for security systems. The OmniClass may be changed at the discretion of the designer from a Revit dropdown list.